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ELSKY IPC200U Industrial Computer Specifications
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
PC size diagram
[image: E:/主机说明书/AAAAAA主机规格书待做/1U 2U 4U机箱规格书/IPC200U/尺寸.jpg尺寸]
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Front Interface Diagram
[image: E:/主机说明书/AAAAAA主机规格书待做/1U 2U 4U机箱规格书/IPC200U/1.jpg1]
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface diagram with network port in the middle and small audio port.
[image: E:/主机说明书/AAAAAA主机规格书待做/1U 2U 4U机箱规格书/IPC200U/小音频口+网口中间.jpg小音频口+网口中间]
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface side view of network port + large audio port diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface diagram DP optional
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear I/O panel: Dual HDMI optional
[image: E:/主机说明书/1U 2U 4U机箱规格书/IPC200U/主机图片/双HDMI.jpg双HDMI]
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
		Rear interface diagram, dual network optional
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear Interface Diagram 2COM (Optional)
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
[image: E:/主机说明书/AAAAAA主机规格书待做/1U 2U 4U机箱规格书/IPC200U/4.jpg4]
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
PC size diagram
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The pictures are for reference only. Please refer to the actual product.
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	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.1
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V
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	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc21396][bookmark: _Toc1889][bookmark: _Toc23178] IPC200U-Phytium ET2000

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	Color
	black

	Compatible motherboard models
	ET2000

	Motherboard
	CPU
	Domestic Phytium Tengrui D2000, octa-core, 2.3GHz;
Domestic Phytium Tengrui FT2000 Quad-core 2.6GHz;

	
	graphics card
	Supports onboard X100 4G/8G discrete graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory supports 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 7A or 19V 5A or higher.

	
	Display Interface
	1 VGA interface (1920*1080@60Hz)
1*HDMI® 1.4 port (4096/3840*2160@30HZ)

	
	LAN
	Single gigabit network card: YT6801 or Realtek 8111H are optional;
Dual Gigabit Ethernet Adapters: YT6801 + YT8521SC or Realtek 8111H + YT8521SC (optional)
Supports Wake-on-LAN functionality;

	
	USB
	2 USB 3.1 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	Storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x4 / SATA dual-protocol adaptive standard SSDs.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 & USB signals, and WiFi/Bluetooth/4G modules; can be modified to support mSATA drives.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	Operating system
	Supports domestic operating systems such as Kylin-Desktop-V10-SP1-Release-2503-ARM64 and Linux (must support X100 version).


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 30Hz
	1024*768@60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	1*NB-DDR4
MAX 32G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc20705][bookmark: _Toc28558] IPC200U - Phytium QT2000

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	Color
	black

	Compatible motherboard models
	QT2000

	Motherboard
	CPU
	Domestic Phytium Tenlong E2000Q Quad-core 1.5GHz;

	
	graphics card
	Supports single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR4 supports 2133/2400/2666MHz memory, with a maximum support of 32GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 4A or 19V 3A or higher.

	
	Display Interface
	1 VGA interface (1024*768@60Hz)
1*HDMI® 1.4 port (1920*1080@30Hz)

	
	LAN
	Single Gigabit network card: Supports Yutai Micro YT8521SC;
Dual Gigabit Ethernet Adapters: Supports YT8521SC + YT8521SC;
Supports Wake-on-LAN functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	Storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x4 / SATA dual-protocol adaptive standard SSDs.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M2_WIFI
	One M.2 Wi-Fi interface, supporting Key-E interface M.2 2230 PCIe 3.0 x1 & USB signals, and supporting Wi-Fi and Bluetooth modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	Operating system
	Supports Kylin Embedded System (V10-SP1-General-Release-Base-2309-ARM64), Tongxin and other domestic systems.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.1
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	4
	4
	2/6
	1*M.2
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	2
	
	
	
	

	

	PC model
	[bookmark: _Toc31867][bookmark: _Toc21325] IPC200U - Phytium ET3000

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	ET3000

	motherboard
	CPU
	Domestic Phytium Tengrui D3000, octa-core 2.5GHz;

	
	graphics card
	Supports onboard X100 4G/8G discrete graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 7A or 19V 5A or higher.

	
	Display Interface
	1 VGA interface (1920*1080@60Hz)
1*HDMI® 1.4 port (4096/3840*2160@30Hz)

	
	LAN
	Single gigabit network card: YT6801 or Realtek 8111H are optional;
Dual Gigabit Ethernet Adapters: YT6801 + YT8521SC or Realtek 8111H + YT8521SC (optional)
Supports Wake-on-LAN functionality;

	
	USB
	4 USB 3.1 Gen1 ports (2 USB 3.1 Gen1 ports for dual-network PCs)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVME PCIe 4.0 x4 / SATA dual-protocol adaptive standard SSD;
Optional M.2 2242 hard drive;

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 & USB signals, and supporting WIFI, Bluetooth/4G modules; can be modified to support mSATA drives.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Supports domestic operating systems such as Kylin-Desktop-V10-SP1-Release-2503-ARM64 and Linux (must support X100 version).


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc9212][bookmark: _Toc14097] IPC200U - Zhaoxin KC6000

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	KC6000

	motherboard
	CPU
	Supports the entire series of domestic Zhaoxin KX6000 16NM surface-mount CPUs.
KX 6640MA Quad-core 2.2GHz, Turbo Boost 2.6GHz;
KX 6640A Quad-core 2.6GHz;
KX U6580 Octa-core 2.5GHz;
KX U6780A Octa-core 2.7GHz; KX U6780 Octa-core 2.7GHz

	
	graphics card
	Integrated ZX C960 DX11 super graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory supports 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 5A or higher.

	
	Display Interface
	1 VGA interface (1920*1080@60Hz)
1*HDMI® 1.4 port (4096/3840*2160@30HZ)

	
	LAN
	Single gigabit network card: Realtek 8111H or Yutaiwei YT6801 are optional;
Dual Gigabit network cards: Realtek 8111H + Realtek 8111H or Yutai Micro YT6801 + Yutai Micro YT6801 optional;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 signal and WiFi module; can be modified to support 4G/Bluetooth module.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI1®​
	VGA/ HDMI2®
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA: 2K 60Hz
HDMI2® : 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc5467][bookmark: _Toc22106][bookmark: _Toc3605] IPC200U - Zhaoxin KC7000

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	KC7000

	motherboard
	CPU
	Supports the entire series of domestic Zhaoxin KX7000 surface mount CPUs
Zhaoxin KX 7000 Octa-core 3.5GHz;

	
	graphics card
	Integrated ZX C1199 graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666/3200MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 5A or higher.

	
	Display Interface
	1 VGA interface (1920*1080@60Hz)
1*HDMI1® 2.0 port (4096/3840*2160@60Hz)
Optional 1*HDMI2® 2.0 interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card: YT6801 or Realtek 8111H are optional;
Dual Gigabit network cards: YT6801 + YT6801 or Realtek 8111H + Realtek 8111H optional;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, with default support for RS232;

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 4.0 x2 / SATA dual-protocol adaptive standard SSDs.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M2_WIFI
	One M.2 Wi-Fi interface, supporting Key-E interface M.2 2230 PCIe 4.0 x1 & USB, supporting Wi-Fi and Bluetooth modules.

	
	CN1
	One CN1 interface supports Key-B interface M.2 5G (3052/3042) modules, and the hardware can be modified to support M.2 4G (3042) modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	7
	1
	2/6
	1*MSATA
1*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	5
	
	
	
	
	

	

	PC model
	[bookmark: _Toc20841][bookmark: _Toc30690]IPC200U -J1900 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M218F, M219F, M218H, M219H, M284F, M294F, M284H, M294H, QM1800E, QM1800L, QM1900E, QM1900L

	motherboard
	CPU
	Supports Intel Bay Trail J and N series CPUs;
Intel Celeron J1800 Dual-core 2.41GHz, Turbo Boost 2.58GHz; Intel Celeron J1900 Quad-core 1.99GHz, Turbo Boost 2.4GHz;
Intel Pentium J2900 Quad-core 2.41GHz, Turbo Boost 2.66GHz;
Intel Celeron N2840 Dual-core 2.16GHz, Turbo Boost 2.58GHz; Intel Celeron N2930 Quad-core 1.83GHz, Turbo Boost 2.16GHz;
Intel Celeron N2940 Quad-core 1.83GHz, Turbo Boost 2.25GHz;

	
	graphics card
	Intel® HD Graphics graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 1.4 port (1920*1080@60Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	1 USB 3.0 port (the port under the blue group is the USB 3.0 port)
3 USB 2.0 ports (1 USB 2.0 port for dual-network PC)

	
	COM
	6 COM interfaces, default RS232; optional support for 2 RS232/RS422/RS485, or 1 RS232/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc32106][bookmark: _Toc9308]IPC200U -M316 Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M316F

	motherboard
	CPU
	Intel Celeron N3150 Quad-core 1.6GHz, Turbo Boost 2.08GHz;
Intel Celeron N3160 Quad-core 1.6GHz, Turbo Boost 2.24GHz;
Intel Celeron N3700 Quad-core 1.6GHz, Turbo Boost 2.40GHz;

	
	graphics card
	Intel® HD Graphics graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 1.4 port (1920*1080@60Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supporting 4G/ WiFi/Bluetooth modules

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*MSATA
1*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	1
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc32254][bookmark: _Toc26329]IPC200U -J3355 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M335F

	motherboard
	CPU
	Intel Celeron J3355, dual-core 2.0GHz, turbo boost 2.5GHz;
Intel Celeron J3455 Quad-core 1.5GHz, Turbo Boost 2.3GHz;
Intel Pentium N4200 Quad-core 1.1GHz, Turbo Boost 2.5GHz;

	
	graphics card
	Intel® HD Graphics 500/505 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; optional support for 2 RS232/RS422/RS485

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2242 hard drives; SATA and NVMe (PCIe) protocols are optional.

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supporting 4G/ WiFi/Bluetooth modules

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
OptionalDP 4K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	1*NB-DDR4
MAX 16G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc15828][bookmark: _Toc30827]IPC200U -J4125 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M415F

	motherboard
	CPU
	Supports Intel Gemini Lake Refresh J and N series CPUs;
Intel Celeron J4025 Dual-core 2.0GHz, Turbo Boost 2.9GHz; Intel Celeron J4125 Quad-core 2.0GHz, Turbo Boost 2.7GHz;
Intel Celeron N4020 Dual-core 1.1GHz, Turbo Boost 2.8GHz; Intel Celeron N4120 Quad-core 1.1GHz, Turbo Boost 2.6GHz;
Intel Pentium N5030 Quad-core 1.1GHz, Turbo Boost 3.1GHz; Intel Pentium J5040 Quad-core 2.0GHz, Turbo Boost 3.2GHz;

	
	graphics card
	The Intel HD Graphics 600 graphics controller supports single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 2400MHz memory, maximum support 16GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM1/COM3/COM4 are optional and support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.1
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	1*NB-DDR4
MAX 16G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc6737][bookmark: _Toc22402][bookmark: _Toc9392] IPC200U -J6412 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M612F

	motherboard
	CPU
	Supports Intel Elkhart Lake J and N series CPUs;
Intel Celeron J6412 Quad-core 2.0GHz, Turbo Boost 2.6GHz; Intel Celeron J6413 Quad-core 1.8GHz, Turbo Boost 3.0GHz;
Intel Celeron N6210 dual-core 1.2GHz, turbo boost 2.6GHz; Intel Celeron N6211 dual-core 1.2GHz, turbo boost 3.0GHz;
Intel Pentium J6426 Quad-core 2.0GHz, Turbo Boost 3.0GHz; Intel Pentium N6415 Quad-core 1.2GHz, Turbo Boost 3.0GHz;

	
	graphics card
	Intel® UHD Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 2400MHz memory, maximum support 16GB

	Front panel interface
	USB
	4 USB 2.0 ports

	
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.1 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM1/COM3/COM4/COM6 are optional and support RS232/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x2 / SATA dual-protocol adaptive standard SSDs.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 3.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
OptionalDP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	1*NB-DDR4
MAX 16G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc27213][bookmark: _Toc18051] IPC200U -M100F series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes, fanless or with silent fan cooling

	color
	black

	Compatible motherboard models
	M100F

	motherboard
	CPU
	Supports Intel Alder Lake-N series CPUs;
Intel Core i3-N300: Eight-core, 0.8GHz, turbo boost up to 3.8GHz; Core i3-N300: Eight-core, 1.8GHz, turbo boost up to 3.8GHz;
Intel N50 has a maximum turbo frequency of 3.4GHz; Intel N95 is a quad-core processor with a 1.7GHz turbo frequency of 3.4GHz.
Intel N97 Quad-core 2.0GHz, Turbo Boost 3.6GHz; Intel N100 Quad-core 0.8GHz, Turbo Boost 3.4GHz;
Intel N200 Quad-core 1.0GHz, Turbo Boost 3.7GHz;

	
	graphics card
	Intel® UHD Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 2400MHz memory, maximum support 16GB

	Front panel interface
	USB
	4 USB 2.0 ports

	
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 4A or higher power supply.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H; optional domestic Yutai Micro YT6801 gigabit network card;
Dual Gigabit Ethernet cards; supports Realtek 8111H+Realtek 8111H; optional domestic YT6801+YT6801;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM2/COM6 can be RS232/RS485; COM3/COM4 can be RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x2 / SATA dual-protocol adaptive standard SSDs.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M.2 WiFi
	One M.2 Key-E slot, supporting M.2 2230 PCIe 3.0 x1 & USB signals, and supporting WiFi and Bluetooth modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
2*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc23990][bookmark: _Toc15777]IPC200U -1037 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	1007F, 1037F, 2117F

	motherboard
	CPU
	Supports Intel Ivy Bridge Celeron series CPUs;
Intel Celeron 1007U Dual-Core 1.5GHz;
Intel Celeron 1037U Dual-Core 1.8GHz;
Intel Pentium 2117U Dual-Core 1.8GHz;

	
	graphics card
	Intel® HD Graphics 4000 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 5A or higher power supply.

	
	Display Interface
	1 HDMI 1.4 port (1920*1080@60Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM2 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	One mSATA slot supports mSATA drives; the SATA signal can be converted to the PCIe signal, which, after conversion, supports WiFi modules.

	
	SATA
	2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Windows XP, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1/2*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc24149][bookmark: _Toc4376]IPC200U -2nd Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6600, QM6637, QM6616, QM2360

	motherboard
	CPU
	Intel Core i3-2310M Dual-core 2.1GHz; Intel Core i3-2330M Dual-core 2.2GHz;
Intel Core i3-2350M Dual-core 2.3GHz; Intel Core i3-2370M Dual-core 2.4GHz;
Intel Core i5-2410M dual-core 2.3GHz, turbo boost 2.9GHz; Core i5-2430M dual-core 2.4GHz, turbo boost 3.0GHz;
Intel Core i5-2520M dual-core 2.5GHz, turbo boost 3.2GHz; Core i5-2540M dual-core 2.6GHz, turbo boost 3.3GHz;
Intel Core i7-2620M dual-core 2.7GHz, turbo boost 3.4GHz; Core i7-2640M dual-core 2.8GHz, turbo boost 3.5GHz;

	
	graphics card
	Intel® HD Graphics 3000 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, 12V 7A or higher power supply recommended.

	
	Display Interface
	1*HDMI® 1.4 port (1920*1080@60Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM2 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	1/2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Windows XP, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1/2*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc32023][bookmark: _Toc7342]IPC200U - 3rd Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	i3HGP, i5HGP, i7HGP, QM6600, QM6637, QM6616, QM2360

	motherboard
	CPU
	Intel® Ivy Bridge U and M series Core i3-3217U, i3-3110M, i5-3317U, i5-3210M, i7-3517U, i7-3520M
(See the next page for CPU list details)

	
	graphics card
	Intel® HD Graphics 4000 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1* Power interface, built-in DC power adapter. For the U series, a 12V 5A or higher power supply is recommended; for the M series, a 12V 7A or higher power supply is recommended.

	
	Display Interface
	1*HDMI® 1.4 port (1920*1080@60Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H;
Dual Gigabit Ethernet adapters; supports Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM2 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	1/2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Windows XP, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements! 
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption (W)
	Full load power consumption is approximately (W)

	3rd generation i3
	Core
	3217U
	Dual-core 1.8G
	
	17
	40

	
	
	3227U
	Dual-core 1.9G
	
	17
	40

	3rd generation i5
	Core
	3317U
	Dual-core 1.7GHz
	2.6G
	17
	40

	
	
	3337U
	Dual-core 1.8G
	2.7G
	17
	40

	
	
	3427U
	Dual-core 1.8G
	2.8G
	17
	40

	
	
	3437U
	Dual-core 1.9G
	2.9G
	17
	40

	3rd generation i7
	Core
	3517U
	Dual-core 1.9G
	3.0G
	17
	40

	
	
	3537U
	Dual-core 2.0G
	3.1G
	17
	40

	
	
	3667U
	Dual-core 2.0G
	3.2G
	17
	40

	
	
	3687U
	Dual-core 2.1G
	3.3G
	17
	40

	3rd generation i3
	Core
	3110M
	Dual-core 2.4G
	
	35
	60

	
	
	3120M
	Dual-core 2.5G
	
	35
	60

	
	
	3130M
	Dual-core 2.6G
	
	35
	60

	3rd generation i5
	Core
	3210M
	Dual-core 2.5G
	3.1G
	35
	60

	
	
	3230M
	Dual-core 2.6G
	3.2G
	35
	60

	
	
	3320M
	Dual-core 2.6G
	3.3G
	35
	60

	
	
	3340M
	Dual-core 2.7GHz
	3.4G
	35
	60

	
	
	3360M
	Dual-core 2.8G
	3.5G
	35
	60

	
	
	3380M
	Dual-core 2.9G
	3.6G
	35
	60

	3rd generation i7
	Core
	3520M
	Dual-core 2.9G
	3.6G
	35
	60

	
	
	3540M
	Dual-core 3.0G
	3.7G
	35
	60



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1/2*SATA
	1*NB-DDR3
MAX 8G
	12V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc27489][bookmark: _Toc5802]IPC200U - 4th & 5th Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	M series: QM8680, QM8680L
U series: QM9400/QM9400H/QM9400L/QM9450, QM9500/QM9500H/QM9500L/QM9550

	motherboard
	CPU
	4th generation: Intel Haswell U and M series Core i3-4005U, i3-4000M, i5-4200U, i5-4200M, i7-4500U, i7-4600M, etc.
5th generation: Intel Broadwell Core i3-5005U, i5-5200U, i7-5500U, etc.;
(See the next page for CPU list details)

	
	graphics card
	4th generation M series: Intel® HD Graphics 4600 graphics controller, supporting single display, dual display duplication, and dual display expansion;
4th generation U series: Intel® HD Graphics 4400 graphics controller, supporting single display, dual display duplication, and dual display expansion;
5th generation: Intel® HD Graphics 5500 graphics controller, supporting single display, dual display duplication, and dual display expansion;

	
	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1333/1600MHz memory, maximum support 8GB

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface

	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended 12V 5A or higher power supply.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single gigabit network card; default support for Realtek 8111H gigabit network card or Realtek 8111F gigabit network card;
Dual Gigabit Ethernet adapters; supports dual Realtek 8111H Gigabit Ethernet adapters or dual Realtek 8111F Gigabit Ethernet adapters.
Supports Wake-on-LAN and PXE functionality.

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; optional support for 1 RS232/RS422/RS485

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	It has 2 SATA 3.0 hard drive interfaces or 1 SATA 3.0 and 1 SATA 2.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 2.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	AMI BIOS supports power-on, scheduled power-on, remote power-on, and intelligent device identification.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Linux, etc.



The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	TDP power consumption (W)
	Full load power consumption is approximately (W)

	4th generation i3
	Core
	4000M
	Dual-core 2.4G
	
	37
	60

	
	
	4100M
	Dual-core 2.5G
	
	37
	60

	
	
	4110M
	Dual-core 2.6G
	
	37
	60

	4th generation i5
	Core
	4200M
	Dual-core 2.5G
	3.1G
	37
	60

	
	
	4210M
	Dual-core 2.6G
	3.2G
	37
	60

	
	
	4300M
	Dual-core 2.6G
	3.3G
	37
	60

	
	
	4310M
	Dual-core 2.7GHz
	3.4G
	37
	60

	
	
	4330M
	Dual-core 2.8G
	3.5G
	37
	60

	
	
	4340M
	Dual-core 2.9G
	3.6G
	37
	60

	4th generation i7
	Core
	4600M
	Dual-core 2.9G
	3.6G
	37
	60

	
	
	4610M
	Dual-core 3.0G
	3.7G
	37
	60

	
	Intel Pentium
	3825U
	Dual-core 1.9G
	
	10
	30

	4th generation i3
	Intel
Core
	4005U
	Dual-core 1.7GHz
	
	15
	40

	
	
	4010U
	Dual-core 1.7GHz
	
	15
	40

	
	
	4025U
	Dual-core 1.9G
	
	15
	40

	
	
	4030U
	Dual-core 1.9G
	
	15
	40

	
	
	4100U
	Dual-core 1.8G
	
	15
	40

	4th generation i5
	Intel
Core
	4200U
	Dual-core 1.6G
	2.6G
	15
	40

	
	
	4210U
	Dual-core 1.7GHz
	2.7G
	15
	40

	
	
	4250U
	Dual-core 1.3G
	2.6G
	15
	40

	
	
	4278U
	Dual-core 2.6G
	3.1G
	28
	50

	
	
	4300U
	Dual-core 1.9G
	2.9G
	15
	40

	
	
	4308U
	Dual-core 2.8G
	3.3G
	28
	50

	
	
	4310U
	Dual-core 2.0G
	3.0G
	15
	40

	4th generation i7
	Intel
Core
	4500U
	Dual-core 1.8G
	3.0G
	15
	40

	
	
	4510U
	Dual-core 2.0G
	3.1G
	15
	40

	
	
	4550U
	Dual-core 1.5G
	3.0G
	15
	40

	
	
	4558U
	Dual-core 2.8G
	3.3G
	15
	40

	
	
	4578U
	Dual-core 3.0G
	3.5G
	28
	50

	
	
	4600U
	Dual-core 2.1G
	3.3G
	15
	35

	
	
	4650U
	Dual-core 1.7GHz
	3.0G
	15
	40

	5th generation i3
	Intel
Core
	5005U
	Dual-core 2.0G
	
	15
	40

	
	
	5010U
	Dual-core 2.1G
	
	15
	40

	
	
	5015U
	Dual-core 2.1G
	
	15
	40

	
	
	5020U
	Dual-core 2.2GHz
	
	15
	40

	5th generation i5
	Intel
Core
	5200U
	Dual-core 2.2GHz
	2.7G
	15
	40

	
	
	5250U
	Dual-core 1.6G
	2.7G
	15
	40

	
	
	5257U
	Dual-core 2.7GHz
	3.1G
	15
	40

	
	
	5287U
	Dual-core 2.9G
	3.3G
	28
	50

	
	
	5300U
	Dual-core 2.3G
	2.9G
	15
	40

	
	
	5350U
	Dual-core 1.8G
	2.9G
	15
	40

	5th generation i7
	Intel
Core
	5500U
	Dual-core 2.4G
	3.0G
	15
	40

	
	
	5550U
	Dual-core 2.0G
	3.0G
	15
	40

	
	
	5557U
	Dual-core 3.1GHz
	3.4G
	28
	50

	
	
	5600U
	Dual-core 2.6G
	3.2G
	15
	40

	
	
	5650U
	Dual-core 2.2GHz
	3.1G
	15
	40



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
2*SATA
	2*NB-DDR3
MAX 32G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc31622][bookmark: _Toc27964][bookmark: _Toc1647] IPC200U - 6th and 7th generation series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9600, QM9700, QM9600H, QM9700H

	motherboard
	CPU
	6th generation: Intel® Celeron 3855U, 3955U and Sky Lake Core i3-6100U, i5-6200U, i7-6500U, etc.;
7th generation: Intel® Celeron 3865U, 3965U and Kaby Lake Core i3-7100U, i5-7200U, i7-7500U, etc.;
(See the next page for CPU list details)

	
	graphics card
	6th generation: Intel® HD Graphics 510/520 graphics controller, supporting single display, dual display duplication, and dual display expansion.
7th generation: Intel® HD Graphics 610/620 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR3 memory modules, supporting 1.35V, 1600MHz memory, maximum support 32GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended power supply is 12V 5A or 19V 3A or higher.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30HZ)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Supports Realtek 8111F, Realtek 8111H, or Yutaiwei YT6801 Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Supports Realtek 8111F + Realtek 8111F or optionally supports Realtek 8111H + Intel I219-LM
Alternatively, it may support Yutai Micro YT6801+ Intel I219-LM;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, default RS232; COM2 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 signal and WiFi module; optional support for WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	TDP power consumption (W)
	Full load power consumption is approximately (W)

	6th generation
	Cy Young
	3855U
	Dual-core 1.6G
	
	15
	40

	
	
	3955U
	Dual-core 2.0G
	
	15
	40

	6th generation i3
	Core
	6006U
	Dual-core 2.0G
	
	15
	40

	
	
	6100U
	Dual-core 2.3G
	
	15
	40

	6th generation i5
	Core
	6200U
	Dual-core 2.3G
	2.8G
	15
	40

	
	
	6300U
	Dual-core 2.4G
	3.0G
	15
	40

	6th generation i7
	Core
	6500U
	Dual-core 2.5G
	3.1G
	15
	40

	
	
	6600U
	Dual-core 2.6G
	3.4G
	15
	40

	
	
	6650U
	Dual-core 2.2GHz
	3.4G
	15
	40

	7th generation
	Cy Young
	3865U
	Dual-core 1.8G
	
	15
	40

	
	
	3965U
	Dual-core 2.2GHz
	
	15
	40

	7th generation i3
	Core
	7020U
	Dual-core 2.3G
	
	15
	40

	
	
	7100U
	Dual-core 2.4G
	
	15
	40

	
	
	7130U
	Dual-core 2.7GHz
	
	15
	40

	7th Gen i5
	Core
	7200U
	Dual-core 2.5G
	3.1G
	15
	40

	
	
	7300U
	Dual-core 2.6G
	3.5G
	15
	40

	7th generation i7
	Core
	7500U
	Dual-core 2.7GHz
	3.5G
	15
	40

	
	
	7600U
	Dual-core 2.8G
	3.9G
	15
	40



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 32G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc16926][bookmark: _Toc12382][bookmark: _Toc18941] IPC200U -QM9850 Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9650, QM9750, QM9850

	motherboard
	CPU
	6th generation: Intel® Celeron 3855U, 3955U and Sky Lake Core i3-6100U, i5-6200U, i7-6500U, etc.;
7th generation: Intel® Celeron 3865U, 3965U and Kaby Lake Core i3-7100U, i5-7200U, i7-7500U, etc.;
8th generation: Intel® Kaby Lake R Core i3-8130U, i5-8250U, i7-8550U, etc.;
(See the next page for CPU list details)

	
	graphics card
	6th generation: Intel® HD Graphics 510/520 graphics controller, supporting single display, dual display duplication, and dual display expansion;
7th generation: Intel® HD Graphics 610/620 graphics controller, supporting single display, dual display duplication, and dual display expansion;
8th generation: Intel® UHD Graphics 620 graphics controller, supporting single display, dual display duplication, and dual display expansion;

	
	Memory
	2*NB-DDR4 memory supports 2133/2400MHz, with a maximum capacity of 32GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended power supply is 12V 7A or 19V 4A or higher.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card: Realtek 8111H;
Dual Gigabit Ethernet adapters: Realtek 8111H + Realtek 8111H;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	One M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x4 / SATA adaptive standard SSDs; optional M.2 2242 hard drive.

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 signal and WiFi module; optional support for WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	6th and 7th generation: Windows 10, Windows 7, Linux, etc.
8th generation: Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	TDP power consumption (W)
	Full load power consumption is approximately (W)

	6th generation
	Cy Young
	3855U
	Dual-core 1.6G
	
	15
	40

	
	
	3955U
	Dual-core 2.0G
	
	15
	40

	6th generation i3
	Core
	6006U
	Dual-core 2.0G
	
	15
	40

	
	
	6100U
	Dual-core 2.3G
	
	15
	40

	6th generation i5
	Core
	6200U
	Dual-core 2.3G
	2.8G
	15
	40

	
	
	6300U
	Dual-core 2.4G
	3.0G
	15
	40

	6th generation i7
	Core
	6500U
	Dual-core 2.5G
	3.1G
	15
	40

	
	
	6600U
	Dual-core 2.6G
	3.4G
	15
	40

	
	
	6650U
	Dual-core 2.2GHz
	3.4G
	15
	40

	7th generation i3
	Core
	7020U
	Dual-core 2.3G
	
	15
	40

	
	
	7100U
	Dual-core 2.4G
	
	15
	40

	
	
	7130U
	Dual-core 2.7GHz
	
	15
	40

	7th Gen i5
	Core
	7200U
	Dual-core 2.5G
	3.1G
	15
	40

	
	
	7300U
	Dual-core 2.6G
	3.5G
	15
	40

	7th generation i7
	Core
	7500U
	Dual-core 2.7GHz
	3.5G
	15
	40

	
	
	7600U
	Dual-core 2.8G
	3.9G
	15
	40

	8th generation i3
	Core
	8130U
	Dual-core 2.2GHz
	3.4G
	15
	60

	8th Gen i5
	Core
	8250U
	Quad-core 1.6GHz
	3.4G
	15
	60

	
	
	8350U
	Quad-core 1.7GHz
	3.6G
	15
	60

	8th Gen i7
	Core
	8550U
	Quad-core 1.8GHz
	4.0G
	15
	60

	
	
	8650U
	Quad-core 1.9GHz
	4.2G
	15
	60



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1/2*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc16775][bookmark: _Toc6328][bookmark: _Toc29205] IPC200U - 8th and 10th Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM8H, QM9H, QM10H, QM8U, QM10U

	motherboard
	CPU
	QM8H/QM8U: Intel® Whiskey Lake 8th generation Core i3-8145U, i5-8265U, i7-8565U, etc.;
QM9H: Intel® Coffee Lake 8th generation Core i3-8109U, i5-8259U, i7-8559U, etc.;
QM10H/QM10U: Intel Comet Lake 10th generation Core i3-10110U, i5-10210U, i7-10510U, etc.;
(See the next page for CPU list details)

	
	graphics card
	Intel® UHD Graphics graphics controller, supporting single display, dual display duplication, and dual display expansion;

	
	Memory
	2*NB-DDR4 memory supports 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended power supply is 12V 7A or 19V 5A or higher.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111H Gigabit Ethernet adapter; optional Yutai Micro YT6801 Gigabit Ethernet adapter;
Dual Gigabit Ethernet Adapters: Realtek 8111H + Realtek 8111H Gigabit Ethernet Adapter; Optional: YT6801 + YT6801 Gigabit Ethernet Adapter
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	One M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x4 / SATA adaptive standard SSDs; optional M.2 2242 hard drive.

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	1/2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	One Mini-PCIe slot, supporting PCIe 3.0 x1 signal and WiFi module; optional support for WiFi, Bluetooth/4G modules.

	
	M.2_5G
	One optional M.2 Key-B slot, supporting M.2 5G (3052/3042) modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU Model
	clock speed
	Turbo Boost
	TDP power consumption
	The full load power consumption of the entire board is approximately

	
	Cy Young
	4305U
	Dual-core 2.2GHz
	/
	15W
	60W

	8th generation i3
	Core
	8145U
	Dual-core 2.1G
	3.9G
	15W
	60W

	8th Gen i5
	Core
	8365U
	Quad-core 1.6GHz
	4.1G
	15W
	60W

	
	
	8265U
	Quad-core 1.6GHz
	3.9G
	15W
	60W

	8th Gen i7
	Core
	8665U
	Quad-core 1.9GHz
	4.8G
	15W
	60W

	
	
	8565U
	Quad-core 1.8GHz
	4.6G
	15W
	60W

	8th generation i3
(QM9H)
	Core
	8109U
	Dual-core 3.0G
	3.6G
	28W
	70W

	
	
	8140U
	Dual-core 2.1G
	3.9G
	15W
	60W

	8th generation i5
(QM9H)
	Core
	8259U
	Quad-core 2.3GHz
	3.8G
	28W
	70W

	
	
	8269U
	Quad-core 2.6GHz
	4.2G
	28W
	70W

	
	
	8279U
	Quad-core 2.4GHz
	4.1G
	28W
	70W

	
	
	8257U
	Quad-core 1.4GHz
	3.9G
	15W
	60W

	
	
	8260U
	Quad-core 1.6GHz
	3.9G
	15W
	60W

	8th Gen i7
(QM9H)
	Core
	8559U
	Quad-core 2.7GHz
	4.50
	28W
	70W

	
	
	8569U
	Quad-core 2.8GHz
	4.7G
	28W
	70W

	
	
	8557U
	Quad-core 1.7GHz
	4.5G
	15W
	60W

	10th Gen i3
	Core
	10110U
	Dual-core 2.1G
	4.10G
	15W
	60W

	10th Gen i5
	Core
	10310U
	Quad-core 1.7GHz
	4.40G
	15W
	60W

	
	
	10210U
	Quad-core 1.6GHz
	4.20G
	15W
	60W

	10th Gen i7
	Core
	10510U
	Quad-core 1.8GHz
	4.90G
	15W
	60W

	
	
	10610U
	Quad-core 1.8GHz
	4.90G
	15W
	60W

	
	
	10810U
	Six-core 1.1GHz
	4.90G
	15W
	60W

	
	
	10710U
	Six-core 1.1GHz
	4.70G
	15W
	60W



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc20166][bookmark: _Toc11895][bookmark: _Toc29083] IPC200U - 11th Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM11U, QM11H

	motherboard
	CPU
	Supports Intel® Tiger Lake 11th Gen CPUs: i3-1115G4E, i5-1145G7E, i7-1185GRE, etc.
(See the next page for a detailed list of CPU information)

	
	graphics card
	Intel® UHD Graphics / Intel Iris Xe Graphics controller, supporting single display, dual display duplication, and dual display expansion;

	
	Memory
	2*NB-DDR4 memory supports 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V, recommended power supply is 12V 7A or 19V 5A or higher.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Intel i219V Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Supports Intel i219V + Realtek 8111H Gigabit Ethernet adapters, with optional support for Intel i219V + Realtek 8111H Gigabit Ethernet adapters;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1/COM2 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	One M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 3.0 x4 / SATA adaptive standard SSDs; optional M.2 2242 hard drive.

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	1/2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 3.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!

	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	TDP power consumption (W)

	
	Cy Young
	6305E
	Dual-core 2.8G
	/
	15

	11th Gen i3
	Core
	1115G4E
	Dual-core 2.2GHz
	3.9G
	15

	
	Core
	1115GRE
	Dual-core 2.2GHz
	3.9G
	15

	
	Core
	1115G4
	Dual-core 3.0G
	4.1G
	28

	
	Core
	1125G4
	Quad-core 2.0GHz
	3.7G
	28

	11th Gen i5
	Core
	1145G7E
	Quad-core 1.5GHz
	4.1G
	15

	
	Core
	1145GRE
	Quad-core 1.5GHz
	4.1G
	15

	
	Core
	1145G7
	Quad-core 2.6GHz
	4.4G
	28

	
	Core
	1135G7
	Quad-core 2.4GHz
	4.2G
	28

	
	Core
	1155G7
	Quad-core 2.5GHz
	4.4G
	28

	
	Core
	11300H
	Quad-core 3.1GHz
	4.4G
	35

	
	Core
	11320H
	Quad-core 3.2GHz
	4.5G
	35

	11th Gen i7
	Core
	1185GRE
	Quad-core 1.8GHz
	4.4G
	15

	
	Core
	1185G7E
	Quad-core 1.8GHz
	4.4G
	15

	
	Core
	1185G7
	Quad-core 3.0GHz
	4.8G
	28

	
	Core
	1165G7
	Quad-core 2.8GHz
	4.7G
	28

	
	Core
	1195G7
	Quad-core 2.9GHz
	5.0G
	28

	
	Core
	11370H
	Quad-core 3.3GHz
	4.8G
	35

	
	Core
	11375H
	Quad-core 3.3GHz
	5.0G
	35

	
	Core
	11390H
	Quad-core 3.4GHz
	5.0G
	35



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc17762][bookmark: _Toc7363][bookmark: _Toc19319][bookmark: _Toc30700] IPC200U - 12th and 13th Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM12U, QM13U, QM12P, QM13P, QM12H, QM13H

	motherboard
	CPU
	Supports Intel® Alder Lake 12th generation U, P, and H series Core i3-1215U, i5-1235U, i7-1260P, i9-12900H, etc.
Supports Intel® Raptor Lake 13th generation U, P, and H series Core i3-1305U, i5-1334U, i7-1340P, i9-13900H, etc.
(See the next page for a complete CPU list)

	
	graphics card
	Intel® UHD Graphics / Intel Iris Xe Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666/2933/3200MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V.
The maximum turbo frequency power consumption of U-series CPUs is 55W, and it is recommended to use a power supply with 12V 7A or 19V 5A or higher.
The maximum turbo frequency power consumption of P-series CPUs is 64W, and it is recommended to use a power supply with 12V 7A or 19V 5A or higher.
The maximum turbo frequency power consumption of H-series CPUs is 115W, and it is recommended to use a power supply of 12V 10A or 19V 6.3A or higher.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Intel i219V Gigabit Ethernet adapter;
Dual Gigabit Ethernet Adapters: Intel i219V + Realtek 8111H Gigabit Ethernet Adapter
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 4.0 x4 / SATA adaptive standard SSD; optional M.2 2242 hard drive;

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M.2 WiFi
	1 M.2 Key-E slot, supports M.2 2230 PCIe 3.0 x1 & USB, supports WiFi and Bluetooth modules.

	
	M.2_5G
	One M.2 Key-B slot, supporting M.2 5G (3052/3042) modules or M.2 4G (3042) modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	kernel/thread
	clock speed
	Turbo Boost
	CPU base power consumption (W)
	Maximum turbo power consumption (W)

	12th Gen i3
	Core
	1215U
	Six cores and eight threads
	1.2G
	4.4G
	15
	55

	12th Gen i5
	Core
	1235U
	Ten cores and twelve threads
	1.3G
	4.4G
	15
	55

	
	
	1245U
	Ten cores and twelve threads
	1.6G
	4.4G
	15
	55

	12th Gen i7
	Core
	1265U
	Ten cores and twelve threads
	1.8G
	4.8G
	15
	55

	
	
	1255U
	Ten cores and twelve threads
	1.7G
	4.7G
	15
	55

	13th generation i3
	Core
	1305U
	Five cores and six threads
	1.6G
	4.5G
	15
	55

	
	
	1315U
	Six cores and eight threads
	1.2G
	4.5G
	15
	55

	13th Gen i5
	Core
	1334U
	Ten cores and twelve threads
	1.3G
	4.6G
	15
	55

	
	
	1335U
	Ten cores and twelve threads
	1.3G
	4.6G
	15
	55

	
	
	1345U
	Ten cores and twelve threads
	1.6G
	4.7G
	15
	55

	13th Gen i7
	Core
	1355U
	Ten cores and twelve threads
	1.7G
	5.0G
	15
	55

	
	
	1365U
	Ten cores and twelve threads
	1.8G
	5.2G
	15
	55

	12th Gen i3
	Core
	1220P
	Ten cores and twelve threads
	1.5G
	4.4G
	28
	64

	12th Gen i5
	Core
	1240P
	Twelve cores and sixteen threads
	1.7G
	4.4G
	28
	64

	
	
	1250P
	Twelve cores and sixteen threads
	1.7G
	4.4G
	28
	64

	12th Gen i7
	Core
	1280P
	Fourteen cores and twenty threads
	1.8G
	4.8G
	28
	64

	
	
	1260P
	Twelve cores and sixteen threads
	2.1G
	4.7G
	28
	64

	
	
	1270P
	Twelve cores and sixteen threads
	2.2G
	4.8G
	28
	64

	13th Gen i5
	Core
	1340P
	Twelve cores and sixteen threads
	1.8G
	4.6G
	28
	64

	
	
	1350P
	Twelve cores and sixteen threads
	1.9G
	4.7G
	28
	64

	13th Gen i7
	Core
	1360P
	Twelve cores and sixteen threads
	2.2G
	5.0G
	28
	64

	
	
	1370P
	Fourteen cores and twenty threads
	1.9G
	5.2G
	28
	64

	12th Gen i5
	Core
	12450H
	Eight cores and twelve threads
	2.0G
	4.4G
	45
	95

	
	
	12500H
	Twelve cores and sixteen threads
	2.5G
	4.5G
	45
	95

	
	
	12600H
	Twelve cores and sixteen threads
	2.7G
	4.5G
	45
	95

	12th Gen i7
	Core
	12800H
	Fourteen cores and twenty threads
	2.4G
	4.8G
	45
	115

	
	
	12700H
	Fourteen cores and twenty threads
	2.7G
	4.7G
	45
	115

	
	
	12650H
	Ten cores and sixteen threads
	2.3G
	4.7G
	45
	115

	12th Gen i9
	Core
	12900H
	Fourteen cores and twenty threads
	2.5G
	5.0G
	45
	115

	13th Gen i5
	Core
	13420H
	Eight cores and twelve threads
	2.1G
	4.60G
	45
	95

	
	
	13500H
	Twelve cores and sixteen threads
	2.6G
	4.70G
	45
	95

	
	
	13600H
	Twelve cores and sixteen threads
	2.8G
	4.80G
	45
	95

	13th Gen i7
	Core
	13620H
	Ten cores and sixteen threads
	2.4G
	4.90G
	45
	115

	
	
	13700H
	Fourteen cores and twenty threads
	2.4G
	5.00G
	45
	115

	
	
	13800H
	Fourteen cores and twenty threads
	2.5G
	5.20G
	45
	115

	13th generation i9
	Core
	13900H
	Fourteen cores and twenty threads
	2.6G
	5.40G
	45
	115



	CPU
brand
	CPU
Specification
	CPU
model
	kernel/thread
	Performance core (P core)
	Energy efficiency core (E core)
	CPU base power consumption (W)
	CPU maximum turbo frequency power consumption (W)

	
	
	
	
	Basic frequency
	Turbo Boost
	Basic frequency
	Turbo Boost
	
	

	Intel
	Core 3
	100U
	Six cores and eight threads
	1.2G
	4.7G
	900M
	3.3G
	15
	55

	Intel
	Core 5
	120U
	Ten cores and twelve threads
	1.4G
	5.0G
	900M
	3.8G
	15
	55

	
	
	220U
	Ten cores and twelve threads
	1.4G
	5.0G
	900M
	3.8G
	15
	55

	
	
	210H
	Eight cores and twelve threads
	2.2G
	/
	1.6G
	3.6G
	45
	115

	
	
	220H
	Twelve cores and sixteen threads
	2.7G
	/
	2.0G
	3.7G
	45
	115

	Intel
	Core 7
	150U
	Ten cores and twelve threads
	1.8G
	5.4G
	1.2G
	4.0G
	15
	55

	
	
	250U
	Ten cores and twelve threads
	1.8G
	5.4G
	1.2G
	4.0G
	15
	55

	
	
	240H
	Ten cores and sixteen threads
	2.5G
	5.2G
	1.8G
	4.0G
	45
	115

	
	
	250H
	Fourteen cores and twenty threads
	2.5G
	5.4G
	1.8G
	4.0G
	45
	115

	Intel
	Core 9
	270H
	Fourteen cores and twenty threads
	2.7G
	5.8G
	2.0G
	4.1G
	45
	115


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 8K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	Onboard
LPDDR4 16G
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc4405][bookmark: _Toc10242] IPC200U - QM12M

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM12M

	motherboard
	CPU
	Supports Intel® Alder Lake-M 12th generation:
Intel Pentium 8200U: Five cores, 1.0GHz, turbo boost up to 4.4GHz;
Intel Core i3-1210U, six cores, 1.0GHz, turbo boost up to 4.4GHz;
Intel Core i5-1230U: 10 cores, 1.0GHz, turbo boost up to 4.4GHz;
Intel Core i5-1240U: 10 cores, 1.1GHz, turbo boost up to 4.4GHz;
Intel Core i7-1250U: 10 cores, 1.1GHz, turbo boost up to 4.7GHz;
Intel Core i7-1260U: 10 cores, 1.1GHz, turbo boost up to 4.7GHz;

	
	graphics card
	Intel® UHD Graphics / Intel Iris Xe Graphics integrated graphics, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	It supports 16GB of onboard LPDDR4 4000MHz by default, with an optional maximum support of 64GB 4267MHz.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended to use a 12V 5A or 19V 3A or higher power supply.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (7680 x 2160 @ 60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111H Gigabit Ethernet adapter, with optional support for Yutai Micro YT6801 Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Realtek 8111H + Realtek 8111H Gigabit Ethernet adapter; optional support for YT6801 + YT6801 Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 4.0 x4 / SATA adaptive standard SSD; optional M.2 2242 hard drive;

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M.2 WiFi
	1 M.2 Key-E slot, supports M.2 2230 PCIe 3.0 x1 & USB, supports WiFi and Bluetooth modules.

	
	M.2_5G
	One M.2 Key-B slot, supporting M.2 5G (3052/3042) modules or M.2 4G (3042) modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 8K 120Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 96G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc14776][bookmark: _Toc6590][bookmark: _Toc8230][bookmark: _Toc16055] IPC200U - 14th Generation Series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM14U, QM14H, QM15U, 1M15H

	motherboard
	CPU
	Supports Intel® Meteor Lake 14th generation U/H series Core processors: Ultra 5-125U, Ultra 7-155U, Ultra 7-155H, Ultra 9-185H, etc.
Supports Intel® Arrow Lake 15th generation U/H series Core processors such as Ultra 5-225U, Ultra 7-255U, and Ultra 9-285H.
(See the next page for a complete CPU list)

	
	graphics card
	Integrated Intel® Graphics /Intel Arc Graphics hyper-graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR5 memory modules support 4800/5600MT/s, with a maximum capacity of 96GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V.
The maximum turbo frequency power consumption of U-series CPUs is 57W, and it is recommended to use a power supply with 12V 7A or 19V 5A or higher.
The maximum turbo frequency power consumption of H-series CPUs is 115W, and it is recommended to use a power supply of 12V 10A or 19V 6.3A or higher.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (7680*2160@120Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Intel i219V Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Intel i219V + Realtek 8111H Gigabit Ethernet adapter, with optional support for Intel i219V + Yutai Micro YT6801 Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 NVMe PCIe 4.0 x4 / SATA adaptive standard SSD; optional M.2 2242 hard drive;

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M.2 WiFi
	1 M.2 Key-E slot, supports M.2 2230 PCIe 4.0 x1 & USB, supports WiFi and Bluetooth modules.

	
	M.2_5G
	One M.2 Key-B slot, supporting M.2 5G (3052/3042) modules or M.2 4G (3042) modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU
brand
	CPU
Specification
	CPU
model
	kernel/thread
	Performance core (P core)
	Energy efficiency core (E core)
	CPU base power consumption (W)
	CPU maximum turbo frequency power consumption (W)

	
	
	
	
	Basic frequency
	Turbo Boost
	Basic frequency
	Turbo Boost
	
	

	Intel
Core
	14th generation
Ultra 5
	125U
	Twelve cores and fourteen threads
	1.3G
	4.3G
	800M
	3.6G
	15
	57

	
	
	135U
	Twelve cores and fourteen threads
	1.6G
	4.4G
	1.1G
	3.6G
	15
	57

	
	
	125H
	Fourteen cores and eighteen threads
	1.2G
	4.5G
	700M
	3.6G
	28
	115

	
	
	135H
	Fourteen cores and eighteen threads
	1.7G
	4.6G
	1.2G
	3.6G
	28
	115

	Intel
Core
	14th generation
Ultra 7
	155U
	Twelve cores and fourteen threads
	1.7G
	4.8G
	1.2G
	3.8G
	15
	57

	
	
	165U
	Twelve cores and fourteen threads
	1.7G
	4.9G
	1.2G
	3.8G
	15
	57

	
	
	155H
	Sixteen cores and twenty-two threads
	1.4G
	4.8G
	900M
	3.8G
	28
	115

	
	
	165H
	Sixteen cores and twenty-two threads
	1.4G
	5.0G
	900M
	3.8G
	28
	115

	Intel
Core
	14th generation
Ultra 9
	185H
	Sixteen cores and twenty-two threads
	2.3G
	5.1G
	1.8G
	3.8G
	45
	115

	Intel
Core
	15th generation
Ultra 5
	225U
	Twelve cores and fourteen threads
	1.5G
	4.8G
	1.3G
	3.8G
	15
	57

	
	
	235U
	Twelve cores and fourteen threads
	2.0G
	4.9G
	1.6G
	4.1G
	15
	57

	
	
	225H
	Fourteen cores and fourteen threads
	1.7G
	4.9G
	1.3G
	4.3G
	28
	115

	
	
	235H
	Fourteen cores and fourteen threads
	2.4G
	5.0G
	1.8G
	4.4G
	28
	115

	Intel
Core
	15th generation
Ultra 7
	255U
	Twelve cores and fourteen threads
	2.0G
	5.2G
	1.7G
	4.2G
	15
	57

	
	
	265U
	Twelve cores and fourteen threads
	2.1G
	5.3G
	1.7G
	4.2G
	15
	57

	
	
	255H
	Sixteen cores and sixteen threads
	2.2G
	5.1G
	1.5G
	4.4G
	28
	115

	
	
	265H
	Sixteen cores and sixteen threads
	2.2G
	5.3G
	1.7G
	4.5G
	28
	115

	Intel
Core
	15th generation
Ultra 9
	285H
	Sixteen cores and sixteen threads
	2.9G
	5.4G
	2.7G
	4.5G
	45
	115


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz
	1
	3
	4
	2/6
	1*M.2
2*SATA
Optional 1*MSATA
	1*NB-DDR4
MAX 16G
	12V/19V

	
	
	2
	2
	
	
	
	
	

	

	PC model
	[bookmark: _Toc4080][bookmark: _Toc28933] IPC200U -QM1100

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM1100

	motherboard
	CPU
	Supports SkyLake 6th generation LGA1151 Core i3-6100, i5-6400, i7-6700, etc.
Supports Kaby Lake 7th generation LGA1151 Core i3-7100, i5-7400, i7-7700, etc.
(See the next page for a complete CPU list)

	
	graphics card
	6th generation: Intel® HD Graphics 530 graphics controller, supporting single display, dual display expansion, and dual display duplication.
7th generation: Intel® HD Graphics 630 graphics controller, supporting single display, dual display expansion, and dual display duplication.

	
	Memory
	1*NB-DDR4 supports 2133/2400MHz memory, with a maximum support of 16GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	2 USB 3.0 ports
1 USB 2.0 port (dual-network PC supports 2 USB 2.0 ports)

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 6A or higher.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111F Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Realtek 8111F + Realtek 8111F Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2 SSD
	1 M.2 Key-M slot, supporting M.2 2280 SATA protocol, with optional M.2 NVMe PCIe 3.0 x4 protocol; optional M.2 2242 hard drive;

	
	mSATA
	One mSATA slot is optional, supporting mSATA drives.

	
	SATA
	2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 3.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Supports Windows 10, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption is approximately (W)
	CPU full load power consumption (W)

	6th generation i3
	Intel
Core
	6100
	Dual-core 3.7G
	
	65
	90

	
	
	6300
	Dual-core 3.8G
	
	65
	90

	
	
	6320
	Dual-core 3.9G
	
	65
	90

	6th generation i5
	Intel
Core
	6400
	Quad-core 2.7GHz
	3.3G
	65
	90

	
	
	6500
	Quad-core 3.2GHz
	3.6G
	65
	90

	
	
	6600
	Quad-core 3.3GHz
	3.9G
	65
	90

	6th generation i7
	Intel Core
	6700
	Quad-core 3.4GHz
	4.0G
	65
	90

	7th generation i3
	Intel
Core
	7100
	Dual-core 3.9G
	
	65
	90

	
	
	7300
	Dual-core 4.0G
	
	65
	90

	
	
	7320
	Dual-core 4.1G
	
	65
	90

	7th Gen i5
	Intel
Core
	7400
	Quad-core 3.0GHz
	3.5G
	65
	90

	
	
	7500
	Quad-core 3.4GHz
	3.8G
	65
	90

	
	
	7600
	Quad-core 3.5GHz
	4.1G
	65
	90

	7th generation i7
	Intel Core
	7700
	Quad-core 3.6GHz
	4.2G
	65
	90





※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc10491][bookmark: _Toc7809] IPC200U -H310 series

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM3100, QM3600

	motherboard
	CPU
	Supports Intel® Skylate 6th generation LGA1151 Core i3-6100, i5-6400, i7-6700, etc.
Supports Intel® Kaby Lake 7th generation LGA1151 Core i3-7100, i5-7400, i7-7700, etc.
Supports Intel® Coffee Lake 8th generation LGA1151 Core i3-8100, i5-8400, i7-8700, etc.
Supports Intel® Coffee Lake 9th generation LGA1151 Core i3-9100, i5-9400, i7-9700, i9-9900, etc.
(See the next page for a complete CPU list)

	
	graphics card
	6th generation: Intel® HD Graphics 530 graphics controller, supporting single display, dual display expansion, and dual display duplication.
7th generation: Intel® HD Graphics 630 graphics controller, supporting single display, dual display expansion, and dual display duplication.
8th and 9th generation: Intel® UHD Graphics 630 graphics controller, supporting single display, dual display expansion, and dual display duplication.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 6A or higher.

	
	Display Interface
	1*HDMI® 1.4 port (4096/3840*2160@30Hz)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111H Gigabit Ethernet adapter, optional Yutai Micro YT6801 Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Realtek 8111H + Realtek 8111H Gigabit Ethernet adapter, optional Yutai Micro YT6801 + Yutai Micro YT6801 Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.0 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 3.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	6th and 7th generation motherboards support: Windows 11, Windows 10, Windows 8, Windows 7, Linux, etc.
8th and 9th generation motherboards support: Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The CPU information below is for reference only. Please consult our sales team for specific requirements!
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption is approximately (W)
	CPU full load power consumption (W)

	6th generation i3
	Intel
Core
	6100
	Dual-core 3.7G
	
	65
	90

	
	
	6300
	Dual-core 3.8G
	
	65
	90

	
	
	6320
	Dual-core 3.9G
	
	65
	90

	6th generation i5
	Intel
Core
	6400
	Quad-core 2.7GHz
	3.3G
	65
	90

	
	
	6500
	Quad-core 3.2GHz
	3.6G
	65
	90

	
	
	6600
	Quad-core 3.3GHz
	3.9G
	65
	90

	6th generation i7
	Intel Core
	6700
	Quad-core 3.4GHz
	4.0G
	65
	90

	7th generation i3
	Intel
Core
	7100
	Dual-core 3.9G
	
	65
	90

	
	
	7300
	Dual-core 4.0G
	
	65
	90

	
	
	7320
	Dual-core 4.1G
	
	65
	90

	7th Gen i5
	Intel
Core
	7400
	Quad-core 3.0GHz
	3.5G
	65
	90

	
	
	7500
	Quad-core 3.4GHz
	3.8G
	65
	90

	
	
	7600
	Quad-core 3.5GHz
	4.1G
	65
	90

	7th generation i7
	Intel Core
	7700
	Quad-core 3.6GHz
	4.2G
	65
	90

	8th generation i3
	Intel
Core
	8100
	Quad-core 3.6GHz
	
	65
	90

	
	
	8300
	Quad-core 3.7GHz
	
	65
	90

	8th Gen i5
	Intel
Core
	8400
	Six-core 2.8GHz
	4.0G
	65
	90

	
	
	8500
	Six-core 3.0GHz
	4.1G
	65
	90

	
	
	8600
	Six-core 3.2GHz
	4.3G
	65
	90

	8th Gen i7
	Intel Core
	8700
	Six-core 3.2GHz
	4.6G
	65
	90

	9th generation i3
	Intel Core
	9100
	Quad-core 3.6GHz
	4.2G
	65
	90

	
	
	9300
	Quad-core 3.7GHz
	4.2G
	65
	90

	9th Gen i5
	Intel
Core
	9400
	Six-core 2.9GHz
	4.1G
	65
	90

	
	
	9500
	Six-core 3.0GHz
	4.4G
	65
	90

	
	
	9600
	Six-core 3.1GHz
	4.6G
	65
	90

	9th Gen i7
	Intel Core
	9700
	Octa-core 3.0G
	4.7G
	65
	90

	9th generation I9
	Intel Core
	9900
	Octa-core 3.1GHz
	5.0G
	65
	90



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
Optional 4K 60Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*MSATA
2*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc4560][bookmark: _Toc10726] IPC200U -QM5100

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM5100

	motherboard
	CPU
	Supports Intel® Comet late 10th generation LGA1200 Core i3-10100, i5-10400, i7-10700, i9-10900, etc.
Supports Intel® Rocket Lake 11th Gen LGA1200 Core i5-11400, i7-11700, i9-11900, etc.
(See the next page for a complete CPU list)

	
	graphics card
	10th Gen: Intel® HD Graphics 630 integrated graphics, supporting single display, dual display duplication, and dual display expansion;
11th Gen: Intel® HD Graphics 730/750 integrated graphics, supporting single display, dual display duplication, and dual display expansion;

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666/2933MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 6A or higher.

	
	Display Interface
	1 HDMI® port
When the CPU is an 11th generation i5/i7/i9, the motherboard's HDMI® 2.0 supports 4K@60Hz;
When the CPU is a 10th generation i3/i5/i7/i9, the motherboard's HDMI® 1.4 supports 4K@30Hz.
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111H Gigabit Ethernet adapter, with optional support for Yutai Micro YT6801 Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Realtek 8111H + Realtek 8111H Gigabit Ethernet adapter, with optional support for Yutai Micro YT6801 + Yutai Micro YT6801 Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM interfaces, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	mSATA
	1 mSATA slot, supports mSATA drives

	
	SATA
	2 SATA 3.0 hard drive interfaces, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIe slot, supports PCIe 3.0 x1 & USB signal, supports WiFi, Bluetooth/4G modules.

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Supports Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!

	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power (W)
	Full load power consumption (W)

	10th Gen i3
	Intel Core
	10100
	Quad-core 3.6GHz
	4.3G
	65
	110

	
	
	10105
	Quad-core 3.7GHz
	4.4G
	65
	110

	
	
	10300
	Quad-core 3.7GHz
	4.4G
	65
	110

	
	
	10305
	Quad-core 3.8GHz
	4.5G
	65
	110

	
	
	10320
	Quad-core 3.8GHz
	4.6G
	65
	110

	
	
	10325
	Quad-core 3.9GHz
	4.7G
	65
	110

	10th Gen i5
	Intel Core
	10400
	Six-core 2.9GHz
	4.3G
	65
	110

	
	
	10505
	Six-core 3.2GHz
	4.6G
	65
	110

	
	
	10500
	Six-core 3.1GHz
	4.5G
	65
	110

	
	
	10600
	Six-core 3.3GHz
	4.8G
	65
	110

	10th Gen i7
	Intel Core
	10700
	Octa- core 2.9GHz
	4.8G
	65
	110

	10th Gen i9
	Intel Core
	10900
	Deca core 2.8G
	5.2G
	65
	110

	11th Gen i5
	Intel Core
	11400
	Six-core 2.6GHz
	4.4G
	65
	110

	
	
	11500
	Six-core 2.7GHz
	4.6G
	65
	110

	
	
	11600
	Six-core 2.8GHz
	4.8G
	65
	110

	11th Gen i7
	Intel Core
	11700
	Octa-core 2.5GHz
	4.9G
	65
	110

	11th Gen i9
	Intel Core
	11900
	Octa-core 2.5GHz
	5.2G
	65
	110



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®​
	VGA/DP
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc11379][bookmark: _Toc8909] IPC200U -QM6100

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6100

	motherboard
	CPU
	Supports Intel® Alder Lake 12th generation LGA 1700 Core i3-12100, i5-12400, i7-12700, i9-12900, etc.
Supports Intel® Raptor Lake 13th generation LGA 1700 Core i3-13100, i5-13400, i7-13400, i9-13900, etc.
Supports Intel® Raptor Lake 14th generation LGA 1700 Core i3-14100, i5-14400, i7-14700, i9-14900, etc.
(See the next page for a complete CPU list)

	
	graphics card
	Intel® UHD Graphics 730/770 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666/2933/3200MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 6A or higher.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60HZ)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60HZ)

	
	LAN
	Single Gigabit Ethernet adapter: Intel WG I219V Gigabit Ethernet adapter;
Dual Gigabit Ethernet adapters: Intel WG I219V + Realtek 8111H Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	2 USB 3.2 Gen1 ports
2 USB 2.0 ports (dual-network PCs do not have this port)

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2
	1 M.2 Key-M slot, supporting M.2 2280 NVME PCIe 3.0 x4 protocol, can be modified to support SATA protocol; optional M.2 2242 hard drive;

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	Mini-PCIe
	1 Mini-PCIE slot, supporting PCIE 3.0 x1 & USB signal, and supporting WiFi, Bluetooth/4G modules;

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Supports Windows 11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
The CPU information below is for reference only. Please consult our sales team for specific requirements!

	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption (W)
	Maximum turbo power consumption (W)

	12th Gen i3
	Intel Core
	1 21 00
	Quad- core 3.3 GHz
	4.3 G
	60
	89

	
	Intel Core
	12300
	Quad- core 3.5 GHz
	4.4 G
	60
	89

	12th Gen i5
	Intel Core
	1 2 400
	Six-core 2.5GHz
	4.4G
	65
	117

	
	
	1 2 500
	Six-core 3.0GHz
	4.6G
	65
	117

	
	
	1 2 600
	Six-core 3.3GHz
	4.8G
	65
	117

	12th Gen i7
	Intel Core
	12700
	12 cores 2.1GHz
	4.9G
	65
	180

	12th Gen i9
	Intel Core
	1 2 900
	Sixteen cores , 2.4 GHz
	5.1 G​
	65
	202

	13th generation i3
	Intel Core
	13100
	Quad-core 3.4GHz
	4.5G
	60
	89

	13th Gen i5
	Intel Core
	13400
	deca-core 2.5GHz
	4.6G
	65
	154

	13th Gen i5
	Intel Core
	13500
	Fourteen cores 2.5G
	4.8G
	65
	154

	13th Gen i5
	Intel Core
	13600
	Fourteen cores 2.7GHz
	5.3G
	65
	154

	13th Gen i7
	Intel Core
	13700
	16 cores 2.1GHz
	5.2G
	65
	219

	13th generation i9
	Intel Core
	13900
	24 cores 2.3GHz
	5.6G
	65
	219

	14th Gen i3
	Intel Core
	14100
	Quad-core 3.5GHz
	4.7G
	60
	154

	14th Gen i5
	Intel Core
	14400
	Deca core 2.5GHz
	4.7G
	65
	219

	14th Gen i5
	Intel Core
	14500
	Fourteen cores 2.6GHz
	5.0G
	65
	219

	14th Gen i5
	Intel Core
	14600
	Fourteen cores, 2.7GHz
	5.2G
	65
	219

	14th Gen i7
	Intel Core
	14700
	Twenty cores 2.1GHz
	5.4G
	65
	219

	14th Gen i9
	Intel Core
	14900
	24 cores 2.0GHz
	5.8G
	65
	219



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz
OptionalDP 4K 60Hz
	1
	4
	4
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	

	PC model
	[bookmark: _Toc21638][bookmark: _Toc6292] IPC200U -QM6300

	PC size
	Dimensions with handle: 428mm(L)*350mm(W)*88mm(H) Dimensions with handle: 480mm(L)*350mm(W)*88mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6300

	motherboard
	CPU
	Supports Intel® Alder Lake 12th generation LGA 1700 Core i3-12100, i5-12400, i7-12700, i9-12900, etc.
Supports Intel® Raptor Lake 13th generation LGA 1700 Core i3-13100, i5-13400, i7-13400, i9-13900, etc.
Supports Intel® Raptor Lake 14th generation LGA 1700 Core i3-14100, i5-14400, i7-14700, i9-14900, etc.
(See the next page for a complete CPU list)

	
	graphics card
	Intel® UHD Graphics 730/770 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	Memory
	2*NB-DDR4 memory modules support 2133/2400/2666/2933/3200MHz, with a maximum capacity of 64GB.

	Front panel interface
	POWER
	1* Switch button

	
	RESET
	1* Restart Switch

	
	led
	1 power indicator, 1 hard drive indicator

	
	USB
	4 USB 2.0 ports

	Rear panel interface
	Power interface
	1 power interface, built-in DC power adapter, supports DC 12V/19V, recommended power supply is 12V 10A or 19V 6A or higher.

	
	Display Interface
	1*HDMI® 2.0 port (4096/3840*2160@60HZ)
1 VGA interface (1920*1080@60Hz)
Optional 1*DP interface (4096/3840*2160@60HZ)

	
	LAN
	Single Gigabit Ethernet adapter: Realtek 8111H Gigabit Ethernet adapter;
Supports Wake-on-LAN and PXE network functionality;

	
	USB
	4 USB 3.2 Gen1 ports

	
	COM
	6 COM ports, supporting RS232 by default; COM1 can optionally support RS232/RS422/RS485.

	
	audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2 WiFi antenna interfaces

	storage
	M.2
	1 M.2 Key-M slot, supporting M.2 2280 NVME PCIe 3.0 x4 / SATA adaptive standard SSD;

	
	SATA
	One SATA 3.0 hard drive interface, supporting 2.5-inch SSDs/HDDs or 3.5-inch HDDs.

	
	Hard drive bays in the chassis
	4 hard drive bays (2 x 2.5-inch SSD/HDD bays, 2 x 3.5-inch HDD bays; this only indicates the number of hard drives the case can accommodate).

	Extend
	M.2 WiFi
	1*M.2 Key-E slot, supports M.2 2230 PCIE3.0 x1 & USB signals, supports WiFi and Bluetooth modules;

	Operating environment
	Operating temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	relative humidity
	5%-95% relative humidity, non-condensing

	
	Working vibration
	0.5grms/5-500HZ/random/operating

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Supports Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
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The CPU information below is for reference only. Please consult our sales team for specific requirements!

	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption (W)
	Maximum turbo power consumption (W)

	12th Gen i3
	Intel Core
	1 21 00
	Quad- core 3.3 GHz
	4.3 G
	60
	89

	
	Intel Core
	12300
	Quad- core 3.5 GHz
	4.4 G
	60
	89

	12th Gen i5
	Intel Core
	1 2 400
	Six-core 2.5GHz
	4.4G
	65
	117

	
	
	1 2 500
	Six-core 3.0GHz
	4.6G
	65
	117

	
	
	1 2 600
	Six-core 3.3GHz
	4.8G
	65
	117

	12th Gen i7
	Intel Core
	12700
	12 cores 2.1GHz
	4.9G
	65
	180

	12th Gen i9
	Intel Core
	1 2 900
	Sixteen cores , 2.4 GHz
	5.1 G​
	65
	202

	13th generation i3
	Intel Core
	13100
	Quad-core 3.4GHz
	4.5G
	60
	89

	13th Gen i5
	Intel Core
	13400
	deca-core 2.5GHz
	4.6G
	65
	154

	13th Gen i5
	Intel Core
	13500
	Fourteen cores 2.5G
	4.8G
	65
	154

	13th Gen i5
	Intel Core
	13600
	Fourteen cores 2.7GHz
	5.3G
	65
	154

	13th Gen i7
	Intel Core
	13700
	16 cores 2.1GHz
	5.2G
	65
	219

	13th generation i9
	Intel Core
	13900
	24 cores 2.3GHz
	5.6G
	65
	219

	14th Gen i3
	Intel Core
	14100
	Quad-core 3.5GHz
	4.7G
	60
	154

	14th Gen i5
	Intel Core
	14400
	Deca core 2.5GHz
	4.7G
	65
	219

	14th Gen i5
	Intel Core
	14500
	Fourteen cores 2.6GHz
	5.0G
	65
	219

	14th Gen i5
	Intel Core
	14600
	Fourteen cores, 2.7GHz
	5.2G
	65
	219

	14th Gen i7
	Intel Core
	14700
	Twenty cores 2.1GHz
	5.4G
	65
	219

	14th Gen i9
	Intel Core
	14900
	24 cores 2.0GHz
	5.8G
	65
	219
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illustrate
Except for the accessories listed that come with the product, the contents of this manual do not represent a commitment by the company, and the company reserves the right to make changes to this manual without prior notice.
We are not responsible for any direct, indirect, intentional or unintentional damage or potential hazards caused by improper installation or use.
Before ordering a product, please consult with the distributor to understand in detail whether the product performance meets your needs.
The contents of this manual are protected by copyright. All rights reserved. No part of this manual may be reproduced in any mechanical, electronic or other manner without permission.
The final interpretation right of this instruction manual belongs to SHENZHEN ELSKY TECHNOLOGY CO.,LTD.

The above ordering information is for reference only. Please contact our sales department for details. Tel: 0755-82260150
Motherboard driver download: https://pan.baidu.com/s/1ie7qi5NutS53ipPecRSYtw
Access password: cbn5
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