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ELSKY IPC400U Industrial Computer Specifications
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
PC size diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear DVI interface diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Diagram of connecting the PC to the graphics card
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface diagram with network port in the middle and small audio port.
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface side view of network port + large audio port diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Front Interface Diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
PC size diagram
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
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―――――――――――――――――――――――――――――――――――――――――――――――――――――――
The pictures are for reference only. Please refer to the actual product.
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	7
	1
	/
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc4802][bookmark: _Toc20966]IPC400U-J1900 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes, fanless or silent fan cooling

	Color
	black

	Compatible motherboard models
	M218F, M219F, M218H, M219H, M284F, M284FC, M284FN, M294F, M294FC, M294FN, M284H, M294H, QM1800E, QM1800L, QM1900E, QM1900L

	Power supply
	ATX power supply
	Supports 12V, a power supply of 200W or higher is recommended.

	CPU
	Intel Celeron J1800 Dual-Core 2.41GHz, Turbo Boost 2.58GHz;
Intel Celeron J1900 Quad-core 1.99GHz, Turbo Boost 2.4GHz;
Intel Pentium J2900 Quad-core 2.41GHz, Turbo Boost 2.66GHz;
Intel Celeron N2840 dual-core 2.16GHz, turbo boost 2.58GHz;
Intel Celeron N2930 Quad-core 1.83GHz, Turbo Boost 2.16GHz;
Intel Celeron N2940 Quad-core 1.83GHz, Turbo Boost 2.25GHz;

	Chipset
	Intel Bay Trail SOC

	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	USB function
	1 USB 3.0 port
	The blue group of USB ports is for USB 3.0 (the blue group, the ones on the bottom of the case are USB 3.0).

	
	7 USB 2.0 ports
	The black group of USB ports is USB 2.0 (the blue group, the ones on the top of the case, are USB 2.0).

	Sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	6*COM interface
	Supports RS232 (RS485 support can be customized).

	
	M218FN/M219FN/M284FN/M294FN have no COM port; M218FC/M219FC/M284FC/M294FC support 1 COM port; QM1800E/QM1800L/QM1900E/QM1900L support 2 COM ports.
M218F/M219F/M219H/218H/M284H/M294H/M284F/M294F supports 6*COM;

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	Operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc3015][bookmark: _Toc31022]IPC400U-M316F series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes, fanless or silent fan cooling

	color
	black

	Compatible motherboard models
	M316F

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Intel Celeron N3150 Quad-core 1.6GHz, Turbo Boost 2.08GHz;
Intel Celeron N3160 Quad-core 1.6GHz, Turbo Boost 2.24GHz;
Intel Celeron N3700 Quad-core 1.6GHz, Turbo Boost 2.40GHz;

	Chipset
	Intel Bay Trail SOC

	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Network function
	1 RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet NIC
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662 HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2
	1*M.2
1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc11506][bookmark: _Toc26381][bookmark: _Toc17677]IPC400U-J3355 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes, fanless or silent fan cooling

	color
	black

	Compatible motherboard models
	M335F

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	Intel Celeron J3355, dual-core 2.0GHz, turbo boost 2.5GHz;
Intel Celeron J3455 Quad-core 1.5GHz, Turbo Boost 2.3GHz;
Intel Pentium N4200 Quad-core 1.1GHz, Turbo Boost 2.5GHz;

	Chipset
	Intel Apollo Lake SOC

	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1600MHz memory, maximum support 8GB

	Network function
	1 RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet controller; supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 500/505 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller
Or integrate Shunxin ES8336 audio chip

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
1*MSATA drive;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR4
MAX 16G
	200W
The above power supply
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	PC model
	[bookmark: _Toc16485][bookmark: _Toc25137][bookmark: _Toc9922]IPC400U-J4125 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes, fanless or silent fan cooling

	color
	black

	Compatible motherboard models
	M415F

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	Intel Celeron J4025 dual-core 2.0GHz, turbo boost 2.9GHz;
Intel Celeron J4125 Quad-core 2.0GHz, Turbo Boost 2.7GHz;
Intel Celeron N4020 dual-core 1.1GHz, turbo boost up to 2.8GHz;
Intel Celeron N4120 Quad-core 1.1GHz, Turbo Boost 2.6GHz;
Intel Pentium N5030 Quad-core 1.1GHz, Turbo Boost 3.1GHz;
Intel Pentium J5040 Quad-core 2.0GHz, Turbo Boost 3.2GHz;

	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 2400MHz memory, maximum support 16GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	The Intel HD Graphics 600 graphics controller supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 2.0 port
	Supports 4K resolution 4096/3840*2160@60Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.1
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
	1*NB-DDR4
MAX 32G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc9295][bookmark: _Toc1067][bookmark: _Toc23632]IPC400U-J6412 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes, fanless or silent fan cooling

	color
	black

	Compatible motherboard models
	M612F

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Intel Celeron J6412 Quad-core 2.0GHz, Turbo Boost 2.6GHz;
Intel Celeron J6413 Quad-core 1.8GHz, Turbo Boost 3.0GHz;
Intel Celeron N6210 dual-core 1.2GHz, turbo boost 2.6GHz;
Intel Celeron N6211 dual-core 1.2GHz, turbo boost 3.0GHz;
Intel Pentium J6426 Quad-core 2.0GHz, Turbo Boost 3.0GHz;
Intel Pentium N6415 Quad-core 1.2GHz, Turbo Boost 3.0GHz;

	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 3200MHz memory, maximum support 32GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel UHD Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 2.0 port
	Supports 4K resolution 4096/3840*2160@60Hz

	USB function
	2 USB 3.1 ports
	The blue group of USB ports is USB 3.1 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc5226][bookmark: _Toc11476][bookmark: _Toc26121]IPC400U-1037 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	1007F, 1037F, 2117F

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Intel Celeron 1007U Dual-Core 1.5GHz;
Intel Celeron 1037U Dual-Core 1.8GHz;
Intel Pentium 2117U Dual-Core 1.8GHz;

	Chipset
	Intel 6 series chipsets: HM65, HM67, QM67
Intel 7 series chipsets: NM70, HM70, HM75, HM76, HM77, QM77

	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 4000 graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232; COM2 can optionally support RS485/RS422, which can be configured via BIOS.

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Windows XP, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1*2.5 inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc26490][bookmark: _Toc19423][bookmark: _Toc24714]IPC400U-2nd Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6600, QM6637, QM6616, QM2360

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	Second-generation CPU
	Intel Core i3-2310M Dual-core 2.1GHz; Intel Core i3-2330M Dual-core 2.2GHz;
Intel Core i3-2350M Dual-core 2.3GHz; Intel Core i3-2370M Dual-core 2.4GHz;
Intel Core i5-2410M dual-core 2.3GHz, turbo boost 2.9GHz; Core i5-2430M dual-core 2.4GHz, turbo boost 3.0GHz;
Intel Core i5-2520M dual-core 2.5GHz, turbo boost 3.2GHz; Core i5-2540M dual-core 2.6GHz, turbo boost 3.3GHz;
Intel Core i7-2620M dual-core 2.7GHz, turbo boost 3.4GHz; Core i7-2640M dual-core 2.8GHz, turbo boost 3.5GHz;

	Chipset
	Intel 6 series chipsets: HM65, HM67, QM67
Intel 7 series chipsets: NM70, HM70, HM75, HM76, HM77, QM77

	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 3000 graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Windows XP, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	2K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc20635][bookmark: _Toc24413][bookmark: _Toc27176]IPC400U-3rd Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	i3HGP, i5HGP, i7HGP, QM6600, QM6637, QM6616, QM2360

	power supply
	ATX power supply
	The DC connector has an inner diameter of 2.5mm and supports 12V.
For the U series, a 12V 5A or higher power supply is recommended; for the M series, a 12V 7A or higher power supply is recommended.

	Third generation CPU
	Intel Celeron 1037U Dual-Core 1.8GHz; Intel Pentium 2117U Dual-Core 1.8GHz;
Intel Core i3-3217U Dual-core 1.8GHz; Intel Core i3-3227U Dual-core 1.9GHz;
Intel Core i5-3317U dual-core 1.7GHz, turbo boost 2.6GHz; Intel Core i5-3337U dual-core 1.8GHz, turbo boost 2.7GHz; Intel Core i5-3427U dual-core 1.8GHz, turbo boost 2.8GHz; Intel Core i5-3437U dual-core 1.9GHz, turbo boost 2.9GHz;
Intel Core i7-3517U dual-core 1.9GHz, turbo boost 3.0GHz; Intel Core i7-3537U dual-core 2.0GHz, turbo boost 3.1GHz; Intel Core i7-3667U dual-core 2.0GHz, turbo boost 3.2GHz; Intel Core i7-3687U dual-core 2.1GHz, turbo boost 3.3GHz;
Intel Core i3-31 10M dual-core 2.4GHz; Intel Core i3-312 0M dual-core 2.5GHz;
Intel Core i5-3210M dual-core 2.5GHz, turbo boost 3.1GHz; Core i5-3230M dual-core 2.6GHz, turbo boost 3.2GHz;
Intel Core i5-3320M dual-core 2.6GHz, turbo boost 3.3GHz; Core i5-3340M dual-core 2.7GHz, turbo boost 3.4GHz;
Intel Core i5-3360M dual-core 2.8GHz, turbo boost 3.5GHz; Core i5-3380M dual-core 2.9GHz, turbo boost 3.6GHz;
Intel Core i7-3520M dual-core 2.9GHz, turbo boost 3.6GHz; Core i7-3540M dual-core 3.0GHz, turbo boost 3.7GHz;

	Chipset
	Intel 6 series chipsets: HM65, HM67, QM67
Intel 7 series chipsets: NM70, HM70, HM75, HM76, HM77, QM77

	Memory
	1*NB-DDR3 memory, supports 1.35V/1.5V, supports 1333/1600MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 4000 graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Windows XP, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc31071][bookmark: _Toc15084][bookmark: _Toc22017]IPC400U-4th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9400, QM9400H, QM9400L, QM9400E, QM9450, QM9360

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	





Fourth generation CPU
	Intel Core i3-4005U Dual-core 1.7GHz; Core i3-4010U Dual-core 1.7GHz;
Intel Core i3-4025U Dual-core 1.9GHz; Core i3-4030U Dual-core 1.9GHz;
Intel Core i3-4100U Dual-Core 1.8GHz;
Intel Core i5-4200U dual-core 1.6GHz, turbo boost 2.6GHz; Core i5-4210U dual-core 1.7GHz, turbo boost 2.7GHz;
Intel Core i5-4250U dual-core 1.3GHz, turbo boost 2.6GHz; Core i5-4278U dual-core 2.6GHz, turbo boost 3.1GHz;
Intel Core i5-4300U dual-core 1.9GHz, turbo boost 2.9GHz; Core i5-4308U dual-core 2.8GHz, turbo boost 3.3GHz;
Intel Core i5-4310U dual-core 2.0GHz, turbo boost 3.0GHz; Core i7-4500U dual-core 1.8GHz, turbo boost 3.0GHz;
Intel Core i7-4510U dual-core 2.0GHz, turbo boost 3.1GHz; Core i7-4550U dual-core 1.5GHz, turbo boost 3.0GHz;
Intel Core i7-4558U dual-core 2.8GHz, turbo boost 3.3GHz; Core i7-4578U dual-core 3.0GHz, turbo boost 3.5GHz;
Intel Core i7-4600U dual-core 2.1GHz, turbo boost 3.3GHz; Core i7-4650U dual-core 1.7GHz, turbo boost 3.0GHz;

	Chipset
	Haswell-U

	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1333/1600MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H/8111F Gigabit Ethernet adapter or Realtek 810 6E /8105E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	M series: Intel HD Graphics 4600 graphics controller, supporting single display, dual display duplication, and dual display expansion.
U-series: Intel HD Graphics 4400 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1*2.5 inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply
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	PC model
	[bookmark: _Toc16691][bookmark: _Toc23368][bookmark: _Toc8047]IPC400U-5th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9500, QM9500H, QM9500L, QM9500E, QM9550, QM9360

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	


Fifth generation CPU
	Intel Core i3-5005U Dual-core 2.0GHz; Core i3-5010U Dual-core 2.1GHz;
Intel Core i3-5015U dual-core 2.1GHz; Core i3-5020U dual-core 2.2GHz;
Intel Core i5-5200U dual-core 2.2GHz, turbo boost 2.7GHz; Core i5-5250U dual-core 1.6GHz, turbo boost 2.7GHz;
Intel Core i5-5257U dual-core 2.7GHz, turbo boost 3.1GHz; Core i5-5287U dual-core 2.9GHz, turbo boost 3.3GHz;
Intel Core i5-5300U dual-core 2.3GHz, turbo boost 2.9GHz; Core i5-5350U dual-core 1.8GHz, turbo boost 2.9GHz;
Intel Core i7-5500U dual-core 2.4GHz, turbo boost 3.0GHz; Core i7-5550U dual-core 2.0GHz, turbo boost 3.0GHz;
Intel Core i7-5557U dual-core 3.1GHz, turbo boost 3.4GHz; Core i7-5600U dual-core 2.6GHz, turbo boost 3.2GHz;
Intel Core i7-5650U dual-core 2.2GHz, turbo boost 3.1GHz;

	Chipset
	Broadwell-U

	Memory
	1*NB-DDR3 memory, supports 1.35V, supports 1333/1600MHz memory, maximum support 8GB

	Network function
	1 RJ45 LAN interface

	Integrated Realtek 8111H/8111F Gigabit Ethernet adapter or Realtek 810 6E /8105E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	The Intel HD Graphics 5500 graphics controller supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	2*NB-DDR3
MAX 16G
	200W
The above power supply
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	PC model
	[bookmark: _Toc14578][bookmark: _Toc23615][bookmark: _Toc11016]IPC400U-6th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9600, QM9600H

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	


6th generation CPU
	Intel Celeron 3855U Dual-Core 1.6GHz; Celeron 3955U Dual-Core 2.0GHz;
Intel Core i3-6006U Dual-core 2.0GHz; Core i3-6100U Dual-core 2.3GHz;
Intel Core i3-6157U Dual-core 2.4GHz; Core i3-6167U Dual-core 2.7GHz;
Intel Core i5-6200U dual-core 2.3GHz, turbo boost 2.8GHz; Core i5-6300U dual-core 2.4GHz, turbo boost 3.0GHz;
Intel Core i5-6260U dual-core 1.8GHz, turbo boost 2.9GHz; Core i5-6267U dual-core 2.9GHz, turbo boost 3.3GHz;
Intel Core i5-6287U dual-core 3.1GHz, turbo boost 3.5GHz; Core i5-6360U dual-core 2.0GHz, turbo boost 3.1GHz;
Intel Core i7-6500U dual-core 2.5GHz, turbo boost 3.1GHz; Core i7-6600U dual-core 2.6GHz, turbo boost 3.4GHz;
Intel Core i7-6560U dual-core 2.2GHz, turbo boost 3.2GHz; Core i7-6567U dual-core 3.3GHz, turbo boost 3.6GHz;
Intel Core i7-6650U dual-core 2.2GHz, turbo boost 3.4GHz; Core i7-6660U dual-core 2.4GHz, turbo boost 3.4GHz;

	Chipset
	Skylake

	Memory
	2*NB-DDR3 memory modules, supporting 1.35V, 1333/1600MHz memory, maximum support 16GB.

	Network function
	1 RJ45 LAN interface

	Integrated Realtek 8111H/8111F Gigabit Ethernet adapter or Realtek 810 6E /8105E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 510/520 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	2*NB-DDR4
MAX 32G
	200W
The above power supply
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	PC model
	[bookmark: _Toc17138][bookmark: _Toc2944][bookmark: _Toc31411]IPC400U-QM9650

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9650

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	


6th generation CPU
	Intel Celeron 3855U Dual-Core 1.6GHz; Celeron 3955U Dual-Core 2.0GHz;
Intel Core i3-6006U Dual-core 2.0GHz; Core i3-6100U Dual-core 2.3GHz;
Intel Core i3-6157U Dual-core 2.4GHz; Core i3-6167U Dual-core 2.7GHz;
Intel Core i5-6200U dual-core 2.3GHz, turbo boost 2.8GHz; Core i5-6300U dual-core 2.4GHz, turbo boost 3.0GHz;
Intel Core i5-6260U dual-core 1.8GHz, turbo boost 2.9GHz; Core i5-6267U dual-core 2.9GHz, turbo boost 3.3GHz;
Intel Core i5-6287U dual-core 3.1GHz, turbo boost 3.5GHz; Core i5-6360U dual-core 2.0GHz, turbo boost 3.1GHz;
Intel Core i7-6500U dual-core 2.5GHz, turbo boost 3.1GHz; Core i7-6600U dual-core 2.6GHz, turbo boost 3.4GHz;
Intel Core i7-6560U dual-core 2.2GHz, turbo boost 3.2GHz; Core i7-6567U dual-core 3.3GHz, turbo boost 3.6GHz;
Intel Core i7-6650U dual-core 2.2GHz, turbo boost 3.4GHz; Core i7-6660U dual-core 2.4GHz, turbo boost 3.4GHz;

	Chipset
	Skylake

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400MHz memory, maximum support 32GB

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 510/520 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2; 1*2.5-inch SSD or HDD (1*MSATA optional)

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10,Windows 8,Windows 7,Linux etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*MSATA
1*2.5 inch SSD/HDD
	2*NB-DDR3
MAX 16G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc5218][bookmark: _Toc15103][bookmark: _Toc14728]IPC400U-7th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9700, QM9700H

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	


7th generation CPU
	Intel Celeron 3865U Dual-Core 1.8GHz; Celeron 3965U Dual-Core 2.2GHz;
Intel Core i3-7020U Dual-core 2.3GHz; Core i3-7100U Dual-core 2.4GHz;
Intel Core i3-7130U dual-core 2.7GHz;
Intel Core i5-7200U dual-core 2.5GHz, turbo boost 3.1GHz; Core i5-7260U dual-core 2.2GHz, turbo boost 3.4GHz;
Intel Core i5-7267U dual-core 3.1GHz, turbo boost 3.5GHz; Core i5-7287U dual-core 3.3GHz, turbo boost 3.7GHz;
Intel Core i5-7300U dual-core 2.6GHz, turbo boost 3.5GHz; Core i5-7360U dual-core 2.3GHz, turbo boost 3.6GHz;
Intel Core i7-7500U dual-core 2.7GHz, turbo boost 3.5GHz; Core i7-7560U dual-core 2.4GHz, turbo boost 3.8GHz;
Intel Core i7-7567U dual-core 3.5GHz, turbo boost 4.0GHz; Core i7-7660U dual-core 2.5GHz, turbo boost 4.0GHz;
Intel Core i7-7600U dual-core 2.8GHz, turbo boost up to 3.9GHz;

	Chipset
	Kabylake

	Memory
	2*NB-DDR3 memory modules, supporting 1.35V, 1333/1600MHz memory, maximum support 16GB.

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H/8111F Gigabit Ethernet adapter or Realtek 810 6E /8105E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 610/620 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller.

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1 x mSATA drive; 1 x 2.5-inch SSD or HDD hard drive

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	2*NB-DDR4
MAX 32G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc28305][bookmark: _Toc3955][bookmark: _Toc10193]IPC400U-QM9750

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9750

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	


7th generation CPU
	Intel Celeron 3865U Dual-Core 1.8GHz; Celeron 3965U Dual-Core 2.2GHz;
Intel Core i3-7020U dual-core 2.3GHz; Core i3-7100U dual-core 2.4GHz;
Intel Core i3-7130U dual-core 2.7GHz;
Intel Core i5-7200U dual-core 2.5GHz, turbo boost 3.1GHz; Core i5-7260U dual-core 2.2GHz, turbo boost 3.4GHz;
Intel Core i5-7267U dual-core 3.1GHz, turbo boost 3.5GHz; Core i5-7287U dual-core 3.3GHz, turbo boost 3.7GHz;
Intel Core i5-7300U dual-core 2.6GHz, turbo boost 3.5GHz; Core i5-7360U dual-core 2.3GHz, turbo boost 3.6GHz;
Intel Core i7-7500U dual-core 2.7GHz, turbo boost 3.5GHz; Core i7-7560U dual-core 2.4GHz, turbo boost 3.8GHz;
Intel Core i7-7567U dual-core 3.5GHz, turbo boost 4.0GHz; Core i7-7660U dual-core 2.5GHz, turbo boost 4.0GHz;
Intel Core i7-7600U dual-core 2.8GHz, turbo boost up to 3.9GHz;

	Chipset
	Kabylake

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400MHz memory, maximum support 32GB

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet adapter or Realtek 810 6E 100Mbps Ethernet adapter optional.
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel HD Graphics 610/620 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2; (Optional 1*MSATA)
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; 
Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	5
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc26230][bookmark: _Toc5670][bookmark: _Toc14946]IPC400U - 8th and 10th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM9850, QM8U, QM10U, QM8H, QM9H, QM10H

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	




8th generation CPU
	QM9850: Kaby Lake R: Intel Core i3-8130U dual-core 2.2GHz, turbo boost 3.4GHz;
Intel Core i5-8250U quad-core 1.6GHz, turbo boost 3.4GHz; Core i5-8350U quad-core 1.7GHz, turbo boost 3.6GHz;
Intel Core i7-8550U quad-core 1.8GHz, turbo boost 4.0GHz; Core i7-8650U quad-core 1.9GHz, turbo boost 4.2GHz;
QM8U/QM8H: Whiskey Lake: Intel Core i3-8145U dual-core 2.1GHz, turbo boost 3.9GHz;
Intel Core i5-8265U quad-core 1.6GHz, turbo boost 3.9GHz; Core i5-8365U quad-core 1.6GHz, turbo boost 4.1GHz;
Intel Core i7-8565U quad-core 1.8GHz, turbo boost 4.6GHz; Core i7-8665U quad-core 1.9GHz, turbo boost 4.8GHz;
QM9H: Coffee Lake
Intel Core i3-8109U dual-core 3.0GHz, turbo boost 3.6GHz; Core i3-8140U dual-core 2.1GHz, turbo boost 3.9GHz;
Intel Core i5-8259U quad-core 2.3GHz, turbo boost 3.8GHz; Core i5-8269U quad-core 2.6GHz, turbo boost 4.2GHz;
Intel Core i5-8279U quad-core 2.4GHz, turbo boost 4.1GHz; Core i5-8257U quad-core 1.4GHz, turbo boost 3.9GHz;
Intel Core i5-8260U quad-core 1.6GHz, turbo boost 3.9GHz; Core i7-8559U quad-core 2.7GHz, turbo boost 4.5GHz;
Intel Core i7-8569U quad-core 2.8GHz, turbo boost 4.7GHz; Core i7-8557U quad-core 1.7GHz, turbo boost 4.5GHz;

	
10th generation CPU
	Comet Lake: Intel Core i3-10110U dual-core 2.1GHz, turbo boost 4.1GHz;
Intel Core i5-10210U quad-core 1.6GHz, turbo boost 4.2GHz; Core i5-10310U quad-core 1.7GHz, turbo boost 4.4GHz;
Intel Core i7-10510U quad-core 1.8GHz, turbo boost 4.9GHz; Core i7-10610U quad-core 1.8GHz, turbo boost 4.9GHz;
Intel Core i7-10710U: 6 cores, 1.1GHz, turbo boost up to 4.7GHz; Core i7-10810U: 6 cores, 1.1GHz, turbo boost up to 4.9GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666MHz memory, maximum support 64GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H/8111G Gigabit Ethernet controller; supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, and supports 2*WIFI antenna masts (optional support for M.2-5G).

	Display function


	Intel HD Graphics 610/620 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller
Alternatively, it can integrate the Cmedia HS_100B USB audio chip; (BBH621 USB sound card is optional)

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2; (Optional 1*MSATA)
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	5
	2
	2
	1*M.2
1*MSATA
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc31902][bookmark: _Toc26229]IPC400U-QM8900 series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM8900, QM8900H

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	8th generation CPU
	Intel Core i3-8100H Quad-core 3.0GHz;
Intel Core i5-8300H quad-core 2.3GHz, turbo boost 4.0GHz; Core i5-8400H quad-core 2.5GHz, turbo boost 4.2GHz;
Intel Core i7-8750H: Six-core, 2.2GHz, turbo boost up to 4.1GHz; Core i7-8850H: Six-core, 2.6GHz, turbo boost up to 4.3GHz;
Intel Core i9-8950HK: Six-core, 2.9GHz, turbo boost up to 4.6GHz;

	9th generation CPU
	Intel Core i5-9300H quad-core 2.4GHz, turbo boost 4.1GHz; Core i5-9400H quad-core 2.5GHz, turbo boost 4.3GHz;
Intel Core i7-9750H: Six-core, 2.6GHz, turbo boost up to 4.5GHz; Core i7-9850H: Six-core, 2.6GHz, turbo boost up to 4.6GHz;
Intel Core i9-9880H: Eight-core, 2.3GHz, turbo boost up to 4.8GHz; Core i9-9980HK: Eight-core, 2.4GHz, turbo boost up to 5.0GHz;

	
10th generation CPU
	QM8900H: Intel Core i5-10200H quad-core 2.4GHz, turbo boost up to 4.1GHz;
Intel Core i5-10300H: Quad-core 2.5GHz, turbo boost 4.5GHz; Core i5-10500H: Hexa-core 2.5GHz, turbo boost 4.5GHz;
Intel Core i7-10750H: 6 cores, 2.6GHz, turbo boost up to 5.0GHz; Core i7-10870H: 8 cores, 2.2GHz, turbo boost up to 5.0GHz;
Intel Core i9-10980HK, eight cores, 2.4GHz, turbo boost up to 5.3GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666MHz memory, maximum support 64GB

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet controller; supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, and supports 2*WIFI antenna masts (optional support for M.2-5G).

	Display function


	Intel HD Graphics 630 graphics controller, supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	5 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS_100B USB audio chip

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2; 1*MSATA
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	6*COM interface
	Supports RS232 ( RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	200W
The above power supply
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	PC model
	[bookmark: _Toc19725][bookmark: _Toc714][bookmark: _Toc13044]IPC400U-11th Generation Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM11U

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	

11th generation CPU
	Intel Core i3-1115G4E dual-core 2.2GHz, turbo boost 3.9GHz; Core i3-1115GRE dual-core 2.2GHz, turbo boost 3.9GHz;
Intel Core i3-1115G4 dual-core 3.0GHz, turbo boost 4.1GHz; Core i3-1125G4 quad-core 2.0GHz, turbo boost 3.7GHz;
Intel Core i5-1145G7E Quad-core 1.5GHz, Turbo Boost 4.1GHz; Core i5-1145GRE Quad-core 1.5GHz, Turbo Boost 4.1GHz;
Intel Core i5-1145G7 Quad-core 2.6GHz, Turbo Boost 4.4GHz; Core i5-1135G7 Quad-core 2.4GHz, Turbo Boost 4.2GHz;
Intel Core i5-1155G7 Quad-core 2.5GHz, Turbo Boost 4.5GHz; Core i7-1185GRE Quad-core 1.8GHz, Turbo Boost 4.4GHz;
Intel Core i5-1185G7E Quad-core 1.8GHz, Turbo Boost 4.4GHz; Core i5-1185G7 Quad-core 3.0GHz, Turbo Boost 4.8GHz;
Intel Core i5-1165G7 Quad-core 2.8GHz, Turbo Boost 4.7GHz; Core i5-1195G7 Quad-core 2.9GHz, Turbo Boost 5.0GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666/3200MHz memory, maximum support 64GB

	Network function
	1*RJ45 LAN interface

	Single-network Intel WG I219V Gigabit Ethernet controller; Dual-network Intel WG I219V + Realtek 8111H Gigabit Ethernet controller
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Intel UHD/Iris Xe Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 2.0 port
	Supports 4K resolution 4096/3840*2160@60Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller;
Alternatively, it can integrate a Cmedia HS_100B USB audio chip;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2; (Optional 1*MSATA)
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 (2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply
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	PC model
	[bookmark: _Toc21141][bookmark: _Toc15802][bookmark: _Toc5773]IPC400U-12th and 13th generation series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM12U, QM13U, QM12P, QM13P, QM12H, QM13H

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Supports Intel Alder Lake 12th generation U, P, H series i3, i5, i7, i9
Supports Intel Raptor Lake 13th generation U, P, and H series i3, i5, i7, and i9 processors.
(See the next page for a complete CPU list)

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666/2933/3200MHz memory, maximum support 64GB

	Network function
	1*RJ45 LAN interface

	Single-network Intel I219V Gigabit Ethernet adapter; Dual-network Intel I219V + Realtek 8111H Gigabit Ethernet adapter
Supports network power on/off and network PXE functionality.

	
	Supports M.2 Wi-Fi/Bluetooth optional, supports M.2-5G, optional M.2-4G, supports 2*Wi-Fi antenna mounts

	Display function


	Intel UHD/Iris Xe Graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 2.0 port
	Supports 4K resolution 4096/3840*2160@60Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

List of 12th and 13th generation CPUs
	Motherboard Model
	CPU Specifications
	CPU Brand
	CPU model
	kernel/thread
	clock speed
	Turbo Boost

	QM12U
	12th Gen i3
	Core
	1215U
	Six cores and eight threads
	1.2G
	4.4G

	
	
	
	1210U
	Six cores and eight threads
	1.0G
	4.4G

	
	12th Gen i5
	Core
	1235U
	Ten cores and twelve threads
	1.3G
	4.4G

	
	
	
	1240U
	Ten cores and twelve threads
	1.1G
	4.4G

	
	
	
	1230U
	Ten cores and twelve threads
	1.0G
	4.4G

	
	
	
	1245U
	Ten cores and twelve threads
	1.6G
	4.4G

	
	12th Gen i7
	Core
	1250U
	Ten cores and twelve threads
	1.1G
	4.7G

	
	
	
	1260U
	Twelve cores and sixteen threads
	1.1G
	4.7G

	
	
	
	1265U
	Ten cores and twelve threads
	1.8G
	4.8G

	
	
	
	1255U
	Ten cores and twelve threads
	1.7G
	4.7G

	QM13U
	13th Gen i3
	Core
	1305U
	Five cores and six threads
	1.6G
	4.5G

	
	
	
	1315U
	Six cores and eight threads
	1.2G
	4.5G

	
	13th Gen i5
	Core
	1334U
	Ten cores and twelve threads
	1.3G
	4.6G

	
	
	
	1335U
	Ten cores and twelve threads
	1.3G
	4.6G

	
	
	
	1345U
	Ten cores and twelve threads
	1.6G
	4.7G

	
	13th Gen i7
	Core
	1355U
	Ten cores and twelve threads
	1.7G
	5.0G

	
	
	
	1365U
	Ten cores and twelve threads
	1.8G
	5.2G

	QM12P
	12th Gen i3
	Core
	1220P
	Ten cores and twelve threads
	1.5G
	4.4G

	
	12th Gen i5
	Core
	1240P
	Twelve cores and sixteen threads
	1.7G
	4.4G

	
	
	
	1250P
	Twelve cores and sixteen threads
	1.7G
	4.4G

	
	12th Gen i7
	Core
	1280P
	Fourteen cores and twenty threads
	1.8G
	4.8G

	
	
	
	1260P
	Twelve cores and sixteen threads
	2.1G
	4.7G

	
	
	
	1270P
	Twelve cores and sixteen threads
	2.2G
	4.8G

	QM13P
	13th Gen i5
	Core
	1340P
	Twelve cores and sixteen threads
	1.8G
	4.6G

	
	
	
	1350P
	Twelve cores and sixteen threads
	1.9G
	4.7G

	
	13th Gen i7
	Core
	1360P
	Twelve cores and sixteen threads
	2.2G
	5.0G

	
	
	
	1370P
	Fourteen cores and twenty threads
	1.9G
	5.2G

	QM12H
	12th Gen i5
	Core
	12450H
	Eight cores and twelve threads
	1.5G
	4.4G

	
	
	
	12500H
	Twelve cores and sixteen threads
	1.8G
	4.5G

	
	12th Gen i7
	Core
	12800H
	Fourteen cores and twenty threads
	1.8G
	4.8G

	
	
	
	12700H
	Fourteen cores and twenty threads
	1.7G
	4.7G

	
	
	
	12650H
	Ten cores and sixteen threads
	1.7G
	4.7G

	
	
	
	12600H
	Twelve cores and sixteen threads
	2.0G
	4.5G

	
	12th Gen i9
	Core
	12900H
	Fourteen cores and twenty threads
	1.8G
	5.0G

	QM13H
	13th Gen i5
	Core
	13420H
	Eight cores and twelve threads
	2.1G
	4.60G

	
	
	
	13500H
	Twelve cores and sixteen threads
	2.6G
	4.70G

	
	
	
	13505H
	Twelve cores and sixteen threads
	2.6G
	4.70G

	
	
	
	13600H
	Twelve cores and sixteen threads
	2.8G
	4.80G

	
	13th Gen i7
	Core
	13620H
	Ten cores and sixteen threads
	2.4G
	4.90G

	
	
	
	13700H
	Fourteen cores and twenty threads
	2.4G
	5.00G

	
	
	
	13705H
	Fourteen cores and twenty threads
	2.4G
	5.00G

	
	
	
	13800H
	Fourteen cores and twenty threads
	2.5G
	5.20G

	
	13th generation i9
	Core
	13900H
	Fourteen cores and twenty threads
	2.6G
	5.40G







※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc13746][bookmark: _Toc18756][bookmark: _Toc435]IPC400U-Zhaoxin KC6000

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	KC6000

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	Supports the entire series of domestic Zhaoxin KX6000 16NM surface-mount CPUs.
KX 6640MA Quad-core 2.2GHz, Turbo Boost 2.6GHz;
KX 6640A Quad-core 2.6GHz
KX U6580 Octa-core 2.5GHz
KX U6780A Octa-core 2.7GHz
KX U6780 Octa-core 2.7GHz

	Memory
	2*NB-DDR4 memory slots, supporting 2133/2400/2666 MHz memory, maximum support 64 GB.

	Network function
	1*RJ45 LAN interface

	Integrated Realtek 8111H Gigabit Ethernet NIC
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Integrated ZX C960 DX11 super graphics card, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.0 ports
	The blue group of USB ports is USB 3.0.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated CJC6811A high-fidelity USB audio chip;
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Kylin OS, UnionTech OS, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA
2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD with 1 x MSATA option
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	GPU X100 4G video memory
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc27365][bookmark: _Toc24576][bookmark: _Toc32115]IPC400U-Feiteng ET2000

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	ET2000

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Supports domestic Phytium Tengrui D2000 octa-core 2.3GHz processor.

	Memory
	2*NB-DDR4 memory slots, supporting 2133/2400/2666 MHz memory, maximum support 64 GB.

	Network function
	1*RJ45 LAN interface
	Integrated Realtek 8111H Gigabit Ethernet Adapter or YT8521SC/YT6801
Supports network power on/off and network PXE functionality.

	
	Supports optional WIFI/4G/Bluetooth, supports 2*WIFI antenna masts

	Display function


	Integrated X100 super graphics card with 4GB of video memory, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
1 x 2.5-inch SSD or HDD
Optional support for 1*MSATA

	On/off function
	POWER button
	switch button

	Other I/O
	6*COM interface
	Supports RS232

	Operating environment
	Operating temperature: 0℃~60℃; Operating humidity: 5%~95% relative humidity, non-condensing.
Storage temperature: 0℃~70℃;

	BIOS
	Supports power-on upon startup, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Kylin OS, UnionTech OS, Linux, etc. (must support X100 version)


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	1*NB-DDR3
MAX 8G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc5523][bookmark: _Toc6629]IPC400U-4th Generation Independent CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM8680, QM8680L

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Intel PGA946 socket 4th generation M series laptop dedicated CPU
Intel Core i3-4000M Dual-core 2.4GHz; Core i3-4100M Dual-core 2.5GHz;
Intel Core i3-4110M Dual-core 2.6GHz;
Intel Core i5-4200M dual-core 2.5GHz, turbo boost 3.1GHz; Core i5-4210M dual-core 2.6GHz, turbo boost 3.2GHz;
Intel Core i5-4300M dual-core 2.6GHz, turbo boost 3.3GHz; Core i5-4310M dual-core 2.7GHz, turbo boost 3.4GHz;
Intel Core i5-4330M dual-core 2.8GHz, turbo boost 3.5GHz; Core i5-4340M dual-core 2.9GHz, turbo boost 3.6GHz;
Intel Core i7-4600M dual-core 2.9GHz, turbo boost 3.6GHz; Core i7-4610M dual-core 3.0GHz, turbo boost 3.7GHz;

	Memory
	1*NB-DDR3 memory, supports 1.2V, supports 2133/2400/2666/2933/3200MHz memory, maximum support 8GB

	Network function
	1*RJ45 LAN interface

	Integrated with Realtek 8111H Gigabit Ethernet Adapter or Realtek 8106E 100Mbps Ethernet Adapter
Supports network power on/off and network PXE functionality.

	
	Supports optional Wi-Fi/Bluetooth, supports 2*Wi-Fi antenna masts

	Display function


	The Intel HD Graphics 4600 graphics controller supports single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS-100B high-fidelity USB audio chip;
Alternatively, it can integrate a Realtek ALC 662/897 HD digital audio decoder and a 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	3
	4
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	1*NB-DDR4
MAX 16G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc28715][bookmark: _Toc13174]IPC400U-6th/7th Generation Dedicated CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM1100C, QM1100, QM3600

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	1151-pin 6th generation CPU for standalone desktop PCs:
Intel Core i3-6100 Dual-Core 3.7GHz; Core i3-6300 Dual-Core 3.8GHz;
Intel Core i3-6320 dual-core 3.9GHz;
Intel Core i5-6400 Quad-core 2.7GHz, Turbo Boost 3.3GHz; Core i5-6500 Quad-core 3.2GHz, Turbo Boost 3.6GHz;
Intel Core i5-6600 Quad-core 3.3GHz, Turbo Boost 3.9GHz;
Intel Core i7-6700 Quad-core 3.4GHz, Turbo Boost 4.0GHz;
7th generation 1151-pin CPU for standalone desktop PCs:
Intel Core i3-7100 Dual-Core 3.9GHz; Core i3-7300 Dual-Core 4.0GHz;
Intel Core i3-7320 dual-core 4.1GHz;
Intel Core i5-7400 Quad-core 3.0GHz, Turbo Boost 3.5GHz; Core i5-7500 Quad-core 3.4GHz, Turbo Boost 3.8GHz;
Intel Core i5-7600 Quad-core 3.5GHz, Turbo Boost 4.1GHz;
Intel Core i7-7700 Quad-core 3.6GHz, Turbo Boost 4.2GHz;

	Memory
	1*NB-DDR4 memory, supports 1.2V, supports 2133/2400MHz memory, maximum support 16GB

	
	The QM3600 supports 2*NB-DDR4 memory, supporting 2133/2400/2600MHz memory, with a maximum support of 32GB.

	Network function
	1*RJ45 LAN interface
	Integrated with Realtek 8111F Gigabit Ethernet controller, supporting network power on/off and PXE network functionality.

	
	Supports optional Wi-Fi/Bluetooth, supports 2*Wi-Fi antenna masts

	Display function


	Intel HD Graphics 530/630 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	4 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	3 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS-100B high-fidelity USB audio chip;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
One 2.5-inch SSD or HDD hard drive;
Optional 1*MSATA drive;

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	3
	4
	2
	1*M.2
1 x 2.5-inch SSD/HDD
Optional 1*MSATA
	2*NB-DDR4
MAX 32G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc26668][bookmark: _Toc31737]IPC400U-8th/9th Generation Dedicated CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM3100, QM3600

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	8th generation 1151-pin CPU for standalone desktop PCs:
Intel Core i3-8100 Quad-core 3.6GHz; Core i3-8300 Quad-core 3.7GHz;
Intel Core i5-8400: Six-core, 2.8GHz, turbo boost up to 4.0GHz; Core i5-8500: Six-core, 3.0GHz, turbo boost up to 4.1GHz;
Intel Core i5-8600, six cores, 3.2GHz, turbo boost up to 4.3GHz;
Intel Core i7-8700, six cores, 3.2GHz, turbo boost up to 4.6GHz;
9th generation 1151-pin CPU for standalone desktop PCs:
Intel Core i3-9100 Quad-core 3.6GHz, Turbo Boost 4.2GHz; Core i3-9300 Quad-core 3.7GHz, Turbo Boost 4.2GHz;
Intel Core i5-9400: Six-core, 2.9GHz, turbo boost up to 4.1GHz; Core i5-9500: Six-core, 3.0GHz, turbo boost up to 4.4GHz;
Intel Core i5-9600, six cores, 3.1GHz, turbo boost up to 4.6GHz;
Intel Core i7-9700, eight cores, 3.0GHz, turbo boost up to 4.7GHz;
Intel Core i9-9900, eight cores, 3.1GHz, turbo boost up to 5.0GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666MHz memory, maximum support 32GB

	Network function
	1*RJ45 LAN interface
	Integrated with Realtek 8111F Gigabit Ethernet controller, supporting network power on/off and PXE network functionality.

	
	Supports optional Wi-Fi/Bluetooth, supports 2*Wi-Fi antenna masts

	Display function


	Intel HD Graphics 530/630 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	USB function
	4 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	3 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Cmedia HS-100B high-fidelity USB audio chip;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2;
One 2.5-inch SSD or HDD hard drive;
Optional 1*MSATA drive;

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	DVI-I
	LAN
	USB 2.0
	USB 3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	2K 60Hz
	2
	6
	4
	6
	1*M.2
1 x 2.5-inch SSD/HDD
	2*PC-DDR4
MAX 64G
	200W
The above power supply

	

	PC model
	[bookmark: _Toc24538][bookmark: _Toc25020][bookmark: _Toc27805][bookmark: _Toc25085][bookmark: _Toc7736]IPC400U-GK6900 series

	PC size
	428mm (L)*350mm (W)*88mm (H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	GK6900

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	Supports Intel 6th/7th/8th/9th generation desktop platform 1151-pin i3, i5, i7, and i9 discrete CPUs (see next page for CPU list details).

	Chipset
	Intel H310C Chipset

	Memory
	2*PC-DDR4 memory , supports 2133/2400/2666MHz memory, maximum support 64GB

	Network function
	2 RJ45 LAN ports
	Supports dual Gigabit Ethernet controllers (Intel I219V + Intel I225-LM), supports network power on/off, and network PXE functionality.

	Display function


	Intel HD Graphics 530/630 integrated graphics, supporting single display, dual display duplication, and dual display expansion; single display under DOS.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports resolution 1920*1080@60Hz

	
	1*DVI-I interface
	Supports resolution 1920*1080@60Hz

	
	1 PCI-E x16 interface
	A standard PCI-E x16 slot allows for the connection of external devices such as discrete graphics cards.

	USB function
	6 USB 3.0 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	4 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 897 HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*LINE_IN
	Supports line input (blue)

	
	1*LINE_OUT interface
	Supports audio output (green)

	
	1*MIC_IN interface
	Microphone input is supported (red).

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2 disk;
1 x 2.5-inch SSD or HDD

	On/off function
	POWER button
	switch button

	Other I/O
	6*COM interface
	Supports RS232 ( RS485 support can be customized).

	
	1 PS/2 interface
	Standard PS/2 1-to-2 interface, supports PS/2 keyboard/mouse

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Windows 8, Windows 7, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

Information on Intel 6th/7th/8th/9th generation desktop platform 1151-pin discrete CPUs:
	CPU Specifications
	CPU Brand
	CPU model
	clock speed
	Turbo Boost
	CPU power consumption is approximately (W)
	CPU full load power consumption (W)

	6th generation i3
	Intel
Core
	6100
	Dual-core 3.7G
	
	65
	90

	
	
	6300
	Dual-core 3.8G
	
	65
	90

	
	
	6320
	Dual-core 3.9G
	
	65
	90

	6th generation i5
	Intel
Core
	6400
	Quad-core 2.7GHz
	3.3G
	65
	90

	
	
	6500
	Quad-core 3.2GHz
	3.6G
	65
	90

	
	
	6600
	Quad-core 3.3GHz
	3.9G
	65
	90

	6th generation i7
	Intel Core
	6700
	Quad-core 3.4GHz
	4.0G
	65
	90

	7th generation i3
	Intel
Core
	7100
	Dual-core 3.9G
	
	65
	90

	
	
	7300
	Dual-core 4.0G
	
	65
	90

	
	
	7320
	Dual-core 4.1G
	
	65
	90

	7th Gen i5
	Intel
Core
	7400
	Quad-core 3.0GHz
	3.5G
	65
	90

	
	
	7500
	Quad-core 3.4GHz
	3.8G
	65
	90

	
	
	7600
	Quad-core 3.5GHz
	4.1G
	65
	90

	7th generation i7
	Intel Core
	7700
	Quad-core 3.6GHz
	4.2G
	65
	90

	8th generation i3
	Intel
Core
	8100
	Quad-core 3.6GHz
	
	65
	90

	
	
	8300
	Quad-core 3.7GHz
	
	65
	90

	8th Gen i5
	Intel
Core
	8400
	Six-core 2.8GHz
	4.0G
	65
	90

	
	
	8500
	Six-core 3.0GHz
	4.1G
	65
	90

	
	
	8600
	Six-core 3.2GHz
	4.3G
	65
	90

	8th Gen i7
	Intel Core
	8700
	Six-core 3.2GHz
	4.6G
	65
	90

	9th generation i3
	Intel Core
	9100
	Quad-core 3.6GHz
	4.2G
	65
	90

	
	
	9300
	Quad-core 3.7GHz
	4.2G
	65
	90

	9th Gen i5
	Intel
Core
	9400
	Six-core 2.9GHz
	4.1G
	65
	90

	
	
	9500
	Six-core 3.0GHz
	4.4G
	65
	90

	
	
	9600
	Six-core 3.1GHz
	4.6G
	65
	90

	9th Gen i7
	Intel Core
	9700
	Octa-core 3.0G
	4.7G
	65
	90

	9th generation I9
	Intel Core
	9900
	Octa-core 3.1GHz
	5.0G
	65
	90



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2
	1*MSATA
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc9603][bookmark: _Toc13241]IPC400U-10th/11th Generation Dedicated CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM5100

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	1200-pin 10th generation CPU for standalone desktop PC:
Intel Core i3-10100 Quad-core 3.6GHz, Turbo Boost 4.3GHz; Core i3-10105 Quad-core 3.7GHz, Turbo Boost 4.4GHz;
Intel Core i3-10300 Quad-core 3.7GHz, Turbo Boost 4.4GHz; Core i3-10305 Quad-core 3.8GHz, Turbo Boost 4.5GHz;
Intel Core i3-10320 Quad-core 3.8GHz, Turbo Boost 4.6GHz; Core i3-10325 Quad-core 3.9GHz, Turbo Boost 4.7GHz;
Intel Core i5-10400: 6 cores, 2.9GHz, turbo boost up to 4.3GHz; Core i5-10505: 6 cores, 3.2GHz, turbo boost up to 4.6GHz;
Intel Core i5-10500: 6 cores, 3.1GHz, turbo boost up to 4.5GHz; Intel Core i5-10600: 6 cores, 3.3GHz, turbo boost up to 4.8GHz;
Intel Core i7-10700, eight cores, 2.9GHz, turbo boost up to 4.8GHz;
Intel Core i9-10900: 10 cores, 2.8GHz, turbo boost up to 5.2GHz;
1200-pin 11th generation CPU for standalone desktop PCs:
Intel Core i5-11400: 6 cores, 2.6GHz, turbo boost up to 4.4GHz; Core i5-11500: 6 cores, 2.6GHz, turbo boost up to 4.6GHz;
Intel Core i5-11600, six cores, 2.8GHz, turbo boost up to 4.8GHz;
Intel Core i7-11700, eight cores, 2.5GHz, turbo boost up to 4.9GHz;
Intel Core i9-11900, eight cores, 2.5GHz, turbo boost up to 5.2GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666/2933MHz memory, maximum support 64GB

	Network function
	1*RJ45 LAN interface
	Integrated with Realtek 8111H Gigabit Ethernet controller, supporting network power on/off and PXE network functionality.

	
	Supports optional Wi-Fi/Bluetooth, supports 2*Wi-Fi antenna masts

	Display function


	Intel HD Graphics 630/730/750 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	
	10th generation CPUs support 4K at 30Hz; 11th generation CPUs support 4K at 60Hz.

	USB function
	2 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	6 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC 662/897 HD digital audio decoder, 6-channel high-fidelity audio controller;
Alternatively, it can integrate the Cmedia HS-100B high-fidelity USB audio chip;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive; 1*2.5-inch SSD or HDD hard drive;

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	
	
	
	
	
	6
	
	
	

	

	PC model
	[bookmark: _Toc2366][bookmark: _Toc11234]IPC400U-12th/13th Generation Dedicated CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6300, QM6100

	power supply
	ATX power supply
	A power supply of 200W or higher is recommended.

	CPU
	12th generation 1700-pin CPU for standalone desktop PCs:
Intel Core i3-12100 Quad-core 3.3GHz, Turbo Boost 4.3GHz; Core i3-12300 Quad-core 3.5GHz, Turbo Boost 4.4GHz;
Intel Core i5-12400: 6 cores, 2.5GHz, turbo boost up to 4.4GHz; Core i5-12500: 6 cores, 3.0GHz, turbo boost up to 4.6GHz;
Intel Core i5-12600, six cores, 3.3GHz, turbo boost up to 4.8GHz;
Intel Core i7-12700, 12 cores, 2.1GHz, turbo boost up to 4.9GHz;
Intel Core i9-12900, 16 cores, 2.4GHz, turbo boost up to 5.1GHz;
13th generation 1700-pin CPU for standalone desktop PCs:
Intel Core i5-13100 Quad-core 3.4GHz, Turbo Boost 4.5GHz;
Intel Core i5-13400: 10 cores, 2.5GHz, turbo boost up to 4.6GHz; Core i5-13500: 14 cores, 2.5GHz, turbo boost up to 4.8GHz;
Intel Core i5-13600, 14 cores, 2.7GHz, turbo boost up to 5.3GHz;
Intel Core i7-13700, 16 cores, 2.1GHz, turbo boost up to 5.2GHz;
Intel Core i9-13900, 24 cores, 2.3GHz, turbo boost up to 5.6GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666/2933/3200MHz memory, maximum support 128GB

	Network function
	1*RJ45 LAN interface
	Integrated with Realtek 8111H Gigabit Ethernet controller, supporting network power on/off and PXE network functionality.

	
	Supports M.2 Wi-Fi/Bluetooth optional, supports 2*Wi-Fi antenna masts

	Display function


	Intel HD Graphics 730/770 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	
	10th generation CPUs support 4K at 30Hz; 11th generation CPUs support 4K at 60Hz.

	USB function
	4 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	4 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC897 HD digital audio decoder, 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*M.2 drive; 1*2.5-inch SSD or HDD hard drive;

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
[bookmark: _GoBack]
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI
	VGA
	LAN
	USB 2.0
	USB 3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2
	1*M.2
1 x 2.5-inch SSD/HDD
	2*NB-DDR4
MAX 64G
	200W
The above power supply

	

	PC model
	[bookmark: _Toc20800][bookmark: _Toc20364]IPC400U-14th Generation Dedicated CPU Series

	PC size
	380mm(L)*351mm(W)*160mm(H)

	Cooling system
	With ventilation holes and silent fan cooling

	color
	black

	Compatible motherboard models
	QM6100

	power supply
	ATX power supply
	It is recommended to use a power supply of 200W or higher.

	CPU
	14th generation 1700-pin CPU for standalone desktop PCs:
Intel Core i3-14100 Quad-core 3.5GHz, Turbo Boost 4.7GHz;
Intel Core i5-14400: 10 cores, 2.5GHz, turbo boost up to 4.7GHz; Core i5-14500: 14 cores, 2.6GHz, turbo boost up to 5.0GHz;
Intel Core i5-14600, 14 cores, 2.7GHz, turbo boost up to 5.2GHz;
Intel Core i7-14700, 20 cores, 2.1GHz, turbo boost up to 5.4GHz;
Intel Core i9-14900, 24 cores, 2.0GHz, turbo boost up to 5.8GHz;

	Memory
	2*NB-DDR4 memory, supports 1.2V, supports 2133/2400/2666/2933/3200MHz memory, maximum support 128GB

	Network function
	1*RJ45 LAN interface
	Integrated with Realtek 8111H Gigabit Ethernet controller, supporting network power on/off and PXE network functionality.

	
	Supports M.2 Wi-Fi/Bluetooth optional, supports 2*Wi-Fi antenna masts

	Display function


	Intel HD Graphics 730/770 graphics controller, supporting single display, dual display duplication, and dual display expansion.

	
	1*VGA DB15 interface
	Supports resolution 1920*1080@60Hz

	
	1 HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	
	10th generation CPUs support 4K at 30Hz; 11th generation CPUs support 4K at 60Hz.

	USB function
	4 USB 3.2 ports
	The blue group of USB ports is USB 3.2 Gen1.

	
	4 USB 2.0 ports
	The black USB connector is USB 2.0.

	sound function
	Integrated Realtek ALC897 HD digital audio decoder, 6-channel high-fidelity audio controller;

	
	1*SPK interface
	Supports audio output

	
	1*MIC interface
	Microphone input supported

	
	The HDMI interface supports HDMI audio output.

	Hard drive function
	1*MSATA drive; 1*2.5-inch SSD or HDD hard drive;

	On/off function
	POWER button
	switch button

	Other I/O
	2/6*COM interface
	Supports RS232 ( 2*RS485 support can be customized).

	Operating environment
	Operating temperature: -10℃ to 60℃; Operating humidity: 5% to 95% relative humidity, non-condensing.
Storage temperature: -20℃ to 70℃;

	BIOS
	AMI BIOS supports power-on, scheduled power-on, and remote power-on/off.

	Watch Dog
	Watchdog programming with support for hardware reset function (256 levels, 0~255 seconds).

	operating system
	Windows 11, Windows 10, Linux, etc.


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※


1

image6.png
AC/220V





image7.jpeg




image8.jpeg




image9.jpeg




image10.jpeg




image11.png
31

398.40m.

105.,

105,

413m





image12.png
8888888





image2.jpeg
380mm





image3.jpeg
AC/220V





image4.jpeg
AC/220v





image5.jpeg
AC/220V





image1.png
®
FUBTHABCEBFRAREBEAT

(13T SHENZHEN ELSKY TECHNOLOGY CO.,LTD

Titanium





