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ELSKY IPC6000-6C Mini PC Specification
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Mini PC size


―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Single network interface

―――――――――――――――――――――――――――――――――――――――――――――――――――――――




―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Dual network interface




―――――――――――――――――――――――――――――――――――――――――――――――――――――――

DP interface



―――――――――――――――――――――――――――――――――――――――――――――――――――――――











―――――――――――――――――――――――――――――――――――――――――――――――――――――――




―――――――――――――――――――――――――――――――――――――――――――――――――――――――
LPT interface



―――――――――――――――――――――――――――――――――――――――――――――――――――――――



―――――――――――――――――――――――――――――――――――――――――――――――――――――――

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
The pictures are for reference only, please refer to the actual product!
Product model ordering optional:
	PC model
	Motherboard 
	HDMI
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory（MAX）
	Power

	J1900 series
	M219F
	2K 60Hz
	1
	7
	1
	6
	1*MSATA;
1*2.5-inch disk
	1*DDR3;8G
	12V

	
	
	
	2
	5
	1
	6
	
	
	

	J3355 series
	M335F
	4K 30Hz
	1
	5
	2
	6
	
	1*DDR3;8G
	12V

	
	
	
	2
	3
	2
	6
	
	
	

	3rd gen series
	HGP series
	2K 60Hz
	1
	6
	2
	6
	
	1*DDR3;8G
	12V

	
	
	
	2
	4
	2
	6
	
	
	

	4th, 5th gen  series
	QM9400
QM9500
	4K 30Hz
	1
	6
	2
	6
	
	1*DDR3;8G
	12V

	
	
	
	2
	4
	2
	6
	
	
	

	Domestic Zhaoxin
	KC6000
	4K 30Hz
	1
	6
	2
	6
	
	2*DDR4;64G
	12V/19V

	
	
	
	2
	4
	2
	6
	
	
	

	6th, 7th gen  series
	QM9600
QM9700
	4K 30Hz
	1
	6
	2
	6
	
	2*DDR3;16G
	12V/19V

	
	
	
	2
	4
	2
	6
	
	
	

	8th, 10th gen  series
	QM9850
QM10U
	4K 30Hz
	1
	6
	2
	6
	1*MSATA;
1*2.5-inch disk;
1*M.2 SSD
	2*DDR4;32G
	12V/19V

	
	
	
	2
	4
	2
	6
	
	
	



Mini PC Specification:
	PC model
	IPC6000-J1900 series

	Motherboard model
	M218F, M219F, M218FC, M219FC, M218H, M219H

	PC size
	234mm*205mm*53mm

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm and supports 12V. It is recommended to use a power supply of 12V5A or higher

	CPU
	Intel Celeron J1800 dual core 2.41GHz, turbo 2.58GHz;
Intel Celeron J1900 quad core 1.99GHz, turbo 2.4GHz;
Intel Pentium J2900 quad core 2.41GHz, turbo 2.66GHz;
Intel Celeron N2840 Dual Core 2.16GHz, turbo 2.58GHz;
Intel Celeron N2930 quad core 1.83GHz, turbo 2.16GHz;
Intel Celeron N2940 quad core 1.83GHz, turbo 2.25GHz;

	Chipset
	Intel Bay trail SOC chipset

	Memory
	1*NB-DDR3 memory, supports 1.35V, 1600MHz memory, maximum support 8GB

	Network function
	Integrated Realtek 8111E Gigabit Ethernet card or Realtek 8105E 100Mbps Ethernet card optional, supporting Wake on LAN and network PXE function

	
	Supports WIFI/4G/Bluetooth optional, supports 2 * WIFI antenna pole

	Display function

	Intel HD Graphics (Sandy Bridge) graphics controller, support single display, dual display replication, and dual display expansion

	
	1*VGA DB15 port
	Support resolution 1920*1080@60Hz

	
	1*HDMI 1.4 port
	Support resolution 1920*1080@60Hz

	USB function
	1*USB3.0 port
	The blue group USB is USB 3.0 speed (blue group, below the chassis direction is USB 3.0)

	
	5*USB2.0 port
	The black group USB is USB 2.0 speed (the blue group, above the chassis direction is USB 2.0)

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller
Or integrated Cmedia HS_100B USB audio chip

	
	1*SPK port
	Support audio output

	
	1*MIC port
	Support microphone input

	
	HDMI interface supports HDMI audio output

	Hard disk function
	1*MSATA disk; 
1*2.5-inch hard drive (SSD or HDD);

	Switch function
	POWER button
	Switch button

	Other I/O
	6*COM port
	Supports RS232; COM3/4 can optionally support RS232/RS422/RS485;
COM6 can optionally support RS232/RS485;

	
	1*LPT port
	Parallel port, standard printing port 

	Operating environment
	[bookmark: _GoBack]Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS,support power on, timed power on, and remote power on

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10, Windows 8, Windows 7, Linux, etc


Instructions:
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;
Mini PC Specification:
	PC model
	IPC6000-J3355 series

	Motherboard model
	M335F

	PC size
	234mm*205mm*53mm

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm and supports 12V. It is recommended to use a power supply of 12V5A or higher

	CPU
	Intel Celeron J3355 dual core 2.0GHz, turbo 2.5GHz;
Intel Celeron J3455 quad core 1.5GHz, turbo 2.3GHz;
Intel Pentium N4200 quad core 1.1GHz, turbo 2.5GHz;

	Chipset
	Intel Apollo Lake SOC chipset

	Memory
	1*NB-DDR3 memory, supports 1.35V, 1600MHz memory, maximum support 8GB

	Network function
	Integrated Realtek 8111H Gigabit Ethernet card, supporting Wake on LAN and network PXE function

	
	Supports WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Display function

	Intel HD Graphics 500/505 graphics controller, supporting single display, dual display replication, and dual display expansion

	
	1*VGA DB15 port
	Support resolution 1920*1080@60Hz

	
	1*HDMI 1.4 port
	Support 4K resolution 4096/3840*2160@30Hz

	USB function
	2*USB3.0 port
	The blue group USB is USB 3.0 speed

	
	5*USB2.0 port
	The black group USB is USB 2.0 speed

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller

	
	1*SPK port
	Support audio output

	
	1*MIC port
	Support microphone input

	
	HDMI interface supports HDMI audio output

	Hard disk function
	1*MSATA disk;
1*2.5-inch hard drive (SSD or HDD)

	Switch function
	POWER button
	Switch button

	Other I/O
	6*COM port
	Supports RS232; COM4/6 can optionally support RS232/RS422/RS485;

	
	1*LPT port
	Parallel port, standard printing port

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS， Support power on, timed power on, and remote power on

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10 64 bit, Linux, etc


Instructions:
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;








Mini PC Specification:
	PC model
	IPC6000-3rd gen series

	Motherboard model
	1037F, 2117F, i3HGP, i5HGP, i7HGP

	PC size
	234mm*205mm*53mm

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm and supports 12V. 
It is recommended to use a power supply of 12V5A or higher

	3rd gen CPU
	Intel Celeron 1037U dual core 1.8GHz;
Intel Pentium 2117U dual core 1.8GHz;
Intel Core i3-3217U dual core 1.8GHz;
Intel Core i3-3227U Dual Core 1.9GHz;
Intel Core i5-3317U dual core 1.7GHz, turbo 2.6GHz;
Intel Core i5-3337U dual core 1.8GHz, turbo 2.7GHz;
Intel Core i5-3427U dual core 1.8GHz, turbo 2.8GHz;
Intel Core i5-3437U dual core 1.9GHz, turbo 2.9GHz;
Intel Core i7-3517U dual core 1.9GHz, turbo 3.0GHz;
Intel Core i7-3537U dual core 2.0GHz, turbo 3.1GHz;
Intel Core i7-3667U dual core 2.0GHz, turbo 3.2GHz;
Intel Core i7-3687U dual core 2.1GHz, turbo 3.3GHz;

	Chipset
	intel 6 series chipset: HM65, HM67, QM67
intel 7 series chipset: NM70, HM70, HM75, HM76, HM77, QM77

	Memory
	1*NB-DDR3 memory, support 1.35V/1.5V,support 1333/1600MHz memory,maximum support 8G

	Network function
	Integrated Realtek 8111E Gigabit Ethernet card or Realtek 8105E 100Mbps Ethernet card optional, supporting Wake on LAN and network PXE function

	
	Support WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Display function

	Intel HD Graphics 4000 graphics controller, support single display, dual display replication, and dual display expansion

	
	1*VGA DB15 port
	Support resolution 1920*1080@60Hz

	
	1*HDMI 1.4 port
	Support resolution 1920*1080@60Hz

	USB function
	2*USB3.0 port
	The blue group USB is USB3.0 speed 
(USB 2.0 speed when using Intel 6 series chipset)

	
	4*USB2.0 port
	The black group USB is USB2.0 speed

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller
Or integrated Cmedia HS_100B USB audio chip

	
	1*SPK port
	Support audio output

	
	1*MIC port
	Support microphone input

	
	HDMI interface support HDMI audio output

	Hard disk function
	1*MSATA disks;
1*2.5-inch disks (SSD or HDD)

	Switch function
	POWER button
	Switch button

	Other I/O
	6*COM port
	Support RS232; COM2 optional supports RS422/RS485

	
	1*LPT port
	Parallel port, standard printing port

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS,support power on, timed power on, and remote power on

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10, Windows 8, Windows 7, Windows XP, Linux, etc


Instructions:
☆ When the main chipset is an Intel 6 series chipset, the blue USB interface is USB 2.0 and there is no USB 3.0;
☆ When the main chipset is Intel 7 series chipset, the blue USB interface is USB 3.0;
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;



Mini PC Specification:
	PC model
	IPC6000-4th,5th gen series

	Motherboard model
	QM9400, QM9500 series

	PC size
	234mm*205mm*53mm

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm and supports 12V. 
It is recommended to use a power supply of 12V5A or higher.

	



4th gen CPU
	Intel Core i3-4005U dual core 1.7GHz; Core i3-4010U dual core 1.7GHz;
Intel Core i3-4025U dual core 1.9GHz; Core i3-4030U dual core 1.9GHz;
Intel Core i3-4100U Dual Core 1.8GHz;
Intel Core i5-4200U dual core 1.6GHz, turbo 2.6GHz; Core i5-4210U dual core 1.7GHz, turbo 2.7GHz;
Intel Core i5-4250U dual core 1.3GHz, turbo 2.6GHz; Core i5-4278U dual core 2.6GHz, turbo 3.1GHz;
Intel Core i5-4300U dual core 1.9GHz, turbo 2.9GHz; Core i5-4308U dual core 2.8GHz, turbo 3.3GHz;
Intel Core i5-4310U dual core 2.0GHz, turbo 3.0GHz; Core i7-4500U dual core 1.8GHz, turbo 3.0GHz;
Intel Core i7-4510U dual core 2.0GHz, turbo 3.1GHz; Core i7-4550U dual core 1.5GHz, turbo 3.0GHz;
Intel Core i7-4558U dual core 2.8GHz, turbo 3.3GHz; Core i7-4578U dual core 3.0GHz, turbo frequency 3.5GHz;
Intel Core i7-4600U dual core 2.1GHz, turbo 3.3GHz; Core i7-4650U dual core 1.7GHz, turbo 3.0GHz;

	



5th gen CPU
	Intel Core i3-5005U Dual Core 2.0GHz; Core i3-5010U dual core 2.1GHz;  
Intel Core i3-5015U Dual Core 2.1GHz; Core i3-5020U dual core 2.2GHz;
Intel Core i5-5200U dual core 2.2GHz, turbo 2.7GHz; Core i5-5250U dual core 1.6GHz, turbo 2.7GHz;
Intel Core i5-5257U dual core 2.7GHz, turbo 3.1GHz; Core i5-5287U dual core 2.9GHz, turbo 3.3GHz;
Intel Core i5-5300U dual core 2.3GHz, turbo 2.9GHz; Core i5-5350U dual core 1.8GHz, turbo 2.9GHz;
Intel Core i7-5500U dual core 2.4GHz, turbo 3.0GHz; Core i7-5550U dual core 2.0GHz, turbo 3.0GHz;
Intel Core i7-5557U dual core 3.1GHz, turbo 3.4GHz; Core i7-5600U dual core 2.6GHz, turbo 3.2GHz;
Intel Core i7-5650U dual core 2.2GHz, turbo 3.1GHz;

	Chipset
	Intel Bay trail SOC chipset

	Memory
	1*NB-DDR3 memory, supports 1.35V, 1600MHz memory, maximum support 8GB

	Network function
	Integrated Realtek 8111E Gigabit Ethernet card or Realtek 8105E 100Mbps Ethernet card optional, supporting Wake on LAN and network PCIe functionality

	
	Supports WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Display function

	Intel HD Graphics (Sandy Bridge) graphics controller, support single display, dual display replication, and dual display expansion

	
	1*VGA DB15 port
	Support resolution 1920*1080@60Hz

	
	1*HDMI 1.4 port
	Support 4K resolution 4096/3840*2160@30Hz

	USB function
	2*USB3.0 port
	The blue group USB is USB 3.0 speed

	
	4*USB2.0 port
	The black group USB is USB2.0 speed

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller
Or integrated Cmedia HS_100B USB audio chip

	
	1*SPK port
	Support audio output

	
	1*MIC port
	Support microphone input

	
	HDMI interface supports HDMI audio output

	Hard disk function
	1*MSATA disks;
1*2.5-inch disks (SSD or HDD)

	Switch function
	POWER button
	Switch button

	Other I/O
	6*COM port
	Support RS232; COM2 optional support RS422/RS485       

	
	1*LPT port
	Parallel port, standard printing port                              

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS, support power on, timed power on, and remote power on

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10, Windows 8, Windows 7, Linux, etc





Mini PC Specification:
	PC model
	IPC6000-Domestic Zhaoxin Series

	Motherboard model
	KC6000

	PC size
	234mm*205mm*53mm

	CPU
	Support the full range of domestically produced Zhaoxin KX6000 16NM board mounted CPUs

	Memory support
	2*NB-DDR4 memory slot, supports 2133/2400/2666MHZ memory, maximum support 64G

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm, supporting 12V/19V
The U6580 motherboard has a full load power consumption of approximately 90W, and it is recommended to use a power supply of 12V10A or 19V6A or higher

	Display function
	Integrated ZX C960 DX11 ultra core graphics card, supporting single display, dual display/triple display replication, dual display/triple display expansion

	
	1*VGA DB15 port
	Support resolution 1920*1080@60HZ

	
	1*HDMI 1.4 port
	Support 4K resolution 4096/3840*2160@30HZ

	Network function
	1*LAN port
	Realtek 8111H Gigabit Ethernet card chip, supporting network wake-up and PXE diskless boot function

	
	Supports WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Hard disk function
	1*MSATA disks;
1*2.5-inch disks (SSD or HDD)

	
	1*SATA1 port
	Standard SATA 3.0 hard drive interface, maximum transfer speed of 6.0 Gbps

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller

	
	1*LINE_OUT port
	Supports audio output (green)

	
	1*MIC_IN port
	Supports microphone input (red)

	USB function
	2*USB3.0 port
	Rear standard USB 3.0 interface

	
	4*USB2.0 port
	Rear standard USB 2.0 interface

	Switch function
	POWER
	Switch button

	Other I/O
	6*COM port
	Supports RS232; COM1 optional supports RS422/RS485

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS,support power on, timed power on, and intelligent recognition of remote power on/off devices

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Support Windows 10 64, Linux,etc


Explanation:
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;















Mini PC Specification:
	PC model
	IPC6000-6th,7th gen series

	Motherboard model
	QM9600, QM9700 series; 
QM9650,QM9750

	PC size
	234mm*205mm*53mm

	Power supply
	1*DC_IN
	The inner diameter of the DC head is 2.5mm, supporting 12V/19V. 
It is recommended to use a power supply of 12V5A or 19V5A or higher

	



6th gen CPU
	Intel Celeron 3855U dual core 1.6GHz;
Intel Celeron 3955U dual core 2.0GHz;
Intel Core i3-6006U dual core 2.0GHz;
Intel Core i3-6100U dual core 2.3GHz;
Intel Core i5-6200U dual core 2.3GHz, turbo 2.8GHz;
Intel Core i5-6300U dual core 2.4GHz, turbo 3.0GHz;
Intel Core i7-6500U dual core 2.5GHz, turbo 3.1GHz;
Intel Core i7-6600U dual core 2.6GHz, turbo 3.4GHz;

	



7th gen CPU
	Intel Celeron 3865U dual core 1.8GHz;
Intel Celeron 3965U dual core 2.2GHz;
Intel Core i3-7020U dual core 2.3GHz;
Intel Core i3-7100U dual core 2.4GHz;
Intel Core i3-7130U dual core 2.7GHz;
Intel Core i5-7200U dual core 2.5GHz, turbo 3.1GHz;
Intel Core i5-7300U dual core 2.6GHz, turbo 3.5GHz;
Intel Core i7-7500U dual core 2.7GHz, turbo 3.5GHz;
Intel Core i7-7600U dual core 2.8GHz, turbo 3.9GHz;

	Chipset
	Single chip integrated into CPU

	Memory
	2*NB-DDR3 memory, supports 1.35V, 1600MHz memory, maximum support 16GB

	Network function
	Integrated Realtek 8111F Gigabit Ethernet card, supporting Wake on LAN and network PXE function

	
	Supports WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Display function

	6th generation integrated Intel HD Graphics 510/520 graphics controller, supporting single display, dual display replication, and dual display expansion
7th generation integrated Intel HD Graphics 610/620 graphics controller, supporting single display, dual display replication, and dual display expansion

	
	1*VGA DB15 port
	Supports resolution 1920*1080@60HZ

	
	1*HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30HZ

	USB function
	2*USB3.0 port
	The blue group USB is USB 3.0 speed

	
	4*USB2.0 port
	The black group USB is USB2.0 speed

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller
Or integrated Cmedia HS_100B USB audio chip

	
	1*SPK port
	Support audio output

	
	1*MIC port
	Support microphone input

	
	HDMI interface supports HDMI audio output

	Hard disk function
	1*MSATA disks;
1*2.5-inch disks (SSD or HDD)

	Switch function
	POWER button
	Switch button

	Other I/O
	6*COM port
	Supports RS232; COM2 optional supports RS422/RS485

	
	1*LPT port
	Parallel port, standard printing port

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS,support power on, timed power on, and remote power on

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10, Windows 8, Windows 7, Linux, etc


Instructions:
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;



Mini PC Specification:
	PC model
	IPC6000-8th,10th gen series

	Motherboard model
	QM9850, QM10U, QM8H, QM9H, QM10H,etc

	PC size
	234mm*205mm*53mm

	CPU
	Supports 8th generation Whiskey Lake CPU: I3-8145U, I5-8265U, I7-8665U, etc

	
	Supports 10th generation Comet Lake CPU: I3-10110U, I5-10210U, I7-10510U, etc

	Memory
	2*NB-DDR4 memory slot, supports 2133/2400/2666MHz memory, maximum support 64GB

	Power supply
	1*DC_IN
	Supports 12V voltage, with a DC head inner diameter of 2.5MM.
The motherboard full load power consumption of approximately 85W. 
It is recommended to use a 12V7A or higher power supply

	Display function

	Integrated Intel UHD Graphics ultra core graphics card, supporting single display, dual/triple display replication, dual/triple display expansion, single display under DOS

	
	1*VGA DB15 port
	Support resolution 1920*1080@60HZ

	
	1*HDMI 1.4 port
	Support 4K resolution 4096/3840*2160@30HZ

	Network function
	1*LAN port
	Realtek 8111H Gigabit network card chip, support network wake-up and PXE diskless boot function

	
	Support WIFI/4G/Bluetooth optional, supports 2*WIFI antenna pole

	Hard disk function
	1*M.2 port
	Default support for M.2 2280, optional 2242; 
Default NVME (PCIE) protocol, SATA protocol can be changed

	
	1*SATA1 port
	Standard SATA 3.0 hard drive interface, maximum transfer speed of 6.0 Gbps

	
	Choose between SATA1 signal and MSATA signal, default supports SATA1

	
	1*SATA2 port
	Standard SATA 3.0 hard drive interface, maximum transfer speed of 6.0 Gbps

	Sound function
	Integrated Realtek ALC662 HD digital audio decoder, 6-channel high fidelity audio controller
Or integrated BBH621 USB audio chip

	
	1*LINE_OUT port
	Supports audio output (green)

	
	1*MIC_IN port
	Supports microphone input (red)

	USB function
	2*USB3.1 port
	Rear standard USB 3.1 Gen2 interface, with a maximum transmission bandwidth of 10.0Gbps

	
	4*USB2.0 port
	Rear standard USB 2.0 interface, maximum transmission bandwidth of 480Mbps (60MB/s)

	Switch function
	POWER
	Switch button

	Other I/O
	6*COM port
	Supports RS232; COM1 optional supports RS422/RS485

	Operating environment
	Working temperature: -10 ℃~60 ℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS, support power on, timed power on, and intelligent recognition of remote power on/off devices

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Supports Windows 10 64, Linux, etc


Instructions:
☆ Single Gigabit Ethernet port/Dual Gigabit Ethernet port optional for the PC; Dual network ports only affect the number of USB 2.0 ports;
☆ The PC is equipped with wall mounted holes;
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