
ELSKY IPC6900 Mini PC Specification
―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Mini pc size

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface:VGA+large audio port+single network

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface: VGA+small audio port+single network

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface: VGA+small audio port+dual network

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface:DP+large audio port+ single network

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Rear interface:Optional Phoenix Terminal

―――――――――――――――――――――――――――――――――――――――――――――――――――――――

10USB front interface

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
8USB front interface

―――――――――――――――――――――――――――――――――――――――――――――――――――――――

―――――――――――――――――――――――――――――――――――――――――――――――――――――――



Back of mini pc

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
Mini pc size

―――――――――――――――――――――――――――――――――――――――――――――――――――――――
The pictures are for reference only, please refer to the actual product!
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc28520][bookmark: _Toc22106][bookmark: _Toc18339][bookmark: _Toc19283][bookmark: _Toc22507] IPC6900-Zhaoxin KC6000

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	KC6000

	Motherboard
	CPU
	Support the full range of domestically produced Zhaoxin KX6000 16NM board mounted CPUs:
KX 6640MA Quad core 2.2G ,turbo frequency 2.6G;
KX 6640A quad core 2.6G;   KX U6580 octa core 2.5G;
KX U6780A 8-core 2.7G;     KX U6780 8-core 2.7G

	
	Graphics card
	Integrated ZX C960 DX11 ultra core graphics card, supporting single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4,support 2133/2400/2666MHz memory,maximum support 64G

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM port,default RS232;

	
	USB
	4*USB2.0 port

	Rear panel interface
	Power port
	1*DC power interface (5.5 *2.5mm), recommended 12V10A or 19V5A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*VGA port (1920*1080@60Hz)
1*HDMI®1.4 port (4096/3840*2160@30Hz)

	
	LAN
	Single gigabit network card: Realtek 8111H or Motorcomm YT6801 are optional;
Dual gigabit network card: Realtek 8111H+Realtek 8111H or Motorcomm YT6801+Motorcomm YT6801 optional;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.0 port
2*USB2.0 port (dual network pc without this interface)

	
	Audio
	1*LINE_OUT port,audio output;
1*MIC_IN port,microphone input;

	
	WiFi
	2*WiFi antenna interface;

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	MSATA
	1*MSATA slot, support MSATA disks

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1 signal, supports WiFi module; Can be modified to support 4G/Bluetooth modules

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 10, Windows 7, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/HDMI2®
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA:2K 60Hz
HDMI2®:4K60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc16475] IPC6900-Zhaoxin KC7000

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	KC7000

	Motherboard
	CPU
	Support the full range of domestically produced Zhaoxin KX7000 board mounted CPUs:
Zhaoxin KX 7000 Eight Core 3.5G;

	
	Graphics card
	Integrated ZX C1199 graphics card, support single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4 supports 2133/2400/2666MHz memory, maximum support 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM port,default RS232;

	
	USB
	4*USB2.0 port

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V10A or 19V5A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*VGA port (1920*1080@60Hz)
1*HDMI1®2.0 port (4096/3840*2160@60Hz)
Optional 1*HDMI2®2.0 port (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card: Motorcomm YT6801 or Realtek 8111H are optional;
Dual gigabit network card: Motorcomm YT6801+Motorcomm YT6801 or Realtek 8111H+Realtek 8111H optional;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.0 port
2*USB2.0 port (dual network pc without this interface)

	
	Audio
	1*LINE_OUT port,audio output;
1*MIC_IN port,microphone input;

	
	WiFi
	2*WiFi antenna interface;

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot, support M.2 2280 NVME PCIE4.0 x2/SATA dual protocol adaptive standard SSD

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives

	Expansion 
	M2_WIFI
	1*M2_WIFI interface, supports Key-E interface M.2 2230 PCIE4.0 x1&USB, supports WiFi Bluetooth module

	
	CN1
	1*CN1 interface, supports Key-B interface M.2 5G (3052/3042) module, hardware can be modified to support M.2 4G (3042) module

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95%=-0.9relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA
	LAN
	USB2.0
	USB3.1
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	6
	2
	2/6
	1*M.2;
1*SATA;
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc6637] IPC6900-Phytium ET2000

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	ET2000

	Motherboard
	CPU
	Domestic Phytium Tengrui D2000 eight core 2.3G;
Domestic Phytium Tengrui FT2000 quad core 2.6G;

	
	Graphics card
	Supports X100 bridge with 4G video memory and optional support for X100 bridge with 8G video memory. Supports single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4, supports 2133/2400/2666MHz memory, maximum support 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*VGA port (1920*1080@60Hz)
1*HDMI®1.4 port (4096/3840*2160@30Hz)

	
	LAN
	Single gigabit network card: Motorcomm YT6801 or Realtek 8111H are optional;
Dual gigabit network card: Motorcomm YT6801+Motorcomm YT8521SC or Realtek 8111H+Motorcomm YT8521SC optional
Support network wake-up function;

	
	USB
	2*USB3.1 Gen1 port
2*USB2.0 port (dual network pc without this interface)

	
	Audio
	1*LINE_OUT port,audio output;
1*MIC_IN port,microphone input;

	
	WiFi
	2*WiFi antenna interface;

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot, supports M.2 2280 NVME PCIE3.0 x4/SATA dual protocol adaptive standard SSD

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives

	
	MSATA
	Optional 1*MSATA slot, supports WiFi module by default, can be changed to support MSATA disk

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1&USB signals, supports WiFi Bluetooth/4G modules; Can be modified to support MSATA disks

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Support Galaxy Kirin ( Kylin-Desktop-V10-SP1-Release-2503-ARM64), Linux, etc. Domestic system (supporting X100 version)


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA
	LAN
	USB2.0
	USB3.0
	COM
	SSD
	Memory
	Power

	2K 30Hz
	1024*768@60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	1*NB-DDR4
MAX 32G
	12V/19V

	
	
	2
	8
	
	
	
	
	

	

	PC model
	[bookmark: _Toc11652] IPC6900-Phytium QT2000

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QT2000

	Motherboard
	CPU
	Domestic Phytium Tenglong E2000Q quad core 1.5G;

	
	Graphics card
	Support single display, dual display replication, and dual display expansion

	
	Memory
	1*NB-DDR4 supports 2133/2400/2666MHz memory, with a maximum support of 32GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V4A or 19V3A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*VGA port (1024*768@60Hz)
1*HDMI®1.4 port (1920*1080@30Hz)

	
	LAN
	Single gigabit network card: supports Motorcomm YT8521SC;
Dual gigabit network card: supports Motorcomm YT8521SC+Motorcomm YT8521SC;
Support network wake-up function;

	
	USB
	2*USB3.0 port
2*USB2.0 port (dual network pc without this interface)

	
	Audio
	1*LINE_OUT port,audio output;
1*MIC_IN port,microphone input;

	
	WiFi
	2*WiFi antenna interface;

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot, supports M.2 2280 NVME PCIE3.0 x4/SATA dual protocol adaptive standard SSD

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives

	Expansion 
	M2_WIFI
	1*M2_WIFI interface, supports Key-E interface M.2 2230 PCIE3.0 x1&USB signal, supports WiFi Bluetooth module

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Support Galaxy Kylin Embedded System (Kylin-Embedded V10-SP1-General Release Base-2309-ARM64), domestic systems such as Tongxin, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA
	LAN
	USB2.0
	USB3.1
	COM
	SSD
	Memory
	Power

	4K 30Hz
	2K 60Hz
	1
	4
	4
	2/6
	1*M.2;
1*SATA;
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	2
	
	
	
	

	

	PC model
	[bookmark: _Toc18189] IPC6900-Phytium ET3000

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	ET3000

	Motherboard
	CPU
	Domestic Phytium Tengrui D3000 8-core 2.5G;

	
	Graphics card
	Supports X100 bridge with 4G video memory and optional support for X100 bridge with 8G video memory. Supports single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4, supports 2133/2400/2666MHz memory, maximum support 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply

	
	Display port
	1*VGA port (1920*1080@60Hz)
1*HDMI®1.4 port (4096/3840*2160@30Hz)

	
	LAN
	Single gigabit network card: Motorcomm YT6801 or Realtek 8111H are optional;
Dual gigabit network card: Motorcomm YT6801+Motorcomm YT8521SC 
or Realtek 8111H+MotorcommYT8521SC optional
Support network wake-up function;

	
	USB
	Single network host support: 4*USB3.1 Gen1 interface
Dual network host optional support: 2*USB3.1 Gen1 interface

	
	Audio
	1*LINE_OUT port,audio output;
1*MIC_IN port,microphone input;

	
	WiFi
	2*WiFi antenna interface;

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot, support M.2 2280 NVME PCIE4.0 x4/SATA dual protocol adaptive standard SSD; Optional M.2 2242 hard drive;

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives

	
	MSATA
	Optional 1*MSATA slot, supports WiFi module by default, can be changed to support MSATA disk

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1&USB signals, supports WIFI Bluetooth/4G modules; Can be modified to support MSATA disks

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Support Galaxy Kirin(Kylin-Desktop-V10-SP1-Release-2403-ARM64), Linux, Domestic system (supporting X100 version)


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz;
Optional DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2;
1*SATA;
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc7672] IPC6900-8th,10th gen series(QM8H/QM9H/QM10H)

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM8H, QM9H, QM10H

	Motherboard
	CPU
	QM8H: Intel ® Whiskey Lake 8th generation Core i3-8145U, i5-8265U, i7-8655U, etc;
QM9H: Intel ® Coffee Lake 8th generation Core i3-8109U, i5-8259U, i7-8559U, etc;
QM10H: Intel ® Comet Lake 10th generation Core i3-10110U, i5-10210U, i7-10510U, etc;
(See next page for CPU list details)

	
	Graphics card
	Intel UHD Graphics graphics controller, supporting single display, dual display replication, and dual display expansion;

	
	Memory 
	2*NB-DDR4 supports 2133/2400/2666MHz memory, with a maximum support of 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power interface
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply;
1*4Pin Phoenix terminal optional, customizable wire sequence;

	
	Display interface
	1*HDMI®1.4 interface (4096/3840*2160@30Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Realtek 8111H Gigabit Network Card; Optional Motorcomm YT6801 Gigabit Ethernet Card;
Dual Gigabit Network Card: Realtek 8111H+Realtek 8111H Gigabit Network Card; Optional Motorcomm YT6801+Motorcomm YT6801 Gigabit Network Card
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (dual network pc without this interface)

	
	Audio
	1*LINE_OUT interface,audio output;
1*MIC_IN interface,microphone input;

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM port,default RS232; COM1 optional support RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot,support M.2 2280 NVME PCIE3.0 x4 / SATA adaptive standard SSD; 
Optional M.2 2242 hard drive

	
	SATA
	1*SATA3.0 hard drive interface,support 2.5 inch SSD/HDD hard drive or 3.5 inch HDD hard drive

	
	MSATA
	Optional 1 * MSATA slot, supports WiFi module by default, can be changed to support MSATA disk

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1 signal, supports WiFi module; 
Optional support for WiFi Bluetooth/4G module

	
	M.2_5G
	1*M.2 Key-B slot,support M.2 5G(3052/3042) module

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows11, Windows 10, Linux,etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※



The following CPU information is for reference only. Please consult sales for specific requirements!
	CPU 
	CPU brand
	CPU model
	Main frequency
	Turbo
	CPU power consumption
	Full load power consumption of the entire board

	8th gen I3
	Intel Core
	8145U
	Dual core 2.1G
	3.9G
	15W
	60W

	8th gen I5
	Intel Core
	8365U
	Quad core 1.6G
	4.1G
	15W
	60W

	
	
	8265U
	Quad core 1.6G
	3.9G
	15W
	60W

	8th gen I7
	Intel Core
	8665U
	Quad core 1.9G
	4.8G
	15W
	60W

	
	
	8565U
	Quad core1.8G
	4.6G
	15W
	60W

	8th gen I3
(QM9H)
	Intel Core
	8109U
	Dual core 3.0G
	3.6G
	28W
	70W

	
	
	8140U
	Dual core 2.1G
	3.9G
	15W
	60W

	8th gen I5
(QM9H)
	Intel Core
	8259U
	Quad core 2.3G
	3.8G
	28W
	70W

	
	
	8269U
	Quad core 2.6G
	4.2G
	28W
	70W

	
	
	8279U
	Quad core 2.4G
	4.1G
	28W
	70W

	
	
	8257U
	Quad core 1.4G
	3.9G
	15W
	60W

	
	
	8260U
	Quad core 1.6G
	3.9G
	15W
	60W

	8th gen I7
(QM9H)
	Intel Core
	8559U
	Quad core 2.7G
	4.50
	28W
	70W

	
	
	8569U
	Quad core 2.8G
	4.7G
	28W
	70W

	
	
	8557U
	Quad core 1.7G
	4.5G
	15W
	60W

	10th gen I3
	Intel Core
	10110U
	Dual core 2.1G
	4.10G
	15W
	60W

	10th gen I5
	Intel Core
	10310U
	Quad core 1.7G
	4.40G
	15W
	60W

	
	
	10210U
	Quad core 1.6G
	4.20G
	15W
	60W

	10th gen I7
	Intel Core
	10510U
	Quad core 1.8G
	4.90G
	15W
	60W

	
	
	10610U
	Quad core 1.8G
	4.90G
	15W
	60W

	
	
	10810U
	Hexa core 1.1G
	4.90G
	15W
	60W

	
	
	10710U
	Hexa core 1.1G
	4.70G
	15W
	60W



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2 
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc3407] IPC6900-8th,10th gen series(QM8U/QM10U)

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM8U, QM10U

	Motherboard
	CPU
	Support Intel® Whiskey Lake 8th generation:
Intel Celeron 4305U dual core 2.2G; 
Core i3-8145U dual core 2.1GHz, turbo 3.9GHz;    
Intel Core i5-8265U quad core 1.6GHz, turbo 3.9GHz; Core i5-8365U quad core 1.6GHz, turbo 4.1GHz;
Intel Core i7-8655U quad core 1.8GHz, turbo 4.6GHz; Core i7-8665U quad core 1.9GHz, turbo 4.8GHz;
Support Intel ® Comet Lake 10th Generation:
Intel Core i3-10110U dual core 2.1GHz, turbo 4.1GHz;    
Intel Core i5-10210U quad core 1.6GHz, turbo 4.2GHz; Core i5-10310U quad core 1.7GHz, turbo 4.4GHz;
Intel Core i7-10510U quad core 1.8GHz, turbo 4.9GHz; Core i7-10610U quad core 1.8GHz, turbo 4.9GHz;
Intel Core i7-10710U six core 1.1GHz, turbo 4.7GHz; Core i7-10810U six core 1.1GHz, turbo 4.9GHz;

	
	Graphics card
	Intel® UHD Graphics graphics controller, supporting single display, dual display replication, and dual display expansion;

	
	Memory
	2*NB-DDR4,support 2133/2400/2666MHz memory, maximum support 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface ,default RS232;

	
	USB
	4*USB2.0 interface 

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply,
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI®1.4 interface (4096/3840*2160@30Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Realtek 8111H Gigabit Network Card; 
Optional Motorcomm YT6801 Gigabit Ethernet Card;
Dual Gigabit Network Card: Realtek 8111H+Realtek 8111H Gigabit Network Card; 
Optional Motorcomm YT6801+Motorcomm YT6801 Gigabit Network Card
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (dual network host does not have this interface)

	
	Audio
	1*LINE_OUT interface, audio output
1*MIC_IN interface, microphone input

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface, default RS232; COM1 can choose RS232/RS422/RS485;

	Storage
	M.2_SSD
	1*M.2 Key-M slot, support M.2 2280 NVME PCIE3.0 x4/SATA adaptive standard SSD; Optional M.2 2242 hard drive

	
	SATA
	2*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	
	MSATA
	Optional 1*MSATA slot, supports WiFi module by default, 
can be changed to support MSATA disk

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1 signal, supports WiFi module; 
Optional support for WiFi, Bluetooth/4G module

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 11, Windows 10, Linux, etc



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2;
1*SATA
Optional 1*MSATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc1779] IPC6900-11th gen series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM11U

	Motherboard
	CPU
	Support Intel® Tiger Lake 11th generation:
Intel Core i3-1115G4E dual core 2.2GHz, turbo 3.9GHz; Core i3-1115GRE dual core 2.2GHz, turbo 3.9GHz;
Intel Core i3-1115G4 dual core 3.0GHz, turbo 4.1GHz; Core i3-1125G4 quad core 2.0GHz, turbo 3.7GHz;
Intel Core i5-1145G7E quad core 1.5GHz, turbo 4.1GHz; Core i5-1145GRE quad core 1.5GHz, turbo 4.1GHz;
Intel Core i5-1145G7 quad core 2.6GHz, turbo 4.4GHz; Core i5-1135G7 quad core 2.4GHz, turbo 4.2GHz;
Intel Core i5-1155G7 quad core 2.5GHz, turbo 4.5GHz; Core i7-1185GRE quad core 1.8GHz, turbo 4.4GHz;
Intel Core i7-1185G7E quad core 1.8GHz, turbo 4.4GHz; Core i7-1185G7 quad core 3.0GHz, turbo 4.8GHz;
Intel Core i7-1165G7 quad core 2.8GHz, turbo 4.7GHz; Core i7-1195G7 quad core 2.9GHz, turbo 5.0GHz;

	
	Graphics card
	Intel® UHD Graphics / Intel® Iris Xe Graphics graphics controller, support single display, dual display replication, and dual display expansion;

	
	Memory
	2*NB-DDR4,support 2133/2400/2666MHz memory,maximum support 64G

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface,default RS232;

	
	USB
	4*USB2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI®2.0 interface (4096/3840*2160@60Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Supports Intel® i219V Gigabit Ethernet card;
Dual Gigabit Network Card: Supports Intel® i219V +Realtek 8111H Gigabit Ethernet card;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (dual network host does not have this interface)

	
	Audio
	1*LINE_OUT interface ,audio output
1*MIC_IN interface ,microphone input

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface,default RS232; optional support 2*RS232/RS422/RS485

	Storage
	M.2_SSD
	1*M.2 Key-M slot,support M.2 2280 NVME PCIE3.0 x4 / SATA adaptive standard SSD; 
Optional M.2 2242 hard drive

	
	SATA
	1*SATA3.0 hard drive interface, supporting 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	
	MSATA
	Optional 1*MSATA slot, supports WiFi module by default, can be changed to support MSATA disk

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1 signal, supports WiFi module; 
Optional support for WiFi, Bluetooth/4G module

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc5952] IPC6900-12th,13th gen series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM12U, QM13U, QM12P, QM13P, QM12H, QM13H

	Motherboard
	CPU
	Support Intel ® Alder Lake 12th generation U, P, H series Core i3-1215U, i5-1235U, i7-1260P, i9-12900H, etc
Support Intel ® Raptor Lake 13th generation U, P, H series Core i3-1305U, i5-1334U, i7-1340P, i9-13900H, etc
(See next page for CPU list)

	
	Graphics card
	Intel® UHD Graphics / Intel® Iris Xe Graphics graphics controller,support single display,dual display replication,and dual display expansion

	
	Memory
	2*NB-DDR4 supports 2133/2400/2666/2933/320MHz memory, with a maximum support of 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V7A or 19V5A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI®2.0 interface (4096/3840*2160@60Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Intel i219V Gigabit Network Card;
Dual Gigabit Network Card: Intel i219V+Realtek 8111H Gigabit Network Card
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (Dual network host does not have this interface)

	
	Audio
	1*LINE_OUT interface ,audio output;
1*MIC_IN interface,microphone input;

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface,default RS232; COM1 optional support RS232/RS422/RS485

	Storage
	M.2_SSD
	1*M.2 Key-M slot,support M.2 2280 NVME PCIE4.0 x4 / SATA adaptive standard SSD; 
Optional M.2 2242 hard drive;

	
	SATA
	1*SATA3.0 hard drive interface, supporting 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	Expansion 
	M.2_WiFi
	1*M.2 Key-E slot,support M.2 2230 PCIE3.0 x1 & USB,support WiFi Bluetooth module;

	
	M.2_5G
	1*M.2 Key-B slot,support M.2 5G(3052/3042) module or M.2 4G(3042)module;

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The following CPU information is for reference only. Please consult sales for specific requirements!
	CPU
	CPU brand
	CPU model
	Kernel /thread
	Main frequency
	Turbo 
	TDP power consumption(W)
	Maximum turbo power consumption of CPU (W)

	12th gen I3
	Intel Core
	1215U
	6 cores and 8 threads
	1.2G
	4.4G
	15
	55

	12th gen I5
	Intel Core
	1235U
	10 cores and 12 threads
	1.3G
	4.4G
	15
	55

	
	
	1245U
	10 cores and 12 threads
	1.6G
	4.4G
	15
	55

	12th gen I7
	Intel Core
	1265U
	10 cores and 12 threads
	1.8G
	4.8G
	15
	55

	
	
	1255U
	10 cores and 12 threads
	1.7G
	4.7G
	15
	55

	13th gen I3
	Intel Core
	1305U
	5 cores and 6 threads
	1.6G
	4.5G
	15
	55

	
	
	1315U
	6 cores and 8 threads
	1.2G
	4.5G
	15
	55

	13th gen I5
	Intel Core
	1334U
	10 cores and 12 threads
	1.3G
	4.6G
	15
	55

	
	
	1335U
	10 cores and 12 threads
	1.3G
	4.6G
	15
	55

	
	
	1345U
	10 cores and 12 threads
	1.6G
	4.7G
	15
	55

	13th gen I7
	Intel Core
	1355U
	10 cores and 12 threads
	1.7G
	5.0G
	15
	55

	
	
	1365U
	10 cores and 12 threads
	1.8G
	5.2G
	15
	55

	12th gen I3
	Intel Core
	1220P
	10 cores and 12 threads
	1.5G
	4.4G
	28
	64

	12th gen I5
	Intel Core
	1240P
	12 cores and 16 threads
	1.7G
	4.4G
	28
	64

	
	
	1250P
	12 cores and 16 threads
	1.7G
	4.4G
	28
	64

	12th gen I7
	Intel Core
	1280P
	14 cores and 20 threads
	1.8G
	4.8G
	28
	64

	
	
	1260P
	12 cores and 16 threads
	2.1G
	4.7G
	28
	64

	
	
	1270P
	12 cores and 16 threads
	2.2G
	4.8G
	28
	64

	13th gen I5
	Intel Core
	1340P
	12 cores and 16 threads
	1.8G
	4.6G
	28
	64

	
	
	1350P
	12 cores and 16 threads
	1.9G
	4.7G
	28
	64

	13th gen I7
	Intel Core
	1360P
	12 cores and 16 threads
	2.2G
	5.0G
	28
	64

	
	
	1370P
	14 cores and 20 threads
	1.9G
	5.2G
	28
	64

	12th gen I5
	Intel Core
	12450H
	8 cores and 12 threads
	2.0G
	4.4G
	45
	95

	
	
	12500H
	12 cores and 16 threads
	2.5G
	4.5G
	45
	95

	
	
	12600H
	12 cores and 16 threads
	2.7G
	4.5G
	45
	95

	12th gen I7
	Intel Core
	12800H
	14 cores and 20 threads
	2.4G
	4.8G
	45
	115

	
	
	12700H
	14 cores and 20 threads
	2.7G
	4.7G
	45
	115

	
	
	12650H
	10 cores and 16 threads
	2.3G
	4.7G
	45
	115

	12th gen I9
	Intel Core
	12900H
	14 cores and 20 threads
	2.5G
	5.0G
	45
	115

	13th gen I5
	Intel Core
	13420H
	8 cores and 12 threads
	2.1G
	4.60G
	45
	95

	
	
	13500H
	12 cores and 16 threads
	2.6G
	4.70G
	45
	95

	
	
	13600H
	12 cores and 16 threads
	2.8G
	4.80G
	45
	95

	13th gen I7
	Intel Core
	13620H
	10 cores and 16 threads
	2.4G
	4.90G
	45
	115

	
	
	13700H
	14 cores and 20 threads
	2.4G
	5.00G
	45
	115

	
	
	13800H
	14 cores and 20 threads
	2.5G
	5.20G
	45
	115

	13th gen I9
	Intel Core
	13900H
	14 cores and 20 threads
	2.6G
	5.40G
	45
	115



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.1
	COM
	SSD
	Memory
	Power

	4K 30Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc12827] IPC6900-H310 series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM3100, QM3600

	Motherboard
	CPU
	Support Intel ® Skylate 6th generation LGA1151 Core i3-6100, i5-6400, i7-6700, etc
Support Intel ® Kaby Lake 7th generation LGA1151 Core i3-7100, i5-7400, i7-7700, etc
Support Intel ® Coffee Lake 8th generation LGA1151 Core i3-8100, i5-8400, i7-8700, etc
Support Intel ® Coffee Lake 9th generation LGA1151 Core i3-9100, i5-9400, i7-9700, I9-9900, etc
(See next page for CPU list)

	
	Graphics card
	6th generation: Intel® HD Graphics 530 graphics controller, supporting single display, dual display expansion, and dual display replication
7th generation: Intel® HD Graphics 630 graphics controller, supporting single display, dual display expansion, and dual display replication
8th and 9th generations: Intel® UHD Graphics 630 graphics controller, supporting single display, dual display expansion, and dual display replication

	
	Memory 
	2*NB-DDR4,support 2133/2400/2666MHz memory, maximum support 64G

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface,default RS232;

	
	USB
	4*USB2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V10A or 19V6A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI®1.4 interface (4096/3840*2160@30Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Realtek 8111H Gigabit Network Card;
Dual Gigabit Network Card: Realtek 8111H+Realtek 8111H Gigabit Network Card;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.1 Gen1 interface
2*USB2.0 interface (Dual network host does not have thid interface)

	
	Audio
	1*LINE_OUT interface,audio output;
1*MIC_IN interface,microphone input;

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface, default RS232; COM1 can optionally support RS232/RS422/RS485

	Storage
	MSATA
	1*MSATA slot, support MSATA disks

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot,support PCIE3.0 x1 & USB signal,support WiFi Bluetooth/4G modules

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	6th and 7th generation :Supports Windows 11, Windows 10, Windows 8, Windows 7, Linux, etc
8th and 9th generation :Supports Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The following CPU information is for reference only. Please consult sales for specific requirements!
	CPU
	CPU brand
	CPU model
	Main frequency
	Turbo 
	TDP power consumption(W)

	6th gen I3
	Intel Core
	6100
	2 core 3.7G
	
	65

	
	
	6300
	2 core 3.8G
	
	65

	
	
	6320
	2 core 3.9G
	
	65

	6th gen I5
	Intel Core
	6400
	4 core 2.7G
	3.3G
	65

	
	
	6500
	4 core 3.2G
	3.6G
	65

	
	
	6600
	4 core 3.3G
	3.9G
	65

	6th gen I7
	Intel Core
	6700
	4 core 3.4G
	4.0G
	65

	7th gen I3
	Intel Core
	7100
	2 core 3.9G
	
	65

	
	
	7300
	2 core 4.0G
	
	65

	
	
	7320
	2 core 4.1G
	
	65

	7th gen I5
	Intel Core
	7400
	4 core 3.0G
	3.5G
	65

	
	
	7500
	4 core 3.4G
	3.8G
	65

	
	
	7600
	4 core 3.5G
	4.,1G
	65

	7th gen I7
	Intel Core
	7700
	4 core 3.6G
	4.2G
	65

	8th gen I3
	Intel Core
	8100
	4 core 3.6G
	
	65

	
	
	8300
	4 core 3.7G
	
	65

	8th gen I5
	Intel Core
	8400
	6 core 2.8G
	4.0G
	65

	
	
	8500
	6 core 3.0G
	4.1G
	65

	
	
	8600
	6 core 3.2G
	4.3G
	65

	8th gen I7
	Intel Core
	8700
	6 core 3.2G
	4.6G
	65

	9th gen I3
	Intel Core
	9100
	4 core 3.6G
	4.2G
	65

	
	
	9300
	4 core 3.7G
	4.2G
	65

	9th gen I5
	Intel Core
	9400
	6 core 2.9G
	4.1G
	65

	
	
	9500
	6 core 3.0G
	4.4G
	65

	
	
	9600
	6 core 3.1G
	4.6G
	65

	9th gen I7
	Intel Core
	9700
	8 core 3.0G
	4.7G
	65

	9th gen I9
	Intel Core
	9900
	8 core 3.1G
	5.0G
	65



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 30Hz;
 Optional 
4K 60Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*MSATA
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc29684] IPC6900-QM5100 series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM5100

	Motherboard
	CPU
	Support Intel ® Comet lake 10th generation LGA1200 Core i3-10100, i5-10400, i7-10700, i9-10900, etc
Support Intel ® Rocket Lake 11th generation LGA1200 Core i5-11400, i7-11700, i9-11900, etc
(See next page for CPU list)

	
	Graphics card
	10th generation: Intel ® HD Graphics 630 ultra core graphics card, supporting single display, dual display replication, and dual display expansion;
11th generation: Intel ® HD Graphic 730/750 ultra core graphics card, supporting single display, dual display replication, and dual display expansion;

	
	Memory
	2*NB-DDR4,support 2133/2400/2666/2933MHz memory, maximum support 64G

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface,default RS232;

	
	USB
	4*USB2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V10A or 19V6A and above power supply;
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI ® interface
When the CPU is 11th generation i5/i7/i9, the motherboard HDMI ® Supports 4096/3840*2160@60Hz;
When the CPU is 10th generation i3/i5/i7/i9, the motherboard HDMI ® Supports 4096/3840*2160@30Hz;
1 *VGA interface (1920)*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840)*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Realtek 8111H Gigabit Network Card, optional support for Motorcomm YT6801 Gigabit Network Card;
Dual Gigabit Network Card: Realtek 8111H+Realtek 8111H Gigabit Network Card, optional support for Motorcomm YT6801+Motorcomm YT6801 Gigabit Network Card;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (Dual network host does not have this interface)

	
	Audio
	1*LINE_OUT interface,audio output;
1*MIC_IN interface,microphone input;

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface, default RS232; Optional support for 2 * RS232/RS422/RS485

	Storage
	MSATA
	1*MSATA slot, support MSATA disks

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot,support PCIE3.0 x1 & USB signals, support WiFi Bluetooth/4G modules

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity ,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Supports Windows 11, Windows 10, Linux, etc



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The following CPU information is for reference only. Please consult sales for specific requirements!

	CPU
	CPU brand
	CPU model
	Main frequency
	Turbo 
	TDP power consumption(W)

	10th gen I3
	Intel Core
	10100
	4 core 3.6G
	4.3G
	65 

	
	
	10105
	4 core 3.7G
	4.4G
	65 

	
	
	10300
	4 core 3.7G
	4.4G
	65

	
	
	10305
	4 core 3.8G
	4.5G
	65 

	
	
	10320
	4 core 3.8G
	4.6G
	65 

	
	
	10325
	4 core 3.9G
	4.7G
	65 

	10th gen I5
	Intel Core
	10400
	6 core 2.9G
	4.3G
	65 

	
	
	10505
	6 core 3.2G
	4.6G
	65 

	
	
	10500
	6 core 3.1G
	4.5G
	65 

	
	
	10600
	6 core 3.3G
	4.8G
	65 

	10th gen I7
	Intel Core
	10700
	8 core 2.9G
	4.8G
	65 

	10th gen I9
	Intel Core
	10900
	10 core 2.8G
	5.2G
	65 

	11th gen I5
	Intel Core
	11400
	6 core 2.6G
	4.4G
	65

	
	
	11500
	6 core 2.7G
	4.6G
	65

	
	
	11600
	6 core 2.8G
	4.8G
	65 

	11th gen I7
	Intel Core
	11700
	8 core 2.5G
	4.9G
	65

	11th gen I9
	Intel Core
	11900
	8 core 2.5G
	5.2G
	65



※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	
	
	2
	4
	
	
	
	
	

	

	PC model
	[bookmark: _Toc22040]IPC6900-QM6100 series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM6100

	Motherboard
	CPU
	Support Intel ® Alder Lake 12th generation LGA 1700 Core i3-12100, i5-12400, i7-12700, i9-12900, etc
Support Intel ® Raptor Lake 13th generation LGA 1700 Core i3-13100, i5-13400, i7-13400, i9-13900, etc
Support Intel ® Raptor Lake 14th generation LGA 1700 Core i3-14100, i5-14400, i7-14700, i9-14900, etc
(See next page for CPU list)

	
	Graphics card
	Intel ® UHD Graphics 730/770 graphics controller, supporting single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4 supports 2133/2400/2666/2933/320MHz memory, with a maximum support of 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface,default RS232;

	
	USB
	4*USB2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V10A or 19V6A and above power supply;
1*4Pin Phoenix terminal optional, customizable wire sequence;

	
	Display port
	1*HDMI®2.0 interface (4096/3840*2160@60Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Intel ® I219V Gigabit Ethernet card;
Dual Gigabit Network Card: Intel ® I219V+Realtek 8111H Gigabit Ethernet Card;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (Dual network host does not have this interface)

	
	Audio
	1*LINE_OUT interface,audio output
1*MIC_IN interface,microphone input

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface, default RS232; COM1 can optionally support RS232/RS422/RS485

	Storage
	M.2_SSD
	1*M.2 Key-M slot, supports M.2 2280 NVME PCIE3.0 x4 protocol, can be changed to support SATA protocol; Optional M.2 2242 hard drive;

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	Expansion 
	Mini-PCIE
	1*Mini-PCIE slot, supports PCIE 3.0 x1&USB signals, supports WiFi Bluetooth/4G modules;

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Supports Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
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	HDMI®
	VGA/DP
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA 2K 60Hz;
Optional 
DP 4K 60Hz
	1
	6
	2
	2/6
	1*M.2
1*SATA
	2*NB-DDR4
MAX 64G
	12V/19V

	

	PC model
	[bookmark: _Toc23504]IPC6900-QM6300 series

	PC size
	220mm(L)*210mm(W)*80mm(H)

	Cooling system
	Fanless+integrated heat dissipation with chassis

	Color 
	Black

	Adapt to motherboard
	QM6300

	Motherboard
	CPU
	Support Intel ® Alder Lake 12th generation LGA 1700 Core i3-12100, i5-12400, i7-12700, i9-12900, etc
Support Intel ® Raptor Lake 13th generation LGA 1700 Core i3-13100, i5-13400, i7-13400, i9-13900, etc
Support Intel ® Raptor Lake 14th generation LGA 1700 Core i3-14100, i5-14400, i7-14700, i9-14900, etc
(See next page for CPU list)

	
	Graphics card
	Intel ® UHD Graphics 730/770 graphics controller, supporting single display, dual display replication, and dual display expansion

	
	Memory
	2*NB-DDR4 supports 2133/2400/2666/2933/320MHz memory, maximum support of 64GB

	Front panel interface
	POWER
	1*Switch button

	
	COM
	4*COM interface, default RS232;

	
	USB
	4*USB 2.0 interface

	Rear panel interface
	Power port
	1*DC power interface (5.5*2.5mm), recommended 12V10A or 19V6A and above power supply
1*4Pin Phoenix terminal optional, customizable wire sequence

	
	Display port
	1*HDMI®2.0 interface (4096/3840*2160@60Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*DP 1.4 interface (4096/3840*2160@60Hz)

	
	LAN
	Single Gigabit Network Card: Realtek 8111H Gigabit Network Card;
Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface
2*USB2.0 interface (Dual network host does not have this interface)

	
	Audio
	1*LINE-OUT interface: audio output
1*MIC-IN interface: microphone input

	
	WiFi
	2*WiFi antenna interface

	
	COM
	2*COM interface, default RS232; COM1 can optionally support RS232/RS422/RS485

	Storage
	M.2_SSD
	1*M.2 Key-M slot, supporting M.2 2280 NVME PCIE3.0 x4/SATA adaptive standard SSD;

	
	SATA
	1*SATA3.0 hard drive interface, support 2.5-inch SSD/HDD hard drives or 3.5-inch HDD hard drives

	Expansion 
	M.2_WiFi
	1*M.2 Key-E slot, supports M.2 2230 PCIE3.0 x1&USB signal, supports WiFi Bluetooth module;

	Operating environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Supports Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※
[bookmark: _GoBack]
The following CPU information is for reference only. Please consult sales for specific requirements!


	CPU 
	CPU brand
	CPU model
	Main frequency
	Turbo 
	TDP power consumption(W)
	Maximum turbo power consumption of CPU (W)

	12th gen I3
	Intel Core
	12100
	4 core 3.3G
	4.3G
	60
	89

	
	
	12300
	4 core 3.5G
	4.4G
	60
	89

	12th gen I5
	Intel Core
	12400
	6 core 2.5G
	4.4G
	65
	117

	
	
	12500
	6 core 3.0G
	4.6G
	65
	117

	
	
	12600
	6 core 3.3G
	4.8G
	65 
	117

	12th gen I7
	Intel Core
	12700
	12 core 2.1G
	4.9G
	65
	180

	12th gen I9
	Intel Core
	12900
	16 core 2.4G
	5.1G
	65
	202

	13th gen I3
	Intel Core
	13100
	4 core 3.4G
	4.5G
	60
	89

	13th gen I5
	Intel Core
	13400
	10 core2.5G
	4.6G
	65
	154

	
	
	13500
	14 core 2.5G
	4.8G
	65
	154

	
	
	13600
	14 core 2.7G
	5.3G
	65
	154

	13th gen I7
	Intel Core
	13700
	16 core 2.1G
	5.2G
	65
	219

	13th gen I9
	Intel Core
	13900
	44 core 2.3G
	5.6G
	65
	219

	14th gen I3
	Intel Core
	14100
	4 core 3.5GHz
	4.7G
	60
	154

	14th gen I5
	Intel Core
	14400
	10 core 2.5GHz
	4.7G
	65
	219

	
	
	14500
	14 core 2.6GHz
	5.0G
	65
	219

	
	
	14600
	14 core 2.7GHz
	5.2G
	65
	219

	14th gen I7
	Intel Core
	14700
	20 core 2.1GHz
	5.4G
	65
	219

	14th gen I9
	Intel Core
	14900
	24 core 2.0GHz
	5.8G
	65
	219
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