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PC size
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Single network interface diagram
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Dual network interface diagram
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The pictures are for reference only, please refer to the actual product!
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	PC model
	CPU
	4K
	LAN
	COM
	USB2.0
	USB3.0
	SSD
	Memory
	Power

	NANO19
	J1800
J1900
J2900
Optional
	/
	1
	2
	3
	1
	1*MSATA
1*SATA2.0
	1*NB-DDR3
MAX 8GB
	+12V

	
	
	
	2
	2
	1
	1
	
	
	



Important Tips:
1. The PC power supply only supports 12V, and the full load is about 30W. It is recommended to use a 12V4A or above power supply;
2. PC VGA, HDMI support single display, dual display copy, dual display expansion, single display under DOS;
3. The blue USB port on the PC has USB 3.0 at the bottom and USB 2.0 at the top . The black USB port is USB 2.0.
4. The PC MSATA interface defaults to coexisting SATA signals and USB signals, and supports MSATA hard disks or WiFi modules with USB signals by default;
SATA signal can be changed to PCIE signal, and after the change, it can support PCIE signal WiFi module;
5. The PC Mini-PCIE interface defaults to coexisting PCIE signals and USB signals, and supports WiFi/3G/4G/Bluetooth WiFi modules by default;
6. All USB ports on the PC are S-type (no power after shutdown) and cannot be changed to A-type (power after shutdown);
7. The mainboard COM port supports RS232 by default; COM2 can select RS232/RS422/RS485, which is controlled by JP9/JP10/JP11 jumper caps;
8. The ninth pin of the motherboard COM1/2 can be set to 5V/12V through JCOM1/2, the default is 0V;
9. The PC supports 100M and 1000M network cards; single and dual network ports are optional; POE power supply cannot be changed;

Product Specifications
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	NANO19

	PC size
	136 mm ( L ) *1 27 mm ( W ) * 47 mm ( H )

	CPU Processor
	Intel® Processor Celeron J1800, Celeron J1900, Pentium J2900

	Memory support
	1*DDR3 SODIMM memory slot, supports 1600MHz memory, low voltage 1.35V, maximum support 8GB

	Power supply
	1*DC_IN
	Supports 12V voltage, the inner diameter of the DC head is 2.5MM
The motherboard consumes about 30W when fully loaded. It is recommended to use a 12V4A or higher power supply

	Display functions
	Intel HD Graphics graphics controller , supports single display, dual display copy, dual display expansion, single display under DOS

	
	1*HDMI 1.4 interface
	Support resolution 1920*1080@60HZ

	
	1*VGA DB15 interface
	Support resolution 1920*1080@60HZ

	Network Features
	1/2*RJ45 LAN interface
	Realtek 8105E 100M and 8111 F 1000M network cards are optional, supporting network wake-up and PXE diskless boot functions

	
	1*Mini-PCIE interface
	Support WIFI/3G/4G/Bluetooth WiFi module

	Hard disk function
	1*MSATA interface
	Support MSATA disk, support SATA 2.0 

	
	1*SATA1 interface
	Standard SATA2.0 hard disk interface

	
	1*SATA_PWR1 pin
	Hard disk power supply pin, can take 5V, 12V power. (4Pin, 1*4Pin, 2.54mm)

	Sound Features
	1*LIN_OUT interface
	Support audio output (green)

	
	1*MIC_IN interface
	Support microphone input (red)

	USB Function
	1*USB3.0 interface
	Rear standard USB3.0 interface

	
	3*USB2.0 interface
	Rear standard USB2.0 interface

	Switch function
	1* POWER button
	Switch button

	Other I/O
	1*SIM_CARD slot
	Support SIM card, SIM card is required when using 3G/4G

	Operating Environment
	Working temperature: -20℃~60℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS, supports power-on, scheduled power-on, remote power on and off, and intelligent device identification

	Watch Dog
	Watchdog programming, support hardware reset function (256 levels, 0~255 seconds)

	Operating system
	Support Windows 10, Windows 8, Windows7, Linux, etc.
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CPU Information
	CPU Specifications
	CPU Brand
	CPU Model
	Frequency
	Turbo
	CPU power consumption (W)

	
	Intel Celeron
	J1800
	Dual core 2.41G
	2.58G
	10W

	
	Intel Celeron
	J1900
	Quad-core 1.99G
	2.41G
	10W

	
	Intel Pentium
	J2900
	Quad-core 2.41G
	2.66G
	10W
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