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ELSKY NANO1F Mini PC Specification
――――――――――――――――――――――――――――――――――――――――――――――――――――――

PC size diagram
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――――――――――――――――――――――――――――――――――――――――――――――――――――――

Front panel interface
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――――――――――――――――――――――――――――――――――――――――――――――――――――――

Rear panel dual network interface
[image: image3.jpg]= \ ‘,‘[ | | : '1;—“

- ‘e ‘W

| )
R
4.

\.

D





――――――――――――――――――――――――――――――――――――――――――――――――――――――

Rear panel single network interface
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――――――――――――――――――――――――――――――――――――――――――――――――――――――

Rear panel dual HDMI interface(optional)
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――――――――――――――――――――――――――――――――――――――――――――――――――――――
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――――――――――――――――――――――――――――――――――――――――――――――――――――――

Bottom of PC diagram
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――――――――――――――――――――――――――――――――――――――――――――――――――――――

The pictures are for reference only, please refer to the actual product!

	HDMI
	VGA/HDMI
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	VGA:2K
HDMI:4K 60Hz
	1
	6
	2
	2
	1*M.2
	1*NB-DDR4

MAX 16G
	12V~24Vwide voltage

	
	
	2
	4
	2
	
	
	
	

	

	PC model
	NANO1F

	PC size
	136mm(L)*126mm(W)*45mm(H)

	Cooling system
	Equipped with heat dissipation holes, silent fan for heat dissipation or integrated heat dissipation without fan and chassis;

	Color 
	Black

	Adapt to motherboard
	NANO1F

	Motherboard 
	CPU
	Supports Intel Alder Lake-N series N200, N100, N97, N95, i3-N305, etc

	
	Graphics card
	Intel UHD Graphics, supports single display, dual display replication, and dual display expansion

	
	Memory 
	1*NB-DDR4 SODIMM memory slot, supports 3200MHz memory, maximum support 16GB

	Front panel interface
	POWER
	1*switch button

	
	USB
	2*USB2.0 interface
2*UBS3.2 Gen1 interface

	
	COM
	2*COM,default support for RS232, with COM1 optional support for RS232/RS422/RS485

	Rear panel interface
	Power supply
	1*DC power interface, supports 12V~24V wide voltage power supply, recommended 12V/4A or 24V2A or above power supply

	
	Display 
	1*HDMI1 2.0 interface (4096/3840*2160@60Hz)
1*VGA interface (1920*1080@60Hz)
Optional 1*HDMI2 2.0 interface (4096/3840*2160@60Hz)

	
	LAN
	1*LAN: Default support for Realtek 8111H Gigabit Ethernet card; Optional domestic Motorcomm YT6801 Gigabit Ethernet card;

2*LAN: Supports Realtek 8111H+Realtek 8111H Gigabit Ethernet cards;

Optional domestic Motorcomm YT6801+Motorcomm YT6801 gigabit network card;

Support network wake-up and PXE diskless boot function

	
	USB
	4*USB2.0 interface (Dual network PC supports 2*USB)

	
	Audio 
	1*LINE-OUT interface, audio output

1*MIC-IN interface, microphone input

	
	WiFi
	2*WiFi antenna interface

	Storage
	M.2_SSD
	1*M.2 Key-M slot, supports M.2 2280 hard drive, default SATA protocol, optional NVME (PCIE) protocol

	Expansion
	M.2_WiFi
	1*M.2 Key-E slot, supports M.2 2230 WiFi Bluetooth module

	Environment 
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500Hz/random/operating

	BIOS
	AMI BIOS,Support power on, timed power on, and intelligent recognition of remote power on/off devices

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Supports Windows 11, Windows 10, Linux, etc

(N100 and i3-N300 support Windows 10, Windows 11 22H2 and above versions)


The following CPU information is for reference only. Please consult sales for specific requirements!
	CPU brand
	CPU model
	Main frequency
	Maximum turbo
	CPU power consumption
	The full load power consumption

	Intel core
	i3-N300
	Eight core 0.8G
	3.80G
	7W
	20W

	
	i3-N305
	Eight core 1.8G
	3.80G
	15W
	40W

	Intel 
	N50
	
	3.40G
	6W
	20W

	
	N95
	Quad core 1.7G
	3.40G
	15W
	40W

	
	N97
	Quad core 2.0G
	3.60G
	12W
	35W

	
	N100
	Quad core 0.8G
	3.40G
	6W
	20W

	
	N200
	Quad core 1.0G
	3.70G
	6W
	20W


Explanation
Except for the accessories listed with the product configuration, the content contained in this manual does not represent our company's commitment. Our company reserves the right to make changes to this manual without further notice.

We are not responsible for any direct, indirect, intentional or unintentional damage or hidden dangers caused by improper installation or use.

Before ordering the product, please inquire with the distributor in detail about whether the product performance meets your needs.

The content of this manual is protected by copyright, and all rights reserved. Without permission, it may not be copied in any mechanical, electronic, or other way.

The final right of interpretation of this manual belongs to SHENZHEN ELSKY TECHNOLOGY CO.,LTD.

The above ordering information is for reference only. For details, please consult the sales department at 0755-82260150

Motherboard driver download https://pan.baidu.com/s/1ie7qi5NutS53ipPecRSYtw
Access password cbn5
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