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The motherboard picture is for reference only, please refer to the actual product!

Model：

	Model 
	CPU
	4K
	LAN
	USB3.0
	USB2.0
	Type_C

3.0
	Memory（MAX）
	SSD
	Power

	NUC600
	3855U,

3955U,

Skylake 6th gen
i3,i5,i7
	1*HDMI

4K 30Hz
1*MINI-DP
4K 60Hz

	1
	3
	2
	1
	2*NB-DDR4

Max support 64G
	1*M.2 2260
1*SATA
	+12V

	NUC700
	3865U,

3965U,

Kabylake 7th gen
i3,i5,i7
	
	1
	3
	2
	1
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Important tips：

Power supply interface:

The motherboard DC interface specification is 5.5*2.5, and can be changed to 4Pin DC_ATX interface power supply;

The motherboard power supply only supports 12V, about 40W at full load, and it is recommended to use a 12V5A or above power supply;

Display interface:

1. The motherboard HDMI and MINI-DP support single display, dual display copy, dual display expansion, and single display under DOS;

2. The motherboard HDMI interface supports 4K resolution 4096/3840*2160@30Hz;

3. The motherboard MINI-DP supports 4K resolution 4096/3840*2160@60Hz;

4. The motherboard MINI-DP interface must use an active MINI-DP to HDMI cable to connect the MINI-DP to HDMI cable, otherwise there will be no display; it can be used directly when connected to the MINI-DP to DP cable;

M.2 interface:

The motherboard NGFF (M.2) supports Key-M interface M.2 2260 hard disk, supports automatic switching between SATA protocol and NVME (PCIE) protocol;

M2_WIFI on the motherboard supports Key-E interface M.2 2230 WiF module, and supports WiFi/Bluetooth module by default;

USB interface:

The motherboard supports 3*USB3.0; 2*USB2.0; 1*Type C:3.0 interface by default, which can connect USB devices;

The external USB interface and built-in USB pin of the motherboard default to S power (no power after shutdown), among which the external USB interface cannot be changed to A power (powered after shutdown), and the built-in pin can be changed to A power;

Network card:

The motherboard supports Intel i219V single Gigabit network card, dual network cannot be changed, and POE power supply cannot be changed;

Sound card:

The motherboard sound card supports Realtek ALC897 sound card; the motherboard audio interface supports audio output and MIC input;

CPU details

	CPU
	CPU brand
	CPU model
	Frequency
	Turbo
	CPU Power consumption(W)
	Full load power consumption (W)

	6th gen
	Celeron 
	3855U
	2 core 1.6G
	
	15
	40

	
	
	3955U
	2 core 2.0G
	
	15
	40

	6th gen I3
	Core
	6006U
	2 core 2.0G
	
	15
	40

	
	
	6100U
	2 core 2.3G
	
	15
	40

	
	
	6157U
	2 core 2.4G
	
	28
	60

	
	
	6167U
	2 core 2.7G
	
	28
	60

	6th gen I5
	Core
	6200U
	2 core 2.3G
	2.8G
	15
	40

	
	
	6260U
	2 core 1.8G
	2.9G
	15
	40

	
	
	6267U
	2 core 2.9G
	3.3G
	28
	60

	
	
	6287U
	2 core 3.1G
	3.5G
	28
	60

	
	
	6300U
	2 core 2.4G
	3.0G
	15
	40

	
	
	6360U
	2 core 2.0G
	3.1G
	15
	40

	6th gen I7
	Core
	6500U
	2 core 2.5G
	3.1G
	15
	40

	
	
	6560U
	2 core 2.2G
	3.2G
	15
	40

	
	
	6567U
	2 core 3.3G
	3.6G
	28
	60

	
	
	6600U
	2 core 2.6G
	3.4G
	15
	40

	
	
	6650U
	2 core 2.2G
	3.4G
	15
	40

	
	
	6660U
	2 core 2.4G
	3.4G
	15
	40

	7th gen
	Celeron 
	3865U
	2 core 1.8G
	
	15
	40

	
	
	3965U
	2 core 2.2G
	
	15
	40

	7th gen I3
	Core
	7020U
	2 core 2.3G
	
	15
	40

	
	
	7100U
	2 core 2.4G
	
	15
	40

	
	
	7130U
	2 core 2.7G
	
	15
	40

	7th gen  I5
	Core
	7200U
	2 core 2.5G
	3.1G
	15
	40

	
	
	7260U
	2 core 2.2G
	3.4G
	15
	40

	
	
	7267U
	2 core 3.1G
	3.5G
	28
	60

	
	
	7287U
	2 core 3.3G
	3.7G
	28
	60

	
	
	7300U
	2 core 2.6G
	3.5G
	15
	40

	
	
	7360U
	2 core 2.3G
	3.6G
	15
	40

	7th gen I7
	Core
	7500U
	2 core 2.7G
	3.5G
	15
	40

	
	
	7560U
	2 core 2.4G
	3.8G
	15
	40

	
	
	7567U
	2 core 3.5G
	4.0G
	28
	60

	
	
	7600U
	2 core 2.8G
	3.9G
	15
	40

	
	
	7660U
	2 core 2.5G
	4.0G
	15
	40


illustrate
Except for the accessories listed with the product, the contents of this manual do not represent the company's commitment. The company reserves the right to change this manual without further notice.

We are not responsible for any direct, indirect, intentional or unintentional damage and hidden dangers caused by improper installation and use.

Before ordering the product, please ask the dealer for details on whether the product performance meets your needs.

The contents of this manual are protected by copyright and all rights are reserved. Without permission, it shall not be reproduced mechanically, electronically or in any other way.

The final right of interpretation of this manual belongs to SHENZHEN ELSKY TECHNOLOGY CO.,LTD.
BIOS Function key

	BIOS Function key
	Function description

	Press Delete on startup
	The BIOS function screen is displayed

	Press F11 to start
	Select the boot option or access the BIOS function screen

	← →
	Move the left and right arrows to select an entry

	↑ ↓
	Move the up and down arrows to select the entry

	Enter
	Select the item and go to the submenu

	+/-
	Change the selection, or add or subtract values

	F1
	The help content is displayed

	F9
	factory data reset

	F10
	Save the changes and exit

	Esc
	quit


Motherboard Specifications
	Size 
	100mm（L）*100mm（W）*30mm（H）

	CPU
	NUC600
	3855U、3955U and Skylake i3-6100U、i5-6200U、i7-6500U etc

	
	NUC700
	3865U、3965U and Kabylake i3-7100U、i5-7200U、i7-7500U etc

	Chipset
	Integrated in CPU single chip

	Power adapter
	1*DC_IN

(optional 4Pin ATX）
	The inner diameter of the DC head is 2.5MM, and it only supports 12V power supply.

Mainboard power consumption: about 40W. It is recommended to use a 12V5A or higher power supply.

	Memory 
	2*NB-DDR4 Support 2133/2400MHz memory, maximum support 64G

	Display function
	NUC600
	Intel HD510/520 Graphics Controller
	Support single display, dual display copy, dual display expansion, single display under DOS

	
	NUC700
	Intel HD610/620 Graphics Controller
	

	
	1*MINI-DP port
	Supports 4K resolution 4096/3840*2160@60Hz

	
	1*HDMI 1.4 port
	Supports 4K resolution 4096/3840*2160@30Hz

	Network function
	1*LAN port
	Intel i219V Gigabit LAN, supports network wake-up, PXE function

	
	1*M2_WIFI port
	PCIE 3.0 signal, supports Key-E interface M.2 2230 WiFi module, can be changed to support WiFi Bluetooth module

	Hard disk function
	1*NGFF port
	PCIE3.0 signal, supports Key-M interface M.2 2260 hard disk;

Default supports automatic switching between NVME (PCIE) protocol and SATA protocol.

	
	1*SATA1 port
	Standard SATA3.0 hard disk interface, maximum transmission speed 6.0 Gbps.

	
	1*SATA_PWR1 pin
	The hard disk power supply pin can take 5V or 12V power.               

（4Pin，1*4Pin，2.54mm）

	Sound function
	Supports integrated Realtek ALC897HD digital audio decoder, 6-channel high-fidelity audio controller

	
	1*LINE_OUT port
	Support audio output and MIC input

	
	The mainboard HDMI interface supports HDMI display audio output

	
	The mainboard MINI-DP interface supports DP monitor audio output

	USB function
	3*USB3.0 port
	Rear standard USB3.0 interface

	
	1*Type C 3.0 port
	Standard Type C: 3.0 interface, can connect USB devices

	
	1*F_USB1 pin
	Front USB2.0 pin, one set has 2*USB2.0             （9Pin，2*5Pin，2.0mm）

	Switch function
	1*F_PANEL pin
	Switch, power light, hard disk light, restart pin      （9Pin，2*5Pin，2.0mm）

	
	1*IR
	Infrared, supports wireless data transmission

	Other I/O
	1*CPU_FAN
	CPU fan pin, supports temperature control         （3Pin，1*3Pin，1.25mm）

	Operating Environment
	Working temperature: -10℃~60℃; 

Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS，Support power-on, scheduled power-on, remote power on and off, and intelligent device identification

	Watch Dog
	Watchdog programming, support hardware reset function (256 levels, 0~255 seconds)

	OS
	Support Windows 10，Windows 8，Windows 7，Linux etc.
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