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2C motherboard picture
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The motherboard picture is for reference only, please refer to the actual product!

Product model ordering options:
	Motherboard model
	CPU
	4K
	LAN
	COM
	USB
	SSD
	Memory
	Power

	QM9400-2C
	Haswell-U 4th Generation
	support
	1
	2
	8
	1*MSATA
2*SATA 3.0
	
1*NB DDR3
8GB MAX

	The 2C motherboard only supports 12V;
6C motherboard supports 12V/19V

	QM9400-2L2C
	
	
	2
	2
	6
	
	
	

	QM9400-6C
	
	
	1
	6
	8
	
	
	

	QM9400-2L6C
	
	
	2
	6
	6
	
	
	

	QM9500-2C
	Broadwell-U 5th Generation
	support
	1
	2
	8
	
	
	

	QM9500-2L2C
	
	
	2
	2
	6
	
	
	

	QM9500-6C
	
	
	1
	6
	8
	
	
	

	QM9500-2L6C
	
	
	2
	6
	6
	
	
	

	




Important Tips:
1) 2C motherboard only supports 12V; 6C motherboard supports 12V/19V;
2) The motherboard does not have GPIO pins by default. If you need to use them, you need to change the board and declare it in advance;
3) The motherboard VGA, HDMI, and LVDS support single display, dual display/triple display copy, dual display/triple display expansion, and single display under DOS;
4) The motherboard HDMI interface supports 4K resolution 4096/3840*2160@30Hz; Windows 10 system is required to run 4K video;
5) The motherboard supports 2*COM and 6*COM optional, and supports RS232 by default;
6) Motherboard COM2 supports RS232/422/485 optional, through JP9/JP10/JP11 jumper settings;
7) The 9th pin of COM1/2 on the Motherboard can be set to 0V/5V/12V through JCOM1/2;
8) The motherboard Mini-PCIE supports PCIE signals and USB signals by default.
9) MSATA supports SATA signal and USB signal by default, and supports dual WIFI by default;
10) The motherboard supports single Gigabit network card by default, and can optionally support dual Gigabit network cards;



Illustrate

Except for the accessories listed with the product, the contents of this manual do not represent the company's commitment. The company reserves the right to change this manual without further notice.
We are not responsible for any direct, indirect, intentional or unintentional damages and hidden dangers caused by improper installation or use.
Before ordering a product, please consult your dealer to learn in detail whether the product performance meets your needs.
The contents of this manual are protected by copyright. All rights reserved. No reproduction in mechanical, electronic or other ways is allowed without permission.
The final right of interpretation of this manual belongs to SHENZHEN ELSKY TECHNOLOGY CO.,LTD.

The above ordering information is for reference only. For details, please consult the sales department at 0755-82260150
Motherboard driver download https://pan.baidu.com/s/1ie7qi5NutS53ipPecRSYtw 
Access password cbn5


The following CPU information is for reference only. Please consult sales for specific needs!
	CPU Specifications
	CPU Brand
	CPU Model
	Frequency
	Turbo
	CPU power consumption (W)

	4th Generation I3
	Intel
Core
	4005U
	Dual-core 1.7G
	
	15

	
	
	4010U
	Dual-core 1.7G
	
	15

	
	
	4025U
	Dual core 1.9G
	
	15

	
	
	4030U
	Dual core 1.9G
	
	15

	
	
	4100U
	Dual core 1.8G
	
	15

	4th generation I5
	Intel
Core
	4200U
	Dual core 1.6G
	2.6G
	15

	
	
	4210U
	Dual-core 1.7G
	2.7G
	15

	
	
	4250U
	Dual core 1.3G
	2.6G
	15

	
	
	4278U
	Dual core 2.6G
	3.1G
	28

	
	
	4300U
	Dual core 1.9G
	2.9G
	15

	
	
	4308U
	Dual core 2.8G
	3.3G
	28

	
	
	4310U
	Dual-core 2.0G
	3.0G
	15

	4th Generation I7
	Intel
Core
	4500U
	Dual core 1.8G
	3.0G
	15

	
	
	4510U
	Dual-core 2.0G
	3.1G
	15

	
	
	4550U
	Dual-core 1.5G
	3.0G
	15

	
	
	4558U
	Dual core 2.8G
	3.3G
	15

	
	
	4578U
	Dual-core 3.0G
	3.5G
	28

	
	
	4600U
	Dual core 2.1G
	3.3G
	15

	
	
	4650U
	Dual-core 1.7G
	3.0G
	15

	5th Generation I3
	Intel
Core
	5005U
	Dual-core 2.0G
	
	15

	
	
	5010U
	Dual core 2.1G
	
	15

	
	
	5015U
	Dual core 2.1G
	
	15

	
	
	5020U
	Dual core 2.2G
	
	15

	5th Generation I5
	Intel
Core
	5200U
	Dual core 2.2G
	2.7G
	15

	
	
	5250U
	Dual core 1.6G
	2.7G
	15

	
	
	5257U
	Dual-core 2.7G
	3.1G
	15

	
	
	5287U
	Dual-core 2.9G
	3.3G
	28

	
	
	5300U
	Dual core 2.3G
	2.9G
	15

	
	
	5350U
	Dual core 1.8G
	2.9G
	15

	5th Generation I7
	Intel
Core
	5500U
	Dual-core 2.4G
	3.0G
	15

	
	
	5550U
	Dual-core 2.0G
	3.0G
	15

	
	
	5557U
	Dual-core 3.1G
	3.4G
	28

	
	
	5600U
	Dual core 2.6G
	3.2G
	15

	
	
	5650U
	Dual core 2.2G
	3.1G
	15





[bookmark: _Toc26498][bookmark: _Toc19535][bookmark: _Toc20111][bookmark: _Toc28637][bookmark: _Toc13634][bookmark: _Toc16549][bookmark: _Toc4711][bookmark: _Toc10704][bookmark: _Toc11966]Chapter 1. Product Specifications
	Motherboard size
	170mm(L)*170mm(W)*20mm(H)

	CPU Processor
	QM9400 supports 4 generations of CPU: I3-4010U, I5-4200U, I7-4500U, etc.

	
	QM9500 supports 5 generations of CPU: I3-5010U, I5-5200U, I7-5500U, etc.

	Chipset
	Haswell-U, Broadwell-U Express Chipset

	Memory support
	1*DDR3 SODIMM memory slot, supports 1600MHz memory , low voltage 1.35V , maximum support 8GB

	Power supply
	1*DC_IN
	Supports 12V/19V voltage, the inner diameter of the DC head is 2.5MM
Motherboard power consumption: about 30W. It is recommended to use a 12V5A or higher power supply

	
	1*DC_ATX
	

	Display functions
	4th generation integrated Intel® HD 4400 graphics controller , supports single display, dual display / triple display copy, dual display / triple display expansion, single display under DOS

	
	5th generation integrated Intel® HD 5500 graphics controller , supports single display, dual display / triple display copy, dual display / triple display expansion, single display in DOS

	
	1*VGA DB15 interface
	Support resolution 1920*1080@60HZ

	
	1*VGA_OUT pin
	Support resolution 1920*1080@60HZ (12Pin, 1*12Pin, 2.0mm)

	
	1*HDMI 1.4 interface
	Support resolution 4096/3840*2160@30HZ

	
	1*HDMI_CON pin
	Support resolution 4096/3840*2160@30HZ        (16Pin, 2*8Pin, 2.0mm)

	
	1*LVDS pin
	Support resolution 1920*1080@60HZ (30Pin, 2*15Pin, 2.0mm)

	
	1*VCC_SEL pin
	LVDS voltage control pin (6Pin, 2*3Pin, 2.0mm)

	
	1*INVERT pin
	LVDS backlight switch control pin (6Pin, 1*6Pin, 2.0mm)

	
	1*BKLT_CTRL pin
	LVDS backlight brightness adjustment pin (4Pin, 1*4Pin, 2.0mm)

	Network Features
	1*RJ45 LAN interface
	RTL8111 F Gigabit network card chip , supports network wake-up and PXE diskless boot functions .

	
	1*Mini-PCIE interface
	Support WIFI/3G/4G

	Hard disk function
	1*MSATA interface
	Support MSATA disk

	
	2*SATA interface
	Standard SATA3.0 hard disk interface, maximum transmission speed 6.0 Gbps

	
	2*SATA_PWR pin
	Hard disk power supply pin, can take 5V, 12V power. (4Pin, 1*4Pin, 2.54mm)

	Sound Features
	Integrated Realtek ALC662 HD digital audio decoder , 6-channel high-fidelity audio controller

	
	1*LIN_OUT interface
	Support audio output (green)

	
	1*MIC_IN interface
	Support microphone input (red)

	
	1*INT_SPK pin
	The amplifier supports 8 ohm 5 watt speaker dual channel output 
[bookmark: _GoBack](4Pin, 1*4Pin, 2.0mm)

	
	1*F_AUDIO pin
	Standard audio pin (9Pin, 2*5Pin, 2.54mm)

	USB Function
	2*USB3.0 interface
	Rear standard USB3.0 interface

	
	2*USB2.0 interface
	Rear standard USB2.0 interface

	
	1*F_USB2 pin
	Front USB2.0 pin, one set has 2*USB2.0 (9Pin, 2*5Pin, 2.54mm)

	
	1*F_USB3 pin
	Front USB2.0 pin, one set has 2*USB2.0 (9Pin, 2*5Pin, 2.54mm)

	Switch function
	1*F_PANEL pin
	Switch, power light, hard disk light, restart pin (9Pin, 2*5Pin, 2.54mm)

	
	1*AUTO_SW pin
	Hardware control power-on pin (3Pin, 1*3Pin, 2.0mm)

	Other I/O
	1*COM1 pin
	Serial port, only supports RS232 (9Pin, 2*5Pin, 2.54mm)

	
	1*COM2 pin
	Serial port, COM2 supports RS232/RS422/RS485 optional 
(9Pin, 2*5Pin, 2.54mm)

	
	1*JCOM1 pin
	Control COM1 pin 9 voltage 0V/5V/12V optional (6Pin, 2*3Pin, 2.0mm)

	
	1*JCOM2 pin
	Control COM2 pin 9 voltage 0V/5V/12V optional (6Pin, 2*3Pin, 2.0mm)

	
	JP9/JP10/JP11 pin
	COM2 supports RS422 and RS485 signal jumper settings 
(6Pin, 2*3Pin, 2.0mm)

	
	COM3~COM6 pins
	Serial port, supports standard RS232;  (39Pin, 2*20Pin, 2.0mm)

	
	1*MINI_PCIE interface
	Support WIFI/3G/4G/GPS/Bluetooth modules, etc.

	
	1*SIM_CARD slot
	Support SIM card, SIM card is required when using 3G/4G

	
	1*CLR_CMOS pin
	Motherboard reset and discharge pin (2Pin, 1*2Pin, 2.54mm)

	
	1*J_GPIO pin (optional)
	GPIO control pins                                (10Pin, 2*5Pin, 2. 0 mm)

	
	1*SYS_FAN pin
	System fan pin, full speed, does not support temperature control 
(3Pin, 1*3Pin, 2.54mm)

	
	1*CPU_FAN pin
	CPU fan pin, supports temperature control (3Pin, 1*3Pin, 2.54mm)

	Operating Environment
	Working temperature: -20℃~60℃; 
Working humidity: 5%~95% relative humidity, no condensation

	BIOS
	AMI BIOS, supports power-on, scheduled power-on, remote power on and off, and intelligent device identification

	Watch Dog
	Watchdog programming, support hardware reset function (256 levels, 0~255 seconds)

	Operating system
	Supports Windows 10, Windows 8, Windows 7, Linux, etc.
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[bookmark: _Toc11685][bookmark: _Toc25351][image: ]
Single mesh size↓
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Double mesh size↓
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