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ELSKY NUC12U Mini PC Specification
――――――――――――――――――――――――――――――――――――――――――――――――――――――

PC diagram
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Front interface diagram
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Rear interface diagram
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The above pictures are for reference only, please refer to the actual product!
※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

	HDMI
	Mini-DP
	Type-C
	LAN
	USB2.0
	USB3.2
	COM
	SSD
	Memory
	Power

	4K 60Hz
	4K 60Hz
	1. Display function 2.USB data
	1
	2
	3
	1
	1*M.2
	1*NB-DDR4

MAX 32G
	Wide voltage 12V~24V

	

	PC model
	 NUC12U

	PC size
	110mm(L)*107mm(W)*44 mm(H)(excluding foot pad height)

	Cooling system
	Equipped with heat dissipation holes, silent fan for heat dissipation

	Color
	Steel gray

	Adapt to motherboard
	NUC12U,NUC13U

	Motherboard
	CPU
	Supports Intel Alder Lake 12th generation U, P-series Core i3-1215U, i5-1235U, i7-1260P, etc

Supports Intel Raptor Lake 13th generation U, P-series Core i3-1305U, i5-1334U, i7-1340P, etc

(See next page for CPU list)

	
	Graphics card 
	Intel UHD Graphics / Intel Iris Xe Graphics graphics controller, support single display, dual display/triple display replication, dual display/triple display expansion

	
	Memory 
	1*NB-DDR4 , supports 2133/2400/2666/2933/320MHz memory, maximum support 32GB

	Front panel interface
	POWER
	1*switch button

	
	AUDIO
	1*AUDIO interface, support LINE_OUT output and MIC_IN input

	
	USB
	2*USB2.0 interface;
1*USB3.2 Gen1 interface;

	
	Type-C
	1*Type-C interface, support display function (4096/3840)*2160@60Hz ）and USB data transfer function

	Rear panel interface
	Power interface
	1*DC power supply interface (5.5*2.5mm), support DC 12V~24V wide voltage,recommended to 12V7A or above.

	
	Display 
	1*HDMI1.4 interface (4096/3840*2160@60Hz)
1*Mini_DP interface (4096/3840*2160@60Hz)

	
	LAN
	Single gigabit network card: Intel WG i219V Gigabit Network Card;

Support network wake-up function and network PXE function;

	
	USB
	2*USB3.2 Gen1 interface

	
	COM
	1*COM interface, default support for RS232;optional support RS232/RS422/RS485

	
	WiFi
	2*WiFi antenna interface

	Storage
	M.2 SSD
	1*M.2 Key-M slot, support M.2 2280 hard drives; Supports optional SATA and NVME (PCIE) protocols

	Expansion
	M.2_WiFi
	1*M.2 Key-E slot, support M.2 2230 WiFi Bluetooth module

	Operating environment
	Working temperature
	-10℃ ~ 60℃

	
	Storage temperature
	-20℃ ~ 70℃

	
	Relative humidity
	5%-95% relative humidity,no condensation

	
	Working vibration
	0.5g rms/5-500HZ/random/operating

	BIOS
	Support power on, timed power on, remote power on/off, etc

	Watch Dog
	Watchdog programming, supports hardware reset function (256 levels, 0-255 seconds)

	Operating system
	Windows 11, Windows 10, Linux, etc


※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※※

The following CPU information is for reference only,please consult sales for specific requirements!
	CPU
	CPU brand
	CPU model
	Kernel/thread
	Main frequency
	Turbo 
	CPU basic power consumption (W)
	Maximum turbo power consumption (W)

	12th gen I3
	Intel core
	1215U
	6 cores and 8 threads
	1.2G
	4.4G
	15
	55

	12th gen I5
	Intel core
	1235U
	10 cores and 12 threads
	1.3G
	4.4G
	15 
	55

	
	
	1245U
	10 cores and 12 threads
	1.6G
	4.4G
	15 
	55

	12th gen I7
	Intel core
	1265U
	10 cores and 12 threads
	1.8G
	4.8G
	15 
	55

	
	
	1255U
	10 cores and 12 threads
	1.7G
	4.7G
	15 
	55

	12th gen I3
	Intel core
	1220P
	10 cores and 12 threads
	1.5G
	4.4G
	28 
	64

	12th gen I5
	Intel core
	1240P
	12 cores and 16 threads
	1.7G
	4.4G
	28
	64

	
	
	1250P
	12 cores and 16 threads
	1.7G
	4.4G
	28
	64

	12th gen I7
	Intel core
	1280P
	14 cores and 20 threads
	1.8G
	4.8G
	28 
	64

	
	
	1260P
	12 cores and 16 threads
	2.1G
	4.7G
	28 
	64

	
	
	1270P
	12 cores and 16 threads
	2.2G
	4.8G
	28 
	64

	13th gen I3
	Intel core
	1305U
	5 cores and 6 threads
	1.6G
	4.5G
	15 
	55

	
	
	1315U
	6 cores and 8 threads
	1.2G
	4.5G
	15 
	55

	13th gen I5
	Intel core
	1334U
	10 cores and 12 threads
	1.3G
	4.6G
	15
	55

	
	
	1335U
	10 cores and 12 threads
	1.3G
	4.6G
	15
	55

	
	
	1345U
	10 cores and 12 threads
	1.6G
	4.7G
	15
	55

	13th gen I7
	Intel core
	1355U
	10 cores and 12 threads
	1.7G
	5.0G
	15 
	55 

	
	
	1365U
	10 cores and 12 threads
	1.8G
	5.2G
	15 
	55 

	13th gen I5
	Intel core
	1340P
	12 cores and 16 threads
	1.8G
	4.6G
	28
	64

	
	
	1350P
	12 cores and 16 threads
	1.9G
	4.7G
	28
	64

	13th gen I7
	Intel core
	1360P
	12 cores and 16 threads
	2.2G
	5.0G
	28
	64 

	
	
	1370P
	14 cores and 20 threads
	1.9G
	5.2G
	28
	64 


Explanation
Except for the accessories listed with the product configuration, the content contained in this manual does not represent our company's commitment. Our company reserves the right to make changes to this manual without further notice.

We are not responsible for any direct, indirect, intentional or unintentional damage or hidden dangers caused by improper installation or use.

Before ordering the product, please inquire with the distributor in detail about whether the product performance meets your needs.

The content of this manual is protected by copyright, and all rights reserved. Without permission, it may not be copied in any mechanical, electronic, or other way.

The final right of interpretation of this manual belongs to SHENZHEN ELSKY TECHNOLOGY CO.,LTD.

The above ordering information is for reference only. For details, please consult the sales department at 0755-82260150

Motherboard driver download https://pan.baidu.com/s/1ie7qi5NutS53ipPecRSYtw 
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